<?xml version="1.0" encoding="utf-8"?>
<!--This is FunctionCode Struct-->
<FuncGroup>
  <FunctionCode Name="F00.00" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028"	AbsoluteValue="0"			Chinese="控制模式选择" English="control mode" Show="1" />
  <FunctionCode Name="F00.01" Default="0:无PG的V/f控制" DeftEng="0: V/f control without PG"		Max="2" 			Min="0" 			Attribute="0x2088"	AbsoluteValue="0"			Chinese="电机控制方式选择" English="motor control type" Show="1" />
  <FunctionCode Name="F00.02" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028"	AbsoluteValue="0"			Chinese="变频器机型设定" English="inverter type" Show="1" />
  <FunctionCode Name="F00.03" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机选择" English="motor selection" Show="1" />
  <FunctionCode Name="F00.04" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="HD30通用扩展卡选择" English="HD30 general I/O card" Show="1" />
  <FunctionCode Name="F00.05" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="HD30扩展应用功能" English="HD30 extended functions" Show="1" />
  <FunctionCode Name="F00.06" Default="50.00" DeftEng="50.00"	Max="400.00" 	Min="50.00"		Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="最大输出频率" English="Max. frequency output" Show="1" />
  <FunctionCode Name="F00.07" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="上限运行频率设定通道" English="up-limit frequency set" Show="1" />
  <FunctionCode Name="F00.08" Default="50.00" DeftEng="50.00"   Max="400.00" 	Min="0.00" 		Attribute="0x61ac" 	AbsoluteValue="0"			Chinese="上限运行频率" English="up-limit frequency " Show="1" />
  <FunctionCode Name="F00.09" Default="0.00"  DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="下限运行频率" English="low-limit frequency" Show="1" />
  <FunctionCode Name="F00.10" Default="0:操作面板数字设定" DeftEng="0: Operator Panel Digital Settings"		Max="4" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="频率设定通道选择" English="frequency setting channel" Show="1" />
  <FunctionCode Name="F00.11" Default="0:操作面板运行命令通道" DeftEng="0: Operation panel operation command channel"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="运行命令通道选择" English="running command channel" Show="1" />
  <FunctionCode Name="F00.12" Default="2" DeftEng="2"		Max="2" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="多功能键功能选择" English="multi-function selection" Show="1" />
  <FunctionCode Name="F00.13" Default="50.00" DeftEng="50.00"   Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="初始运行频率数字设定" English="Digital set for initial frequency" Show="1" />
  <FunctionCode Name="F00.14" Default="0x1001" DeftEng="0x1001" Max="0x1111" 	Min="0x0000" 	Attribute="0x2061" 	AbsoluteValue="0"			Chinese="UP/DOWN数字设定控制" English="digital set for up and down" Show="1" />
  <FunctionCode Name="F00.15" Default="5.00" DeftEng="5.00"	Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定" English="digital set for dot frequency" Show="1" />
  <FunctionCode Name="F00.16" Default="0" DeftEng="0"	    Max="1000" 	    Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="点动运行间隔时间" English="interval period for dot operation" Show="1" />
  <FunctionCode Name="F00.17" Default="0:方向一致" 	DeftEng="0: Uniform Direction"	Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="运行方向选择" English="direction selection" Show="1" />
  <FunctionCode Name="F00.18" Default="0:允许反转" 	DeftEng="0: Allow Reverse"	Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="防反转选择" English="anti-negtive rotation selection" Show="1" />
  <FunctionCode Name="F00.19" Default="0.0" DeftEng="0.0"	Max="3600.0" 	Min="0.0" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="正反转死区时间" English="non-dead period of postive and negtive rotation" Show="1" />
  <FunctionCode Name="F00.20" Default="0" DeftEng="0"	Max="1" 	        Min="0" 		    Attribute="0x2048" 	AbsoluteValue="0"			Chinese="主键盘选择" English="main key selection" Show="1" />
  <FunctionCode Name="F00.21" Default="0" DeftEng="0"		Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="休眠功能使能" English="sleeping function selection" Show="1" />
  <FunctionCode Name="F00.22" Default="0.0" DeftEng="0.0"	Max="360.0" 	Min="0.0" 		Attribute="0x2622" 	AbsoluteValue="0"			Chinese="休眠唤醒时间" English="awaken time" Show="1" />
  <FunctionCode Name="F00.23" Default="0" 	DeftEng="0"    Max="0" 	    Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F00.24" Default="0.0" DeftEng="0.0"	Max="3600.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="休眠延迟时间" English="sleep delay time" Show="1" />
  <FunctionCode Name="F00.25" Default="0.0" DeftEng="0.0"	Max="400.00" 	Min="0.00" 		Attribute="0xe12a" 	AbsoluteValue="0"			Chinese="休眠频率" English="sleep frequency" Show="1" />
  <FunctionCode Name="F00.26" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="变频器零频运行动作选择" English="selection of Zero-frequency operation" Show="1" />
  <FunctionCode Name="F00.27" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F00.28" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F00.29" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F01.00" Default="0" DeftEng="0"		Max="65535" 	Min="0" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户密码" English="reserved" Show="1" />
  <FunctionCode Name="F01.01" Default="0" DeftEng="0"	    Max="2" 		  Min="0" 	    Attribute="0x2048" 	AbsoluteValue="0"			Chinese="菜单模式选择" English="reserved" Show="1" />
  <FunctionCode Name="F01.02" Default="0:无操作" DeftEng="0: No action"		Max="6" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="功能码参数初始化" English="parameter initialization" Show="1" />
  <FunctionCode Name="F01.03" Default="0:无操作" DeftEng="0: No action"		Max="2" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="参数上传至操作面板" English="update to keypad" Show="1" />
  <FunctionCode Name="F01.04" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F01.05" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F01.06" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F02.00" Default="0:从起动DWELL频率起动" DeftEng="0: Start from the start DWELL frequency"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="起动方式选择" English="start mode selection" Show="1" />
  <FunctionCode Name="F02.01" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动延迟时间" English="start delay time" Show="1" />
  <FunctionCode Name="F02.02" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="起动时DWELL频率设定" English="DWELL frequency set in start" Show="1" />
  <FunctionCode Name="F02.03" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动DWELL频率保持时间" English="DWELL frequency holding time in start" Show="1" />
  <FunctionCode Name="F02.04" Default="50" 	DeftEng="50"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="直流制动电流设定" English="DC brake current set" Show="1" />
  <FunctionCode Name="F02.05" Default="0.00" DeftEng="0.00"	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动时直流制动时间" English="DC brake time in start" Show="1" />
  <FunctionCode Name="F02.06" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F02.07" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F02.08" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F02.09" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F02.10" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F02.11" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F02.12" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F02.13" Default="2:减速停机+直流制动" DeftEng="2: Deceleration stop + DC brake"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="停机方式选择" English="stop mode selection" Show="1" />
  <FunctionCode Name="F02.14" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="停机DWELL频率设定" English="DWELL frequency set at stop" Show="1" />
  <FunctionCode Name="F02.15" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机DWELL频率保持时间" English="DWELL frequency holding time at stop" Show="1" />
  <FunctionCode Name="F02.16" Default="0.50" DeftEng="0.50"	Max="50.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="停机直流制动起始频率" English="beginning frequency of DC brake at stop " Show="1" />
  <FunctionCode Name="F02.17" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机直流制动等待时间" English="waiting time of DC brake at stop" Show="1" />
  <FunctionCode Name="F02.18" Default="0.00" DeftEng="0.00"	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机时直流制动时间" English="DC brake time at stop" Show="1" />
  <FunctionCode Name="F02.19" Default="0" 	 DeftEng="0"   Max="1" 	    Min="0" 		Attribute="0x2088" 	AbsoluteValue="0"			Chinese="点动控制方式" English="dot operation selection" Show="1" />
  <FunctionCode Name="F02.20" Default="0.50" DeftEng="0.50"	Max="0.50" 	    Min="0.00" 		Attribute="0x269c" 	AbsoluteValue="0"			Chinese="预励磁时间" English="Preexcitation time" Show="1" />
  <FunctionCode Name="F02.21" Default="0" DeftEng="0"	Max="0" 	    Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F02.22" Default="0" DeftEng="0"	Max="0" 	    Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F02.23" Default="0" DeftEng="0"	Max="0" 	    Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F03.00" Default="0:直线加减速" DeftEng="0: Linear Acceleration/Deceleration"		Max="1" 			Min="0" 	Attribute="0x2048" 	AbsoluteValue="0"			Chinese="加减速方式选择" English="Acc. and Dec. selection" Show="1" />
  <FunctionCode Name="F03.01" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间1" English="Acc. time1" Show="1" />
  <FunctionCode Name="F03.02" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间1" English="Dec. time1" Show="1" />
  <FunctionCode Name="F03.03" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间2" English="Acc. time2" Show="1" />
  <FunctionCode Name="F03.04" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间2" English="Dec. time2" Show="1" />
  <FunctionCode Name="F03.05" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间3" English="Acc. time3" Show="1" />
  <FunctionCode Name="F03.06" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间3" English="Dec. time3" Show="1" />
  <FunctionCode Name="F03.07" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间4" English="Acc. time4" Show="1" />
  <FunctionCode Name="F03.08" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间4" English="Dec. time4" Show="1" />
  <FunctionCode Name="F03.09" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="加速时间2和1切换频率" English="switch frequency of Acc. time2 and 1" Show="1" />
  <FunctionCode Name="F03.10" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="减速时间2和1切换频率" English="switch frequency of Dec. time2 and 1" Show="1" />
  <FunctionCode Name="F03.11" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="加速开始时S字特性时间" English="S time of Acc. start" Show="0" />
  <FunctionCode Name="F03.12" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="加速结束时S字特性时间" English="S time of Acc. end" Show="0" />
  <FunctionCode Name="F03.13" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="减速开始时S字特性时间" English="S time of Dec. start" Show="0" />
  <FunctionCode Name="F03.14" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="减速结束时S字特性时间" English="S time of Dec. end" Show="0" />
  <FunctionCode Name="F03.15" Default="6.0"  DeftEng="6.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="点动加速时间" English="spot Acc. time" Show="1" />
  <FunctionCode Name="F03.16" Default="6.0"  DeftEng="6.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="点动减速时间" English="spot Dec. time" Show="1" />
  <FunctionCode Name="F03.17" Default="10.0" DeftEng="10.0"		Max="6000.0" 			Min="0.1" 	Attribute="0x266a" 	AbsoluteValue="0"			Chinese="紧急停止减速时间" English="Dec. time of emergency stop" Show="0" />
  <FunctionCode Name="F03.18" Default="0"  DeftEng="0"		Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F03.19" Default="0"  DeftEng="0"		Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F03.20" Default="0"  DeftEng="0"		Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F04.00" Default="0:PID控制无效" DeftEng="0: invalid PID control"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="过程PID功能选择" English="process PID function selection" Show="1" />
  <FunctionCode Name="F04.01" Default="0"  DeftEng="0"		Max="2" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="给定通道选择" English="pro-given channel selection" Show="1" />
  <FunctionCode Name="F04.02" Default="0:模拟量反馈"  DeftEng="0: Analog Feedback"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="反馈通道选择" English="feedback channel selection" Show="1" />
  <FunctionCode Name="F04.03" Default="0.0"  DeftEng="0.0"		Max="200.0" 	Min="0.0"	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="给定量数字设定" English="pro-given digital setting" Show="1" />
  <FunctionCode Name="F04.04" Default="2.00" DeftEng="2.00"	Max="10.00" 	Min="0.00" 		Attribute="0x2064" 	AbsoluteValue="0"			Chinese="比例增益（P）" English="percentage gain" Show="1" />
  <FunctionCode Name="F04.05" Default="1.00" DeftEng="1.00"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="积分时间（I）" English="integral time" Show="1" />
  <FunctionCode Name="F04.06" Default="50.00" DeftEng="50.00" Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="积分项上限" English="integral up limit" Show="0" />
  <FunctionCode Name="F04.07" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="微分时间（D）" English="differential time" Show="1" />
  <FunctionCode Name="F04.08" Default="20.00" DeftEng="20.00" Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="微分限幅值" English="differential limit" Show="1" />
  <FunctionCode Name="F04.09" Default="0.10" DeftEng="0.10"	Max="50.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="采样周期（T）" English="sample period" Show="1" />
  <FunctionCode Name="F04.10" Default="0.0" DeftEng="0.0"	Max="20.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"			Chinese="偏差极限" English="deviation limit" Show="1" />
  <FunctionCode Name="F04.11" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID调节器上限通道" English="PID adjuster up limit channel" Show="1" />
  <FunctionCode Name="F04.12" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID调节器下限通道" English="PID adjuster down limit channel" Show="1" />
  <FunctionCode Name="F04.13" Default="50.00" DeftEng="50.00" Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID调节器上限值" English="PID adjuster up limit" Show="0" />
  <FunctionCode Name="F04.14" Default="0.00" DeftEng="0.00" 	Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID调节器下限值" English="PID adjuster down limit" Show="1" />
  <FunctionCode Name="F04.15" Default="0"   DeftEng="0"		Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID调节器调节特性" English="PID adjuster characteristic" Show="1" />
  <FunctionCode Name="F04.16" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F04.17" Default="0.05" DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="PID输出滤波时间" English="PID output filter time" Show="1" />
  <FunctionCode Name="F04.18" Default="0:PID调节禁止反转" DeftEng="0: PID adjustment prohibited to reverse"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID输出反转选择" English="PID output reversion selection" Show="1" />
  <FunctionCode Name="F04.19" Default="50.00" DeftEng="50.00" Max="400.00" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID输出反转频率上限" English="PID output reversion frequency up limit" Show="1" />
  <FunctionCode Name="F04.20" Default="0" DeftEng="0"		Max="1" 			Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID运算模式" English="PID operation mode" Show="1" />
  <FunctionCode Name="F04.21" Default="0" DeftEng="0"		Max="1" 			Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID休眠使能" English="PID sleep mode" Show="1" />
  <FunctionCode Name="F04.22" Default="10.0" DeftEng="10.0"		Max="100.0" 			Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="唤醒容差" English="awake deviation" Show="1" />
  <FunctionCode Name="F04.23" Default="0.1"  DeftEng="0.1"		Max="6000.0" 			Min="0.1" 	Attribute="0x266a" 	AbsoluteValue="0"			Chinese="唤醒延时" English="awake delay" Show="1" />
  <FunctionCode Name="F04.24" Default="10.0" DeftEng="10.0"		Max="100.0" 			Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="休眠容差" English="sleep deviation" Show="1" />
  <FunctionCode Name="F04.25" Default="20.00" DeftEng="20.00"		Max="400.00" 			Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="休眠频率" English="sleep frequency" Show="1" />
  <FunctionCode Name="F04.26" Default="0.1"  DeftEng="0.1"		Max="6000.0" 			Min="0.1" 	Attribute="0x266a" 	AbsoluteValue="0"			Chinese="休眠延时" English="sleep delay" Show="1" />
  <FunctionCode Name="F04.27" Default="0" DeftEng="0"		Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F04.28" Default="0" DeftEng="0"		Max="0" 			Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F04.29" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F05.00" Default="3:不处理" DeftEng="3: Do not process" Max="3" 	Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="外部给定量曲线选择" English="external pro-given curve selection" Show="1" />
  <FunctionCode Name="F05.01" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线最小给定" English="straight line Min pro-given" Show="1" />
  <FunctionCode Name="F05.02" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线最小给定对应值" English="conresponding value of straight line Min pro-given" Show="1" />
  <FunctionCode Name="F05.03" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线最大给定" English="straight line Max pro-given" Show="1" />
  <FunctionCode Name="F05.04" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线最大给定对应值" English="conresponding value of straight line Max pro-given" Show="1" />
  <FunctionCode Name="F05.05" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="直线2最小给定" English="straight line2 Min pro-given" Show="1" />
  <FunctionCode Name="F05.06" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="直线2最小给定对应值" English="conresponding value of straight line2 Min pro-given" Show="1" />
  <FunctionCode Name="F05.07" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="直线2最大给定" English="straight line2 Max pro-given" Show="0" />
  <FunctionCode Name="F05.08" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="直线2最大给定对应值" English="conresponding value of straight line2 Max pro-given" Show="0" />
  <FunctionCode Name="F05.09" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定" English="broken line Max pro-given" Show="0" />
  <FunctionCode Name="F05.10" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定对应值" English="conresponding value of broken line Max pro-given" Show="0" />
  <FunctionCode Name="F05.11" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点2给定" English="inflection point2 pro-given" Show="0" />
  <FunctionCode Name="F05.12" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点2对应值" English="conresponding value of inflection point2" Show="0" />
  <FunctionCode Name="F05.13" Default="0.0"  DeftEng="0.0"	Max="100.0" 	Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点1给定" English="inflection point1 pro-given" Show="1" />
  <FunctionCode Name="F05.14" Default="0.0"  DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点1对应值" English="conresponding value of inflection point1" Show="1" />
  <FunctionCode Name="F05.15" Default="0.0"  DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定" English="broken line min pro-given" Show="1" />
  <FunctionCode Name="F05.16" Default="0.0"  DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定对应值" English="conresponding value of broken line min pro-given" Show="1" />
  <FunctionCode Name="F05.17" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="跳跃频率1" English="jumping frequency1" Show="1" />
  <FunctionCode Name="F05.18" Default="0" DeftEng="0"	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="跳跃频率2" English="jumping frequency2" Show="1" />
  <FunctionCode Name="F05.19" Default="0" DeftEng="0"	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="跳跃频率3" English="jumping frequency3" Show="1" />
  <FunctionCode Name="F05.20" Default="0.00" DeftEng="0.00"	Max="30.00" 	Min="0.00" 		Attribute="0x2164" 	AbsoluteValue="0"			Chinese="跳跃频率范围"  English="range of jumping frequency" Show="1" />
  <FunctionCode Name="F05.21" Default="5.00" DeftEng="5.00"	    Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定2" English="spot operation frequency digital setting2" Show="0" />
  <FunctionCode Name="F05.22" Default="3" DeftEng="3"	    Max="3" 	Min="0" 		Attribute="0x2088" 	AbsoluteValue="0"			Chinese="键盘电位计曲线选择" English="keypad electric level curve selection" Show="1" />
  <FunctionCode Name="F05.23" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F05.24" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F05.25" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F06.00" Default="5.00" DeftEng="5.00"	Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令1" English="multi-frequency1" Show="1" />
  <FunctionCode Name="F06.01" Default="5.00" DeftEng="5.00"	Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令2" English="multi-frequency2" Show="1" />
  <FunctionCode Name="F06.02" Default="5.00" DeftEng="5.00"	Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令3" English="multi-frequency3" Show="1" />
  <FunctionCode Name="F06.03" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令4" English="multi-frequency4" Show="1" />
  <FunctionCode Name="F06.04" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令5" English="multi-frequency5" Show="1" />
  <FunctionCode Name="F06.05" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令6" English="multi-frequency6" Show="1" />
  <FunctionCode Name="F06.06" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令7" English="multi-frequency7" Show="1" />
  <FunctionCode Name="F06.07" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令8" English="multi-frequency8" Show="0" />
  <FunctionCode Name="F06.08" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令9" English="multi-frequency9" Show="0" />
  <FunctionCode Name="F06.09" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令10" English="multi-frequency10" Show="0" />
  <FunctionCode Name="F06.10" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令11" English="multi-frequency11" Show="0" />
  <FunctionCode Name="F06.11" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令12" English="multi-frequency12" Show="0" />
  <FunctionCode Name="F06.12" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令13" English="multi-frequency13" Show="0" />
  <FunctionCode Name="F06.13" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令14" English="multi-frequency14" Show="0" />
  <FunctionCode Name="F06.14" Default="5.00" DeftEng="5.00"    Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="多段频率指令15" English="multi-frequency15" Show="0" />
  <FunctionCode Name="F06.15" Default="0"    DeftEng="0"    Max="1" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PLC运行方式选择" English="PLC operation mode selection" Show="1" />
  <FunctionCode Name="F06.16" Default="0000" DeftEng="0000"	Max="0x1122" 	Min="0x0000" 	Attribute="0x20a1" 	AbsoluteValue="0"			Chinese="简易PLC运行方式选择" English="simplied PLC operation mode selection" Show="1" />
  <FunctionCode Name="F06.17" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段1设置" English="PLC stage1 setting" Show="1" />
  <FunctionCode Name="F06.18" Default="5.0"  DeftEng="5.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段1运行时间" English="stage1 operation time" Show="1" />
  <FunctionCode Name="F06.19" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段2设置" English="PLC stage2 set" Show="1" />
  <FunctionCode Name="F06.20" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段2运行时间" English="stage2 operation time" Show="1" />
  <FunctionCode Name="F06.21" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="阶段3设置" English="stage3 setting" Show="1" />
  <FunctionCode Name="F06.22" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段3运行时间" English="stage3 operation time" Show="1" />
  <FunctionCode Name="F06.23" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="阶段4设置" English="stage4 set" Show="1" />
  <FunctionCode Name="F06.24" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段4运行时间" English="stage4 operation time" Show="1" />
  <FunctionCode Name="F06.25" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段5设置" English="PLC stage5 set" Show="1" />
  <FunctionCode Name="F06.26" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段5运行时间" English="stage5 operation time" Show="1" />
  <FunctionCode Name="F06.27" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段6设置" English="PLC stage6 set" Show="1" />
  <FunctionCode Name="F06.28" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段6运行时间" English="stage6 operation time" Show="1" />
  <FunctionCode Name="F06.29" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段7设置" English="PLC stage7 set" Show="1" />
  <FunctionCode Name="F06.30" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段7运行时间" English="stage7 operation time" Show="1" />
  <FunctionCode Name="F06.31" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段8设置" English="PLC stage8 set" Show="1" />
  <FunctionCode Name="F06.32" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段8运行时间" English="stage8 operation time" Show="1" />
  <FunctionCode Name="F06.33" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段9设置" English="PLC stage9 set" Show="1" />
  <FunctionCode Name="F06.34" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段9运行时间" English="stage9 operation time" Show="1" />
  <FunctionCode Name="F06.35" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段10设置" English="PLC stage10 set" Show="1" />
  <FunctionCode Name="F06.36" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段10运行时间" English="stage 10 operation time" Show="1" />
  <FunctionCode Name="F06.37" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段11设置" English="PLC stage11 set" Show="1" />
  <FunctionCode Name="F06.38" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段11运行时间" English="stage11 operation time" Show="1" />
  <FunctionCode Name="F06.39" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段12设置" English="PLC stage12 set" Show="1" />
  <FunctionCode Name="F06.40" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段12运行时间" English="stage12 operation time" Show="1" />
  <FunctionCode Name="F06.41" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段13设置" English="PLC stage13 set" Show="1" />
  <FunctionCode Name="F06.42" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段13运行时间" English="stage13 operation time" Show="1" />
  <FunctionCode Name="F06.43" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段14设置" English="PLC stage14 set" Show="1" />
  <FunctionCode Name="F06.44" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段14运行时间" English="stage14 operation time" Show="1" />
  <FunctionCode Name="F06.45" Default="000"  DeftEng="000"	Max="0x321" 	Min="0x000" 	Attribute="0x2059" 	AbsoluteValue="0"			Chinese="PLC阶段15设置" English="PLC stage15 set" Show="1" />
  <FunctionCode Name="F06.46" Default="0.0"  DeftEng="0.0"	Max="3276.7" 	Min="0.0" 		Attribute="0x206a" 	AbsoluteValue="0"			Chinese="阶段15运行时间" English="stage15 operation time" Show="1" />
  <FunctionCode Name="F06.47" Default="0"  DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F06.48" Default="0"  DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F06.49" Default="0"  DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.00" Default="2.2" DeftEng="2.2"	Max="5.5" 	Min="0.2" 		Attribute="0x1222" 	AbsoluteValue="0"			Chinese="电机额定功率" English="motor rate power" Show="1" />
  <FunctionCode Name="F08.01" Default="380" DeftEng="380"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="电机额定电压" English="motor rated voltage" Show="1" />
  <FunctionCode Name="F08.02" Default="13.00" DeftEng="13.00" Max="99.99" 	Min="0.01" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="电机额定电流" English="motor rated current" Show="1" />
  <FunctionCode Name="F08.03" Default="50.0"  DeftEng="50.0"	Max="150.0" 	Min="1.0" 		Attribute="0x010a" 	AbsoluteValue="0"			Chinese="电机额定频率" English="motor rated frequency" Show="1" />
  <FunctionCode Name="F08.04" Default="1500"  DeftEng="1500"	Max="24000" 	Min="1" 			Attribute="0x0408" 	AbsoluteValue="0"			Chinese="电机额定转速" English="motor rated Rpm" Show="1" />
  <FunctionCode Name="F08.05" Default="0.850" DeftEng="0.850"		Max="1.000" 			Min="0.000" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F08.06" Default="0:不动作"  DeftEng="0: No action"		Max="3" 			Min="0" 			Attribute="0x0008" 	AbsoluteValue="0"			Chinese="电机参数自整定" English="motor parameter auto-tuning" Show="1" />
  <FunctionCode Name="F08.07" Default="0.70"  DeftEng="0.70"	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="电机定子电阻" English="motor stator resistor" Show="1" />
  <FunctionCode Name="F08.08" Default="0.67"  DeftEng="0.67"	Max="99.99" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机转子电阻" English="motor rotor resistor" Show="1" />
  <FunctionCode Name="F08.09" Default="0.50"  DeftEng="0.50"		Max="500.00" 		Min="0.00" 			Attribute="0x0c2c" 	AbsoluteValue="0"			Chinese="电机漏电感" English="motor leakage inductance" Show="1" />
  <FunctionCode Name="F08.10" Default="12.40" DeftEng="12.40"	Max="500.00" 		Min="0.00" 			Attribute="0x0c2c" 	AbsoluteValue="0"			Chinese="电机互感抗" English="motor mutual inductance" Show="1" />
  <FunctionCode Name="F08.11" Default="5.30"  DeftEng="5.30"	Max="999.9" 	Min="0.0" 		Attribute="0x0222" 	AbsoluteValue="0"			Chinese="电机空载励磁电流" English="motor empty load excitation current" Show="1" />
  <FunctionCode Name="F08.12" Default="1.00"  DeftEng="1.00"	Max="1.00" 		Min="0.00" 		Attribute="0x001c" 	AbsoluteValue="0"			Chinese="电机铁芯饱和系数1" English="motor Core saturation coefficient1 " Show="1" />
  <FunctionCode Name="F08.13" Default="1.00"  DeftEng="1.00"	Max="1.00" 		Min="0.00" 		Attribute="0x001c" 	AbsoluteValue="0"			Chinese="电机铁芯饱和系数2" English="motor Core saturation coefficient2" Show="1" />
  <FunctionCode Name="F08.14" Default="1.00"  DeftEng="1.00"	Max="1.00" 		Min="0.00" 		Attribute="0x001c" 	AbsoluteValue="0"			Chinese="电机铁芯饱和系数3" English="motor Core saturation coefficient3" Show="1" />
  <FunctionCode Name="F08.15" Default="1.00"  DeftEng="1.00"	Max="1.00" 		Min="0.00" 		Attribute="0x001c" 	AbsoluteValue="0"			Chinese="电机铁芯饱和系数4" English="motor Core saturation coefficient4" Show="1" />
  <FunctionCode Name="F08.16" Default="1.00"  DeftEng="1.00"	Max="1.00" 		Min="0.00" 		Attribute="0x001c" 	AbsoluteValue="0"			Chinese="电机铁芯饱和系数5" English="motor Core saturation coefficient5" Show="1" />
  <FunctionCode Name="F08.17" Default="0" DeftEng="0"	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.18" Default="0" DeftEng="0"	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.19" Default="0" DeftEng="0"	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F09.00" Default="0:直线" 	DeftEng="0: Straight" 	Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机V/F曲线设定" English="motor V/F curve set" Show="1" />
  <FunctionCode Name="F09.01" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 	Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F频率值F3" English="motor V/F frequency F3" Show="1" />
  <FunctionCode Name="F09.02" Default="0.0" DeftEng="0.0"	    Max="100.0" 	Min="0.0" 	Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F电压值V3" English="motor V/F voltage V3" Show="1" />
  <FunctionCode Name="F09.03" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 	Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F频率值F2" English="motor V/F frequency F2" Show="1" />
  <FunctionCode Name="F09.04" Default="0.0" DeftEng="0.0"		Max="100.0" 	Min="0.0" 	Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F电压值V2" English="motor V/F voltage V2" Show="1" />
  <FunctionCode Name="F09.05" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F频率值F1" English="motor V/F frequency F1" Show="1" />
  <FunctionCode Name="F09.06" Default="0.0" DeftEng="0.0"		Max="100.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机V/F电压值V1" English="motor V/F voltage V1" Show="1" />
  <FunctionCode Name="F09.07" Default="2.0" DeftEng="2.0"	Max="30.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"			Chinese="电机转矩提升" English="motor torque boost" Show="1" />
  <FunctionCode Name="F09.08" Default="25.0" DeftEng="25.0"	Max="50.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"			Chinese="电机手动转矩提升截止点" English="motor manual torque boost ending point" Show="1" />
  <FunctionCode Name="F09.09" Default="0.0" DeftEng="0.0" Max="300.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机转差补偿增益" English="Motor slip compensation gain" Show="1" />
  <FunctionCode Name="F09.10" Default="0.10" DeftEng="0.10"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机转差补偿滤波时间" English="Motor slip compensation filter time" Show="1" />
  <FunctionCode Name="F09.11" Default="200.0" DeftEng="200.0" Max="250.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机转差补偿限定" English="Motor slip compensation limit" Show="1" />
  <FunctionCode Name="F09.12" Default="0.193" DeftEng="0.193"	Max="9.999" 		Min="0.000" 		Attribute="0x12a6" 	AbsoluteValue="0"			Chinese="电机铁损" English="Motor iron loss" Show="1" />
  <FunctionCode Name="F09.13" Default="0"   DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="IM1 V/F速度环输出限定" English="IM1 V/F speed loop output limit" Show="1" />
  <FunctionCode Name="F09.14" Default="1:一直动作" 	DeftEng="1: Always Action"	Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机AVR（自动电压调节）功能" English="Motor AVR (automatic voltage regulation) function" Show="1" />
  <FunctionCode Name="F09.15" Default="50" 	DeftEng="50"	Max="200" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机低频抑制震荡系数" English="Motor Low Frequency Suppression Oscillation Coefficient" Show="1" />
  <FunctionCode Name="F09.16" Default="20" 	DeftEng="20"	Max="200" 		    Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机高频抑制震荡系数" English="Motor high Frequency Suppression Oscillation Coefficient" Show="1" />
  <FunctionCode Name="F09.17" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机1节能控制选择" English="Motor 1 Energy Saving Control Options" Show="1" />
  <FunctionCode Name="F09.18" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机1节能系数" English="Motor 1 energy efficiency" Show="1" />
  <FunctionCode Name="F09.19" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F09.20" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F09.21" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F10.00" Default="10.0" DeftEng="10.0"	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1速度控制比例增益1" English="Motor 1 Speed Control Proportional Gain1" Show="1" />
  <FunctionCode Name="F10.01" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机1速度控制积分时间1" English="Motor 1 speed control integration time 1" Show="1" />
  <FunctionCode Name="F10.02" Default="10.0" DeftEng="10.0"	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1速度控制比例增益2" English="Motor 1 Speed Control Proportional Gain1" Show="1" />
  <FunctionCode Name="F10.03" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机1速度控制积分时间2" English="Motor 1 speed control integration time 2" Show="1" />
  <FunctionCode Name="F10.04" Default="10.00" DeftEng="10.00" Max="F10.05" 	Min="0.00" 		Attribute="0x2164" 	AbsoluteValue="0"			Chinese="电机1速度环PI切换频率1" English="Motor 1 speed loop PI switching frequency 1" Show="1" />
  <FunctionCode Name="F10.05" Default="15.00" DeftEng="15.00" Max="50.00" 	Min="F10.04" 		Attribute="0x2164" 	AbsoluteValue="0"			Chinese="电机1速度环PI切换频率2" English="Motor 1 speed loop PI switching frequency 2" Show="1" />
  <FunctionCode Name="F10.06" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1速度环积分项限定" English="Motor 1 speed loop integral term limit" Show="1" />
  <FunctionCode Name="F10.07" Default="0.00"  DeftEng="0.00"	Max="1.00" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="电机1速度环微分时间" English="Motor 1 speed loop differential time" Show="1" />
  <FunctionCode Name="F10.08" Default="0.010" DeftEng="0.010" Max="1.000" 	Min="0.000" 	Attribute="0x2666" 	AbsoluteValue="0"			Chinese="电机1速度环输出滤波时间" English="Motor 1 speed loop output filter time" Show="1" />
  <FunctionCode Name="F10.09" Default="0:不锁定"  DeftEng="0: No lock"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机1转矩限定锁定选择" English="Motor 1 torque limit lock selection" Show="1" />
  <FunctionCode Name="F10.10" Default="0" DeftEng="0"		Max="0x2222" 			Min="0" 			Attribute="0x2061" 	AbsoluteValue="0"			Chinese="电机1转矩限定通道" English="Motor 1 torque limit channel" Show="1" />
  <FunctionCode Name="F10.11" Default="180.0" DeftEng="180.0" Max="250.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1正转时电动转矩限定" English="Electric torque limit when motor 1 rotates forward" Show="1" />
  <FunctionCode Name="F10.12" Default="180.0" DeftEng="180.0" Max="250.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1反转时电动转矩限定" English="Electric torque limit when motor 1 reverses" Show="1" />
  <FunctionCode Name="F10.13" Default="180.0" DeftEng="180.0" Max="250.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1正转时再生转矩限定" English="Regenerative torque limit when motor 1 rotates forward" Show="1" />
  <FunctionCode Name="F10.14" Default="180.0" DeftEng="180.0" Max="250.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1反转时再生转矩限定" English="Revolving torque limit when motor 1 reverses" Show="1" />
  <FunctionCode Name="F10.15" Default="0"     DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F10.16" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F10.17" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F11.00" Default="800"   DeftEng="800"		Max="2000" 			Min="1" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1电流环KP" English="motor1 current loop KP" Show="1" />
  <FunctionCode Name="F11.01" Default="200"   DeftEng="200"		Max="1000" 			Min="1" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1电流环KI" English="Motor1 current loop KI" Show="1" />
  <FunctionCode Name="F11.02" Default="3" 	  DeftEng="3"	Max="31" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1电流环输出滤波次数" English="Motor 1 Current Loop Output Filter Times" Show="1" />
  <FunctionCode Name="F11.03" Default="0:禁止前馈" 	DeftEng="0: Prohibit feedforward"	Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机1电流环前馈使能" English="motor1 current feedback enable" Show="1" />
  <FunctionCode Name="F11.04" Default="0.0" DeftEng="0.0"		Max="30.0" 			Min="0.0" 			Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1励磁增强设定" English="Motor 1 Excitation Enhancement Settings" Show="1" />
  <FunctionCode Name="F11.05" Default="0:禁止磁场定向角度矫正" DeftEng="0: Prohibit field orientation angle correction"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机1磁场定向优化设定" English="Motor 1 field orientation optimization setting" Show="1" />
  <FunctionCode Name="F11.06" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F11.07" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F11.08" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F15.00" Default="2:正转功能" 	DeftEng="2: Forward Function"	Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI1端子功能选择" English="DI1 terminal fucntion selection" Show="1" />
  <FunctionCode Name="F15.01" Default="3:反转功能" 	DeftEng="3: Reverse Function"	Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI2端子功能选择" English="DI2 terminal fucntion selection" Show="1" />
  <FunctionCode Name="F15.02" Default="0:保留" 	DeftEng="0: Reserved"	Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI3端子功能选择" English="DI3 terminal function selection" Show="1" />
  <FunctionCode Name="F15.03" Default="0:保留" 	DeftEng="0: Reserved"	Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI4端子功能选择" English="DI4 terminal function selection" Show="1" />
  <FunctionCode Name="F15.04" Default="0" DeftEng="0"		Max="86" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI5端子功能" English="DI5 terminal function" Show="1" />
  <FunctionCode Name="F15.05" Default="0" DeftEng="0"		Max="86" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI6端子功能" English="DI6 terminal function" Show="1" />
  <FunctionCode Name="F15.06" Default="0" DeftEng="0"		Max="87" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI7端子(扩展卡端子)功能" English="DI7 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.07" Default="0" DeftEng="0"		Max="87" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI8端子(扩展卡端子)功能" English="DI8 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.08" Default="0" DeftEng="0"		Max="87" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI9端子(扩展卡端子)功能" English="DI9 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.09" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI10端子(扩展卡端子)功能" English="DI10 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.10" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI11端子(扩展卡端子)功能" English="DI11 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.11" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI12端子(扩展卡端子)功能" English="DI2 terminal(extended card terminal) function" Show="1" />
  <FunctionCode Name="F15.12" Default="1.00" DeftEng="1.00"	Max="99.99" 	Min="0.00" 		Attribute="0x30a4" 	AbsoluteValue="0"			Chinese="端子UP/DN加减速速率" English="terminal UP/DN Acc. and Dec. rate" Show="1" />
  <FunctionCode Name="F15.13" Default="0:2ms" DeftEng="0:2ms"		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="端子检测间隔时间" English="terminal detection interval time" Show="1" />
  <FunctionCode Name="F15.14" Default="4" 	DeftEng="4" 	Max="10000" 		Min="0" 			Attribute="0x3748" 	AbsoluteValue="0"			Chinese="端子检测滤波次数" English="terminal detection filter times" Show="1" />
  <FunctionCode Name="F15.15" Default="0" 	DeftEng="0" 	Max="0x100f" 	Min="0" 			Attribute="0x2061" 	AbsoluteValue="0"			Chinese="输入端子正反逻辑设定" English="input terminals postive and negtive logic set" Show="1" />
  <FunctionCode Name="F15.16" Default="0:两线式运转模式1" 	DeftEng="0: Two-line operation mode 1"	Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="FWD/REV运转模式设定" English="FWD/REV operation  mode set" Show="1" />
  <FunctionCode Name="F15.17" Default="0"  DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="端子外部设备故障动作选择" English="terminal external fault action selection" Show="1" />
  <FunctionCode Name="F15.18" Default="0"  DeftEng="0"	    Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DO1端子功能" English="DO1 terminal function" Show="1" />
  <FunctionCode Name="F15.19" Default="2:变频器运行中" DeftEng="2: Drive Running"		Max="38" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="DO2端子功能选择" English="DO2 terminal function selection" Show="1" />
  <FunctionCode Name="F15.20" Default="31:变频器故障"  DeftEng="31: Drive Fault"	Max="33" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="继电器1输出功能选择" English="relay1 output function selection" Show="1" />
  <FunctionCode Name="F15.21" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="继电器2(扩展继电器)输出功能" English="relay2(extended relay) output function" Show="1" />
  <FunctionCode Name="F15.22" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="继电器3(扩展继电器)输出功能" English="relay3(extended relay) output function" Show="1" />
  <FunctionCode Name="F15.23" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="继电器4(扩展继电器)输出功能" English="relay4(extended relay) output function" Show="1" />
  <FunctionCode Name="F15.24" Default="0"   DeftEng="0"	Max="0xf" 		Min="0" 			Attribute="0x2049" 	AbsoluteValue="0"			Chinese="输出端子正反逻辑设定" English="output terminal FWD/REV logic set" Show="1" />
  <FunctionCode Name="F15.25" Default="0"   DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="定时功能ON侧延迟时间" English="Timing function ON side delay time" Show="1" />
  <FunctionCode Name="F15.26" Default="0"   DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="定时功能OFF侧延迟时间" English="Timing function OFF side delay time" Show="1" />
  <FunctionCode Name="F15.27" Default="2.50" DeftEng="2.50"	Max="100.00" 	Min="0.00" 		Attribute="0x216c" 	AbsoluteValue="0"			Chinese="频率到达(FAR)检出宽度" English="Frequency arrival (FAR) detection width" Show="1" />
  <FunctionCode Name="F15.28" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xe16c" 	AbsoluteValue="0"			Chinese="零频信号检出值" English="zero-frequency signal detection value" Show="1" />
  <FunctionCode Name="F15.29" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xe16c" 	AbsoluteValue="0"			Chinese="零频回差" English="Zero frequency difference" Show="1" />
  <FunctionCode Name="F15.30" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="FDT1检出方式" English="FDT1 detection method" Show="1" />
  <FunctionCode Name="F15.31" Default="50.00" DeftEng="50.00" Max="400.00" 	Min="0.00" 		Attribute="0xe16c" 	AbsoluteValue="0"			Chinese="FDT1电平" English="FDT1 electric level" Show="1" />
  <FunctionCode Name="F15.32" Default="0.00"  DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0xe16c" 	AbsoluteValue="0.00"			Chinese="FDT1滞后" English="FDT1 delay" Show="1" />
  <FunctionCode Name="F15.33" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="FDT2检出方式" English="FDT2 detection mode" Show="1" />
  <FunctionCode Name="F15.34" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="FDT2电平" English="FDT2 electric level" Show="1" />
  <FunctionCode Name="F15.35" Default="1.00" DeftEng="1.00"	Max="400.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="FDT2滞后" English="FDT2 delay" Show="0" />
  <FunctionCode Name="F15.36" Default="0" 	DeftEng="0"	Max="65535" 	Min="0" 			Attribute="0x3168" 	AbsoluteValue="0"			Chinese="设定运行时间" English="set operation time" Show="1" />
  <FunctionCode Name="F15.37" Default="0" 	DeftEng="0"	Max="9999" 		Min="F15.38" 	Attribute="0x2060" 	AbsoluteValue="0"			Chinese="设定计数值到达给定" English="Set the count value to reach the given" Show="1" />
  <FunctionCode Name="F15.38" Default="0" 	DeftEng="0"	Max="F15.37" 	Min="0" 			Attribute="0x2060" 	AbsoluteValue="0"			Chinese="指令计数值到达给定" English="The instruction count reaches the given value" Show="1" />
  <FunctionCode Name="F15.39" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="欠转矩检出值" English="Under-torque detection value" Show="1" />
  <FunctionCode Name="F15.40" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="欠转矩检出时间" English="Under-torque detection time" Show="1" />
  <FunctionCode Name="F15.41" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="过转矩检出值" English="Over torque detection value" Show="1" />
  <FunctionCode Name="F15.42" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="过转矩检出时间" English="Over torque detection time" Show="1" />
  <FunctionCode Name="F15.43" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="输出端子延时" English="Output terminal delay" Show="1" />
  <FunctionCode Name="F15.44" Default="0:保留" 	DeftEng="0: Reserved"	Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="AI端子（ADI）功能" English="AI terminal (ADI) function" Show="1" />
  <FunctionCode Name="F15.45" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F15.46" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F16.00" Default="0:保留" 	DeftEng="0: Reserved"	Max="12" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="操作面板电位计功能选择" English="Operation panel potentiometer function selection" Show="1" />
  <FunctionCode Name="F16.01" Default="2:频率设定通道" DeftEng="2: Frequency Setting Channel"		Max="12" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="模拟输入AI端子功能选择" English="Analog input AI terminal function selection" Show="1" />
  <FunctionCode Name="F16.02" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI2端子功能" English="AI2 terminal function" Show="1" />
  <FunctionCode Name="F16.03" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI3端子功能" English="AI3 terminal function" Show="1" />
  <FunctionCode Name="F16.04" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI4端子功能" English="AI4 terminal function" Show="1" />
  <FunctionCode Name="F16.05" Default="0.0" DeftEng="0.0"	Max="200.0" 	Min="0.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输入AI偏置" English="Analog input AI offset" Show="1" />
  <FunctionCode Name="F16.06" Default="1.00" DeftEng="1.00"	Max="20.00" 	Min="0.00" 	Attribute="0x2064" 	AbsoluteValue="10.0"	Chinese="模拟输入AI增益" English="Analog input AI gain" Show="1" />
  <FunctionCode Name="F16.07" Default="0.05" DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="模拟输入AI滤波时间" English="Analog input AI filter time" Show="1" />
  <FunctionCode Name="F16.08" Default="0.0"  DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x0028" 	AbsoluteValue="100.0"	Chinese="AI2偏置" English="AI2 offset" Show="0" />
  <FunctionCode Name="F16.09" Default="1.00" DeftEng="1.00"	Max="+10.00" 	Min="-10.00" 	Attribute="0x0028" 	AbsoluteValue="10.00"		Chinese="AI2增益" English="AI2gain" Show="0" />
  <FunctionCode Name="F16.10" Default="0.05" DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI2滤波时间" English="AI2 filter time" Show="0" />
  <FunctionCode Name="F16.11" Default="0.0"  DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x0028" 	AbsoluteValue="100.0"	Chinese="AI3偏置" English="AI3 offset" Show="0" />
  <FunctionCode Name="F16.12" Default="1.00" DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x0028" 	AbsoluteValue="0"		Chinese="AI3增益" English="AI3 gain" Show="0" />
  <FunctionCode Name="F16.13" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI3滤波时间" English="AI3 filter time" Show="1" />
  <FunctionCode Name="F16.14" Default="0.0" DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x0028" 	AbsoluteValue="100.0"	Chinese="AI4偏置" English="AI4 offset" Show="0" />
  <FunctionCode Name="F16.15" Default="1.00" DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x0028" 	AbsoluteValue="0"		Chinese="AI4增益" English="AI4 gain" Show="0" />
  <FunctionCode Name="F16.16" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AI4滤波时间" English="AI4 filter time" Show="1" />
  <FunctionCode Name="F16.17" Default="10000" DeftEng="10000"	Max="50000" 		Min="0" 		Attribute="0x2168" 	AbsoluteValue="0"			Chinese="最大脉冲输入频率" English="Max pulse input frequency" Show="1" />
  <FunctionCode Name="F16.18" Default="0.05"  DeftEng="0.05"		Max="10.00" 		Min="0.01" 			Attribute="0x2664" 	AbsoluteValue="0"			Chinese="输入脉冲滤波时间" English="input pulse filter time" Show="1" />
  <FunctionCode Name="F16.19" Default="2:给定频率(0-最大输出频率)" DeftEng="2: Given frequency (0-max output frequency)"		Max="14" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="AO端子输出功能选择" English="AO terminal output function selection" Show="1" />
  <FunctionCode Name="F16.20" Default="0"  DeftEng="0"		Max="20" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AO2端子功能" English="AO2 terminal function" Show="1" />
  <FunctionCode Name="F16.21" Default="0:保留" 	DeftEng="0: Reserved"	Max="14" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="DO端子输出功能选择" English="DO terminal output function selection" Show="1" />
  <FunctionCode Name="F16.22" Default="0.0" DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输出AO偏置" English="analogue output AO offset" Show="1" />
  <FunctionCode Name="F16.23" Default="100.0"  DeftEng="100.0"   Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="模拟输出AO增益" English="analogue output AO gain" Show="1" />
  <FunctionCode Name="F16.24" Default="0.0" DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x0028" 	AbsoluteValue="100.0"	Chinese="AO2偏置" English="AO2 offset" Show="0" />
  <FunctionCode Name="F16.25" Default="100.0" DeftEng="100.0" Max="200.0" 	Min="0.0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="AO2增益" English="AO2 gain" Show="0" />
  <FunctionCode Name="F16.26" Default="10.00" DeftEng="10.00"	Max="50.00" 		Min="0.01" 		Attribute="0x2964" 	AbsoluteValue="0"			Chinese="DO端子最大输出脉冲频率" English="DO terminal Max output pulse frequency" Show="1" />
  <FunctionCode Name="F16.27" Default="100.0" DeftEng="100.0"      Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0.0"			Chinese="操作面板电位计偏置" English="keypad electric level offset" Show="1" />
  <FunctionCode Name="F16.28" Default="110.0" DeftEng="110.0"      Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0.0"			Chinese="操作面板电位计增益" English="keypad electric level gain" Show="1" />
  <FunctionCode Name="F16.29" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F16.30" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F16.31" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F17.00" Default="0:1-8-2格式,无校验,RTU" 	DeftEng="0:1-8-2 format, no verification, RTU"	Max="6" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="数据格式" English="data formate" Show="1" />
  <FunctionCode Name="F17.01" Default="3:9600bps" DeftEng="3:9600bps"		Max="8" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="波特率选择" English="Baud rate selection" Show="1" />
  <FunctionCode Name="F17.02" Default="2" 	DeftEng="2"	Max="247" 		Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="本机地址" English="local address" Show="1" />
  <FunctionCode Name="F17.03" Default="1" 	DeftEng="1"	Max="1000" 		Min="0" 			Attribute="0x2808" 	AbsoluteValue="0"			Chinese="本机应答延时" English="local machine responding delay" Show="1" />
  <FunctionCode Name="F17.04" Default="0.0" DeftEng="0.0"	Max="600.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="通讯超时检出时间" English="communication over-time detection" Show="1" />
  <FunctionCode Name="F17.05" Default="0.0" DeftEng="0.0"	Max="600.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="通讯错误检出时间" English="communication error detection" Show="1" />
  <FunctionCode Name="F17.06" Default="3" 	DeftEng="3"	    Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯超时动作选择" English="communication over-time action selection" Show="1" />
  <FunctionCode Name="F17.07" Default="3" 	DeftEng="3"	    Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯错误时动作选择" English="communication error action " Show="1" />
  <FunctionCode Name="F17.08" Default="1" 	DeftEng="1"  	Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯外部设备故障动作选择" English="communication external fault action" Show="1" />
  <FunctionCode Name="F17.09" Default="01" 	DeftEng="01"    Max="0x11" 	Min="0" 		Attribute="0x2011" 	AbsoluteValue="0"			Chinese="通讯写功能参数存EEPROM选择" English="communication writing function parameter save EEPROM selection" Show="1" />
  <FunctionCode Name="F17.10" Default="0.0" DeftEng="0.0"	Max="600.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="组网通讯超时检出时间" English="Network communication timeout detection time" Show="1" />
  <FunctionCode Name="F17.11" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F17.12" Default="0"   DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.00" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="语言选择" English="language" Show="1" />
  <FunctionCode Name="F18.01" Default="5" 	DeftEng="5"	Max="10" 			Min="1" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="操作面板LCD显示对比度" English="Operation panel LCD display contrast" Show="1" />
  <FunctionCode Name="F18.02" Default="8:给定频率" 	DeftEng="8: Given Frequency"	Max="49" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数1设置" English="Run display parameter 1 setting" Show="1" />
  <FunctionCode Name="F18.03" Default="7:设定频率" 	DeftEng="7: Setting Frequency"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数2设置" English="Run display parameter 2 setting" Show="1" />
  <FunctionCode Name="F18.04" Default="9:输出频率" 	DeftEng="9: Output Frequency"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数3设置" English="Run display parameter 3 setting" Show="1" />
  <FunctionCode Name="F18.05" Default="13:输出电压" DeftEng="13: Output Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数4设置" English="Run display parameter 4 setting" Show="1" />
  <FunctionCode Name="F18.06" Default="14:输出电流" DeftEng="14: Output Current"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数5设置" English="Run display parameter 5 setting" Show="1" />
  <FunctionCode Name="F18.07" Default="18:直流母线电压" DeftEng="18: DC Bus Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数6设置" English="Run display parameter 6 setting" Show="1" />
  <FunctionCode Name="F18.08" Default="7:设定频率" 	DeftEng="7: Setting Frequency"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数1设置" English="Stop display parameter 1 setting" Show="1" />
  <FunctionCode Name="F18.09" Default="18:直流母线电压" DeftEng="18: DC Bus Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数2设置" English="Stop display parameter 2 setting" Show="1" />
  <FunctionCode Name="F18.10" Default="20:AI输入电压" 	DeftEng="20:AI input voltage"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数3设置" English="Stop display parameter 3 setting" Show="1" />
  <FunctionCode Name="F18.11" Default="19:面板电位计输入电压" 	DeftEng="19: panel potentiometer input voltage"	 Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数4设置" English="Stop display parameter 4 setting" Show="1" />
  <FunctionCode Name="F18.12" Default="43:输入端子状态" DeftEng="43: Input Terminal Status"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数5设置" English="Stop display parameter 5 setting" Show="1" />
  <FunctionCode Name="F18.13" Default="44:输出端子状态" DeftEng="44: Output Terminal Status"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数6设置" English="Stop display parameter 6 setting" Show="1" />
  <FunctionCode Name="F18.14" Default="0" 	DeftEng="0" 	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.15" Default="1000" DeftEng="1000"		Max="65535"			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="最大线速度" English="Max line speed" Show="1" />
  <FunctionCode Name="F18.16" Default="0" 	DeftEng="0"	Max="3"			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="线速度显示精度" English="line speed display accuracy" Show="1" />
  <FunctionCode Name="F18.17" Default="0" 	DeftEng="0"	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.18" Default="0" 	DeftEng="0"	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.19" Default="0" 	DeftEng="0"	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.00" Default="0" 	DeftEng="0"	Max="6" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="辅助频率设定通道选择" English="Auxiliary frequency setting channel selection" Show="1" />
  <FunctionCode Name="F19.01" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x2049" 	AbsoluteValue="0"			Chinese="主辅设定运算" English="Primary and secondary setting operations" Show="1" />
  <FunctionCode Name="F19.02" Default="1.00" DeftEng="1.00"	Max="9.99" 		Min="0.00" 		Attribute="0x205c" 	AbsoluteValue="0"			Chinese="辅助设定系数" English="Auxiliary setting factor" Show="0" />
  <FunctionCode Name="F19.03" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 			Attribute="0x616c" 	AbsoluteValue="0"			Chinese="数字辅助频率初值" English="Digital auxiliary frequency initial value" Show="1" />
  <FunctionCode Name="F19.04" Default="0" 	DeftEng="0"	Max="0x11" 		Min="0" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="数字辅助频率控制选择" English="Digital Auxiliary Frequency Control Selection" Show="1" />
  <FunctionCode Name="F19.05" Default="1" 	DeftEng="1"	Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="设定频率比例调整选择" English="Set frequency scaling selection" Show="1" />
  <FunctionCode Name="F19.06" Default="100.0" DeftEng="100.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="设定频率比例调整系数" English="Set frequency scaling factor" Show="0" />
  <FunctionCode Name="F19.07" Default="0:自动停止方式" DeftEng="0: Automatic Stop Method"		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="冷却风扇控制选择" English="Cooling fan control options" Show="1" />
  <FunctionCode Name="F19.08" Default="30.0" DeftEng="30.0"	Max="600.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="冷却风扇控制延迟时间" English="Cooling fan control delay time" Show="1" />
  <FunctionCode Name="F19.09" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.10" Default="1.00" DeftEng="1.00"	Max="400.00" 	Min="0.00" 		Attribute="0xe16c" 	AbsoluteValue="0"			Chinese="零频阈值" English="Zero frequency threshold" Show="0" />
  <FunctionCode Name="F19.11" Default="0:按照频率指令运行" DeftEng="0: Run according to frequency command"		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="设定频率低于零频阈值时动作选择" English="Action selection when the set frequency is lower than the zero frequency threshold" Show="1" />
  <FunctionCode Name="F19.12" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="瞬时失电不停机功能选择" English="Instantaneous power failure without shutdown selection" Show="1" />
  <FunctionCode Name="F19.13" Default="5.00" DeftEng="5.00"	Max="600.00" 	Min="0.01" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="瞬停不停功能减速时间" English="Instantaneous stop function deceleration time" Show="1" />
  <FunctionCode Name="F19.14" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.15" Default="430" DeftEng="430"	Max="999" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="瞬时失电不停机动作判断电压" English="Instantaneous power loss does not stop operation judge voltage" Show="1" />
  <FunctionCode Name="F19.16" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="欠压再起动功能选择" English="Undervoltage restart function selection" Show="0" />
  <FunctionCode Name="F19.17" Default="2.00" DeftEng="2.00"	Max="10.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="欠压再起动等待时间" English="Undervoltage restart waiting time" Show="0" />
  <FunctionCode Name="F19.18" Default="0.500" 	DeftEng="0.500"	Max="1.000" 			Min="0.000" 			Attribute="0x2066" 	AbsoluteValue="0"			Chinese="过压失速增益" English="Overvoltage stall gain" Show="1" />
  <FunctionCode Name="F19.19" Default="740" DeftEng="740"	Max="999" 		Min="0" 			Attribute="0x0398" 	AbsoluteValue="0"			Chinese="过压失速点" English="Overvoltage stall point" Show="1" />
  <FunctionCode Name="F19.20" Default="0.200" 	DeftEng="0.200"	Max="1.000" 			Min="0.000" 			Attribute="0x2066" 	AbsoluteValue="0"			Chinese="自动限流增益" English="Automatic current limit gain" Show="1" />
  <FunctionCode Name="F19.21" Default="150.0" DeftEng="150.0"   Max="200.0" 	Min="20.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="自动限流水平" English="Automatic current limit level" Show="1" />
  <FunctionCode Name="F19.22" Default="0.02" DeftEng="0.02"	Max="1.000" 	Min="0.000" 		Attribute="0x2066" 	AbsoluteValue="0"			Chinese="自动限流积分常数" English="Automatic current limiting integral constant" Show="1" />
  <FunctionCode Name="F19.23" Default="0:上升沿有效" DeftEng="0: rising edge active"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="端子运行命令有效模式" English="Terminal operation command effective mode" Show="1" />
  <FunctionCode Name="F19.24" Default="720" DeftEng="720"	Max="750" 		Min="630" 		Attribute="0x0398" 	AbsoluteValue="0"			Chinese="制动单元动作电压" English="Braking unit operating voltage" Show="1" />
  <FunctionCode Name="F19.25" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="磁通制动使能" English="Flux brake enable" Show="1" />
  <FunctionCode Name="F19.26" Default="0" 	DeftEng="0"	Max="65535" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="设定长度" English="Set length" Show="1" />
  <FunctionCode Name="F19.27" Default="0" 	DeftEng="0"	Max="65535" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="实际长度" English="Actual length" Show="1" />
  <FunctionCode Name="F19.28" Default="1.000" DeftEng="1.000" Max="30.000" 	Min="0.001" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="长度倍率" English="Length magnification" Show="0" />
  <FunctionCode Name="F19.29" Default="1.000" DeftEng="1.000" Max="1.000" 	Min="0.001" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="长度校正系数" English="Length correction factor" Show="0" />
  <FunctionCode Name="F19.30" Default="10.00" DeftEng="10.00" Max="100.00" 	Min="1.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="测量轴直径" English="Measuring shaft diameter" Show="0" />
  <FunctionCode Name="F19.31" Default="1" 	DeftEng="1"	Max="9999" 		Min="1" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="轴每转脉冲" English="Axis per revolution" Show="1" />
  <FunctionCode Name="F19.32" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="长度到达输出功能选择" English="Length reach output function selection" Show="1" />
  <FunctionCode Name="F19.33" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="长度到达后记录长度处理" English="After the length reaches the record length processing" Show="1" />
  <FunctionCode Name="F19.34" Default="0" 	DeftEng="0"	Max="1" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="停机时记录长度处理" English="Recording length processing when shutting down" Show="1" />
  <FunctionCode Name="F19.35" Default="0.0" DeftEng="0.0"		Max="100.0" 			Min="0.0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="辅助PID输出限定" English="Auxiliary PID output limitation" Show="1" />
  <FunctionCode Name="F19.36" Default="0.0" DeftEng="0.0"		Max="100.0" 			Min="0.0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="辅助PID输出限定提升量" English="Auxiliary PID output limits lift" Show="1" />
  <FunctionCode Name="F19.37" Default="0" 	DeftEng="0"	 Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.38" Default="2000" DeftEng="2000"		Max="10000" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="相间短路检测动作选择" English="Phase-to-phase short-circuit detection action selection" Show="1" />
  <FunctionCode Name="F19.39" Default="00" 	 DeftEng="00"   Max="0x12" 	Min="00" 		Attribute="0x2091" 	AbsoluteValue="0"			Chinese="输入电压选择" English="Input voltage selection" Show="1" />
  <FunctionCode Name="F19.40" Default="0" 	DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.41" Default="0" 	DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.42" Default="0" 	DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.43" Default="0" 	DeftEng="0"    Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.44" Default="5.0" DeftEng="5.0"	Max="999.9" 	Min="0.0" 		Attribute="0x3862" 	AbsoluteValue="0"			Chinese="LCD背光显示时间" English="LCD backlight display time" Show="1" />
  <FunctionCode Name="F20.00" Default="00000" DeftEng="00000" Max="11111" 	Min="00000" 			Attribute="0x2068" 	AbsoluteValue="0"			Chinese="过载报警选择" English="Overload alarm selection" Show="1" />
  <FunctionCode Name="F20.01" Default="150.0" DeftEng="150.0" Max="200.0" 	Min="20.0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="过载预报警检出水平" English="Overload pre-alarm detection level" Show="0" />
  <FunctionCode Name="F20.02" Default="5.0" DeftEng="5.0"	Max="60.0" 		Min="0.0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="过载预报警检出时间" English="Overload pre-alarm detection time" Show="0" />
  <FunctionCode Name="F20.03" Default="0" 	DeftEng="0" 	Max="4" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出动作选择" English="Inverter output load detection action selection" Show="1" />
  <FunctionCode Name="F20.04" Default="30" 	DeftEng="30"	Max="100" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出水平" English="Inverter output off load detection level" Show="1" />
  <FunctionCode Name="F20.05" Default="1.00" DeftEng="1.00"	Max="20.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出时间" English="Inverter output load out detection time" Show="0" />
  <FunctionCode Name="F20.06" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机过热信号输入类型" English="Motor overheat signal input type" Show="1" />
  <FunctionCode Name="F20.07" Default="0" DeftEng="0"	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机过热热敏电阻值" English="Motor overheat Thermistor value" Show="1" />
  <FunctionCode Name="F20.08" Default="6" DeftEng="6"		Max="80" 			Min="0" 			Attribute="0x0548" 	AbsoluteValue="0"			Chinese="输入缺相检测基准" English="Input phase loss detection standard" Show="1" />
  <FunctionCode Name="F20.09" Default="2.00" DeftEng="2.00"	Max="5.00" 		Min="1.00" 		Attribute="0x065c" 	AbsoluteValue="0"			Chinese="输入缺相检测时间" English="Input phase loss detection time" Show="0" />
  <FunctionCode Name="F20.10" Default="20" 	DeftEng="20"	Max="50" 			Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="输出缺相检测基准" English="Output phase loss detection standard" Show="1" />
  <FunctionCode Name="F20.11" Default="3.00" DeftEng="3.00"	Max="20.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="输出缺相检测时间" English="Output phase loss detection time" Show="1" />
  <FunctionCode Name="F20.12" Default="0" 	DeftEng="0"	Max="100" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID给定丢失检出值" English="PID given missing detection value" Show="1" />
  <FunctionCode Name="F20.13" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID给定丢失检出时间" English="PID given lost detection time" Show="0" />
  <FunctionCode Name="F20.14" Default="0" 	DeftEng="0"	Max="100" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出值" English="Loss of PID feedback detection" Show="1" />
  <FunctionCode Name="F20.15" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出时间" English="Loss of PID feedback detection time" Show="0" />
  <FunctionCode Name="F20.16" Default="100" DeftEng="100"	Max="100" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID反馈超限检出值" English="PID feedback limit detection value" Show="1" />
  <FunctionCode Name="F20.17" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="PID反馈超限检出时间" English="PID feedback limit detection time" Show="0" />
  <FunctionCode Name="F20.18" Default="0" DeftEng="0"		Max="100" 		Min="0" 			Attribute="0x2098" 	AbsoluteValue="0"			Chinese="自动复位次数" English="Automatic reset times" Show="1" />
  <FunctionCode Name="F20.19" Default="5.0" DeftEng="5.0"	Max="20.0" 		Min="2.0" 		Attribute="0x269a" 	AbsoluteValue="0"			Chinese="自动复位间隔时间" English="Automatic reset interval" Show="1" />
  <FunctionCode Name="F20.20" Default="00" 	DeftEng="00"	Max="0x11" 		Min="00" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="故障继电器动作选择" English="Fault relay action selection" Show="1" />
  <FunctionCode Name="F20.21" Default="0" 	DeftEng="0"	 Max="34" 			Min="0" 			Attribute="0x0008" 	AbsoluteValue="0"			Chinese="第五次（最近一次）故障类型" English="Fifth (most recent) fault type" Show="1" />
  <FunctionCode Name="F20.22" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时设定频率" English="Set frequency at the last fault" Show="1" />
  <FunctionCode Name="F20.23" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时输出频率" English="output frequency at the last fault" Show="1" />
  <FunctionCode Name="F20.24" Default="0" 	DeftEng="0"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时直流母线电压" English="DC bus voltage at the last fault" Show="1" />
  <FunctionCode Name="F20.25" Default="0" 	DeftEng="0"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电压" English="output voltageat the last fault" Show="1" />
  <FunctionCode Name="F20.26" Default="0.00" DeftEng="0.00"	Max="99.99" 	Min="0.00" 		Attribute="0x0222" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电流" English="output current at the last fault" Show="1" />
  <FunctionCode Name="F20.27" Default="0" 	DeftEng="0"	Max="0x1ff" 	Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输入端子状态" English="input terminals states at the last fault" Show="1" />
  <FunctionCode Name="F20.28" Default="0" 	DeftEng="0"	Max="0x3f" 		Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输出端子状态" English="output terminals states at the last fault" Show="1" />
  <FunctionCode Name="F20.29" Default="0.0" DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="最近一次故障间隔时间" English="interval time Last failures" Show="1" />
  <FunctionCode Name="F20.30" Default="0" 	DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第四次故障类型" English="the fourth fault type" Show="1" />
  <FunctionCode Name="F20.31" Default="0.0" DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第四次故障间隔时间" English="interval time of the fourth fault" Show="1" />
  <FunctionCode Name="F20.32" Default="0" 	DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第三次故障类型" English="the third fault" Show="1" />
  <FunctionCode Name="F20.33" Default="0.0" DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第三次故障间隔时间" English="interval time of the third fault" Show="1" />
  <FunctionCode Name="F20.34" Default="0" 	DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第二次故障类型" English="the second fault type" Show="1" />
  <FunctionCode Name="F20.35" Default="0.0" DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第二次故障间隔时间" English="interval time of the second fault" Show="1" />
  <FunctionCode Name="F20.36" Default="0" 	DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第一次故障类型" English="the 1st fault type" Show="1" />
  <FunctionCode Name="F20.37" Default="0.0" DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第一次故障间隔时间" English="interval time of the 1st fault" Show="1" />
  <FunctionCode Name="F20.38" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F20.39" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F20.40" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F23.00" Default="4" DeftEng="4"	Max="16" 			Min="1" 			Attribute="0x0948" 	AbsoluteValue="0"			Chinese="载波频率设定" English="carrier frequency set" Show="1" />
  <FunctionCode Name="F23.01" Default="0:禁止载波频率自动调整" DeftEng="0: Disable automatic adjustment of carrier frequency"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="载波频率自动调整选择" English="Carrier frequency automatic adjustment selection" Show="1" />
  <FunctionCode Name="F23.02" Default="1:过调制使能有效" DeftEng="1: Overmodulation enabled"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PWM过调制使能" English="PWM overmodulation enable" Show="1" />
  <FunctionCode Name="F23.03" Default="0:两相调制/三相调制切换" DeftEng="0: Two-phase modulation/three-phase modulation switching"		Max="1" 			Min="0" 			Attribute="0x0088" 	AbsoluteValue="0"			Chinese="PWM调制模式" English="PWM modulation mode" Show="1" />
  <FunctionCode Name="F23.04" Default="5.00" DeftEng="5.00"	Max="50.00" 	Min="5.00" 	Attribute="0x01a4" 	AbsoluteValue="0"			Chinese="PWM调制模式切换点1" English="PWM modulation mode switching point 1" Show="1" />
  <FunctionCode Name="F23.05" Default="10.00" DeftEng="10.00"	Max="50.00" 	Min="7.00" 	Attribute="0x01a4" 	AbsoluteValue="0"			Chinese="PWM调制模式切换点2" English="PWM modulation mode switching point 2" Show="1" />
  <FunctionCode Name="F23.06" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F23.07" Default="0" DeftEng="0"	Max="65535" 	Min="0" 		Attribute="0x00a8" 	AbsoluteValue="0"			Chinese="硬件故障屏蔽密码保护" English="Hardware Fault shielding Password Protection" Show="0" />
  <FunctionCode Name="F23.08" Default="0" DeftEng="0"	Max="0xffff" 	Min="0" 		Attribute="0x00a1" 	AbsoluteValue="0"			Chinese="硬件故障屏蔽" English="hardware fault shielding" Show="0" />
  <FunctionCode Name="F23.09" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="R02.00" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x0364" 	AbsoluteValue="0.00"			Chinese="AI1显示电压1" English="AI1 display voltage 1" Show="0" />
  <FunctionCode Name="R02.01" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x0364" 	AbsoluteValue="0.00"			Chinese="AI1实测电压1" English="AI1 detected voltage 1" Show="0" />
  <FunctionCode Name="R02.02" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x0364" 	AbsoluteValue="0.00"			Chinese="AI1显示电压2" English="AI1 display voltage 2" Show="0" />
  <FunctionCode Name="R02.03" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x0364" 	AbsoluteValue="0.00"			Chinese="AI1实测电压2" English="AI1 detected voltage 2" Show="0" />
</FuncGroup>