<?xml version="1.0" encoding="utf-8"?>
<!--This is FunctionCode Struct-->
<FuncGroup>
  <FunctionCode Name="F00.00" Default="0:速度控制" 	DeftEng="0: Speed Control"	  Max="1" 			Min="0" 			Attribute="0x2088"	AbsoluteValue="0"			Chinese="控制模式选择" English="Control Mode Select" Show="1" />
  <FunctionCode Name="F00.01" Default="0:无PG的V/f控制" DeftEng="0: V/f control without PG"		Max="2" 			Min="0" 			Attribute="0x2088"	AbsoluteValue="0"			Chinese="电机1控制方式选择" English="Motor 1 control mode selection" Show="1" />
  <FunctionCode Name="F00.02" Default="0:G型机" DeftEng="0:G Model"		Max="1" 			Min="0" 			Attribute="0x2088"	AbsoluteValue="0"			Chinese="变频器机型设定" English="Inverter model setting" Show="1" />
  <FunctionCode Name="F00.03" Default="0:电机1" DeftEng="0: Motor 1"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机选择" English="Motor Select" Show="1" />
  <FunctionCode Name="F00.04" Default="2:HD30-WIO扩展卡有效" DeftEng="0: HD30-WIO extension card valid"		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="HD30通用扩展卡选择" English="HD31 Universal Expansion Card Selection" Show="1" />
  <FunctionCode Name="F00.05" Default="0:无扩展应用功能" DeftEng="0:No extended application function"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="HD30扩展应用功能" English="HD31 extended application function" Show="1" />
  <FunctionCode Name="F00.06" Default="50.00"	DeftEng="50.00" Max="400.00" 	Min="50.00"		Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="变频器最大输出频率" English="Maximum Output Frequency of Inverter" Show="1" />
  <FunctionCode Name="F00.07" Default="0:数字设定" DeftEng="0: Digital Setting"		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="上限运行频率设定通道" English="upper limit operating frequency setting channel" Show="1" />
  <FunctionCode Name="F00.08" Default="50.00" DeftEng="50.00" Max="F00.06" 	Min="0.00" 		Attribute="0x619c" 	AbsoluteValue="0"			Chinese="上限运行频率" English="upper limit operating frequency" Show="1" />
  <FunctionCode Name="F00.09" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x219c" 	AbsoluteValue="0"			Chinese="下限运行频率" English="lower limit operating frequency" Show="1" />
  <FunctionCode Name="F00.10" Default="0:操作面板设定" DeftEng="0: Operation Panel Settings"		Max="10" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="频率设定通道选择" English="Frequency setting channel selection" Show="1" />
  <FunctionCode Name="F00.11" Default="0:操作面板运行命令通道" DeftEng="0: Operation panel operation command channel"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="命令设定通道选择" English="Command Set Channel Selection" Show="1" />
  <FunctionCode Name="F00.12" Default="2:多功能键无效" DeftEng="2: Invalid Multifunction Key"		Max="3" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="多功能键功能选择" English="Multifunction Key Function Selection" Show="1" />
  <FunctionCode Name="F00.13" Default="50.00" DeftEng="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa15c" 	AbsoluteValue="0"			Chinese="初始运行频率数字设定" English="initial operating frequency of the digital setting" Show="1" />
  <FunctionCode Name="F00.14" Default="0x1001" DeftEng="0x1001"  Max="0x1111" 	Min="0x0000" 	Attribute="0x20a1" 	AbsoluteValue="0"			Chinese="频率设定控制" English="Frequency Setting Control" Show="1" />
  <FunctionCode Name="F00.15" Default="5.00" DeftEng="5.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa15c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定1" English="Operation Frequency Digital Setting 1" Show="1" />
  <FunctionCode Name="F00.16" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2692" 	AbsoluteValue="0"			Chinese="点动运行间隔时间" English="Inching Run Interval" Show="1" />
  <FunctionCode Name="F00.17" Default="0:方向一致" DeftEng="0: Uniform Direction"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="运行方向选择" English="Run Direction Select" Show="1" />
  <FunctionCode Name="F00.18" Default="0:允许反转" DeftEng="0: Allow Reverse"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="防反转选择" English="Anti-reverse selection" Show="1" />
  <FunctionCode Name="F00.19" Default="0.0" DeftEng="0.0"	Max="3600.0" 	Min="0.0" 		Attribute="0x26aa" 	AbsoluteValue="0"			Chinese="正反转死区时间" English="Reversal of dead time" Show="1" />
  <FunctionCode Name="F00.20" Default="0:使能" DeftEng="0: Enable"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="外引面板按键使能" English="External panel button enabled" Show="1" />
  <FunctionCode Name="F00.21" Default="0:禁止" DeftEng="0: Disable"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="休眠功能使能" English="Sleep function enabled" Show="1" />
  <FunctionCode Name="F00.22" Default="1.0" DeftEng="1.0"	Max="6000.0" 	Min="0.0" 		Attribute="0x2692" 	AbsoluteValue="0"			Chinese="休眠唤醒时间" English="Dormancy wake up time" Show="1" />
  <FunctionCode Name="F00.23" Default="0" DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F00.24" Default="1.0" DeftEng="1.0"	Max="6000.0" 	Min="0.0" 		Attribute="0x2692" 	AbsoluteValue="0"			Chinese="休眠延迟时间" English="Sleep delay time" Show="1" />
  <FunctionCode Name="F00.25" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa15c" 	AbsoluteValue="0"			Chinese="休眠频率" English="Sleep Frequency" Show="1" />
  <FunctionCode Name="F00.26" Default="111" DeftEng="111"	Max="332" 	Min="000" 		Attribute="0x2099" 	AbsoluteValue="0"			Chinese="变频器零频运行动作选择" English="nverter Zero Frequency Operation Select" Show="1" />
  <FunctionCode Name="F00.27" Default="000" DeftEng="000"	Max="ddd" 	Min="000" 		Attribute="0x2099" 	AbsoluteValue="0"			Chinese="命令源绑定频率源选择" English="Command source binding frequency source selection" Show="1" />
  <FunctionCode Name="F00.28" Default="0:只在操作面板控制下有效" DeftEng="0: Only available under control of the operation panel"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="STOP键停机功能选择" English="STOP button selects" Show="1" />
  <FunctionCode Name="F00.29" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F01.00" Default="00000" DeftEng="00000"		Max="65535" 	Min="00000" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户密码" English="user password" Show="1" />
  <FunctionCode Name="F01.01" Default="0x010" DeftEng="0x010"	Max="0x111" 		Min="0x000" 	  Attribute="0x2059" 	AbsoluteValue="0"			Chinese="菜单模式选择" English="Menu Mode Select" Show="1" />
  <FunctionCode Name="F01.02" Default="0:无操作" DeftEng="0: No action"		Max="6" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="功能码参数初始化（参数下载）" English="unction Code Parameter Initialization (Parameter Download)" Show="1" />
  <FunctionCode Name="F01.03" Default="0:无操作" DeftEng="0: No action"		Max="2" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="参数复制到操作面板（参数上传）" English="Parameter Copy to Operation Panel (Parameter Upload)" Show="1" />
  <FunctionCode Name="F01.04" Default="0" DeftEng="0"		Max="65535" 			Min="0" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户权限密码1" English="User Authority Password 1" Show="0" />
  <FunctionCode Name="F01.05" Default="0" DeftEng="0"		Max="9999" 			Min="0" 			Attribute="0x0062" 	AbsoluteValue="0"			Chinese="用户允许运行时间1" English="User Allowed Runtime 1" Show="0" />
  <FunctionCode Name="F01.06" Default="0" DeftEng="0"		Max="1" 			Min="0" 			Attribute="0x0048" 	AbsoluteValue="0"			Chinese="用户状态1" English="User Status1" Show="0" />
  <FunctionCode Name="F01.07" Default="0" DeftEng="0"		Max="65535" 			Min="0" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户权限密码2" English="User Authority Password 2" Show="0" />
  <FunctionCode Name="F01.08" Default="0" DeftEng="0"		Max="9999" 			Min="0" 			Attribute="0x0062" 	AbsoluteValue="0"			Chinese="用户允许运行时间2" English="User Allowed Runtime 2" Show="0" />
  <FunctionCode Name="F01.09" Default="0" DeftEng="0"		Max="1" 			Min="0" 			Attribute="0x0048" 	AbsoluteValue="0"			Chinese="用户状态2" English="User Status2" Show="0" />
  <FunctionCode Name="F01.10" Default="0" DeftEng="0"		Max="65535" 			Min="0" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户权限密码3" English="User Authority Password 3" Show="0" />
  <FunctionCode Name="F01.11" Default="0" DeftEng="0"		Max="9999" 			Min="0" 			Attribute="0x0062" 	AbsoluteValue="0"			Chinese="用户允许运行时间3" English="User Allowed Runtime 3" Show="0" />
  <FunctionCode Name="F01.12" Default="0" DeftEng="0"		Max="1" 			Min="0" 			Attribute="0x0048" 	AbsoluteValue="0"			Chinese="用户状态3" English="User Status3" Show="0" />
  <FunctionCode Name="F02.00" Default="0:从起动DWELL频率起动" DeftEng="0: Start from the start DWELL frequency"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="起动方式" English="Starting Mode" Show="1" />
  <FunctionCode Name="F02.01" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动延迟时间" English="Start Delay" Show="1" />
  <FunctionCode Name="F02.02" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="起动DWELL频率设定" English="Start DWELL Frequency Setting" Show="1" />
  <FunctionCode Name="F02.03" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动DWELL频率保持时间" English="Start DWELL Frequency Hold Time" Show="1" />
  <FunctionCode Name="F02.04" Default="50" 	DeftEng="50"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="直流制动电流设定" English="DC braking current setting" Show="1" />
  <FunctionCode Name="F02.05" Default="0.50" DeftEng="0.50"	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动直流制动时间" English="Starting DC Braking Time" Show="1" />
  <FunctionCode Name="F02.06" Default="0.000" DeftEng="0.000"		Max="2.000" 			Min="0.000" 			Attribute="0x2166" 	AbsoluteValue="0"			Chinese="飞速跟踪结果补偿量" English="Speed Tracking Result Compensation" Show="1" />
  <FunctionCode Name="F02.07" Default="1:基于电压搜索" 	DeftEng="1:Voltage based search"	Max="1" 		Min="1" 		Attribute="0x2088" 	AbsoluteValue="0"		Chinese="转速跟踪模式选择" English="Speed tracking mode selection" Show="1" />
  <FunctionCode Name="F02.08" Default="0:无效" 				DeftEng="0:Invalid"					Max="1" 		Min="0" 		Attribute="0x0088" 	AbsoluteValue="0"		Chinese="电压自学习" English="Voltage self-learning" Show="1" />
  <FunctionCode Name="F02.09" Default="0:不取反" 			DeftEng="0:"						Max="1" 		Min="0" 		Attribute="0x0088" 	AbsoluteValue="0"		Chinese="搜索频率方向取反" English="Search frequency direction is reversed" Show="1" />
  <FunctionCode Name="F02.10" Default="15.0" 		DeftEng="15.0"		Max="60.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"		Chinese="转速搜索起动阀值" English="Speed search start threshold" Show="1" />
  <FunctionCode Name="F02.11" Default="30.0" 		DeftEng="30.0"		Max="100" 		Min="0" 		Attribute="0x2558" 	AbsoluteValue="0"		Chinese="电压差值" English="The voltage difference" Show="1" />
  <FunctionCode Name="F02.12" Default="0" 			DeftEng="0"			Max="5.0" 		Min="0.0" 		Attribute="0x2652" 	AbsoluteValue="0"		Chinese="转速搜索出后处理时间" English="Processing time after the speed is searched out" Show="1" />
  <FunctionCode Name="F02.13" Default="0:减速停机" DeftEng="0: Slow Down"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="速度控制停机方式" English="Speed Control Stop Mode" Show="1" />
  <FunctionCode Name="F02.14" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="停机DWELL频率设定" English="Shutdown DWELL Frequency Setting" Show="1" />
  <FunctionCode Name="F02.15" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机DWELL频率保持时间" English="Stop DWELL Frequency Hold Time" Show="1" />
  <FunctionCode Name="F02.16" Default="0.50" DeftEng="0.50"	Max="50.00" 	Min="0.00" 		Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="停机直流制动起始频率" English="Stop DC braking start frequency" Show="1" />
  <FunctionCode Name="F02.17" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机直流制动等待时间" English="Stop DC Braking Wait Time" Show="1" />
  <FunctionCode Name="F02.18" Default="0.50" DeftEng="0.50"	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机直流制动时间" English="Stop DC braking time" Show="1" />
  <FunctionCode Name="F02.19" Default="10"   DeftEng="10"	Max="11" 	Min="00" 		Attribute="0x2091" 	AbsoluteValue="0"			Chinese="点动控制方式" English="ogging Control Mode" Show="1" />
  <FunctionCode Name="F02.20" Default="0.50" DeftEng="0.50"	Max="0.50" 	Min="0.00" 		Attribute="0x269c" 	AbsoluteValue="0"			Chinese="预励磁时间" English="Pre-excitation time" Show="1" />
  <FunctionCode Name="F02.21" Default="0.00" 	 DeftEng="0.00"	Max="20.00" 			Min="0.00" 			Attribute="0x2164" 	AbsoluteValue="0"			Chinese="电压判断频率阈值" English="Voltage pressure judgment frequency threshold" Show="1" />
  <FunctionCode Name="F02.22" Default="0:限制转速根据频率变化方向" 	 DeftEng="0:Limit the speed according to the direction of frequency change"	Max="0" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="频率方向限制" English="Frequency direction limitation" Show="1" />
  <FunctionCode Name="F02.23" Default="0" 	 DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F03.00" Default="00" 	 DeftEng="00"	Max="11" 			Min="00" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="加减速方式选择" English="Acceleration/deceleration mode selection" Show="1" />
  <FunctionCode Name="F03.01" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间1" English="Acceleration time 1" Show="1" />
  <FunctionCode Name="F03.02" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间1" English="Deceleration Time 1" Show="1" />
  <FunctionCode Name="F03.03" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间2" English="Acceleration time 2" Show="1" />
  <FunctionCode Name="F03.04" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间2" English="Deceleration Time 2" Show="1" />
  <FunctionCode Name="F03.05" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间3" English="Acceleration time 3" Show="1" />
  <FunctionCode Name="F03.06" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间3" English="Deceleration Time 3" Show="1" />
  <FunctionCode Name="F03.07" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加速时间4" English="Acceleration time 4" Show="1" />
  <FunctionCode Name="F03.08" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减速时间4" English="Deceleration Time 4" Show="1" />
  <FunctionCode Name="F03.09" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="加速时间2和1切换频率" English="switching frequency Acceleration time 1 and 2" Show="1" />
  <FunctionCode Name="F03.10" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="减速时间2和1切换频率" English="switching frequency Deceleration time 1 and 2" Show="1" />
  <FunctionCode Name="F03.11" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="加速开始时S字特性时间" English="S-characteristic time at the beginning of acceleration" Show="1" />
  <FunctionCode Name="F03.12" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="加速结束时S字特性时间" English="S-characteristic time at the end of acceleration" Show="1" />
  <FunctionCode Name="F03.13" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="减速开始时S字特性时间" English="S-characteristic time when deceleration starts" Show="1" />
  <FunctionCode Name="F03.14" Default="0.20" DeftEng="0.20"	Max="2.50" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="减速结束时S字特性时间" English="S-characteristic time at the end of deceleration" Show="1" />
  <FunctionCode Name="F03.15" Default="6.0"  DeftEng="6.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="点动加速时间" English="Inching acceleration time" Show="1" />
  <FunctionCode Name="F03.16" Default="6.0"  DeftEng="6.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="点动减速时间" English="Inching deceleration time" Show="1" />
  <FunctionCode Name="F03.17" Default="10.0" DeftEng="10.0"	Max="6000.0" 	Min="0.1" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="紧急停机减速时间" English="Emergency stop deceleration time" Show="1" />
  <FunctionCode Name="F03.18" Default="0" 	 DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F03.19" Default="0" 	 DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F03.20" Default="0" 	 DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="Reserved" Show="1" />
  <FunctionCode Name="F04.00" Default="0:PID控制无效" DeftEng="0: invalid PID control"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="过程PID控制选择" English="Process PID Control Selection" Show="1" />
  <FunctionCode Name="F04.01" Default="0:数字给定" DeftEng="0: digital given"		Max="8" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="给定通道选择" English="given channel selection" Show="1" />
  <FunctionCode Name="F04.02" Default="0:模拟量反馈" DeftEng="0: Analog Feedback"		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="反馈通道选择" English="Feedback Channel Selection" Show="1" />
  <FunctionCode Name="F04.03" Default="0.0" DeftEng="0.0"		Max="+100.0" 	Min="-100.0"	Attribute="0x255a" 	AbsoluteValue="100.0"	Chinese="给定量数字设定" English="Set a quantitative figure" Show="1" />
  <FunctionCode Name="F04.04" Default="50.0" DeftEng="50.0"	Max="500.0" 	Min="0.0" 		Attribute="0x2052" 	AbsoluteValue="0"			Chinese="比例增益（P1）" English="Proportional Gain (P1)" Show="1" />
  <FunctionCode Name="F04.05" Default="1.00" DeftEng="1.00"	Max="10.00" 	Min="0.01" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="积分时间（I1）" English="Integral Time (I1)" Show="1" />
  <FunctionCode Name="F04.06" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0xa552" 	AbsoluteValue="0"			Chinese="积分项上限" English="Maximum Integral Term" Show="1" />
  <FunctionCode Name="F04.07" Default="0.00" DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="微分时间（D1）" English="Differential Time (D1)" Show="1" />
  <FunctionCode Name="F04.08" Default="20.0" DeftEng="20.0" Max="100.0" 	Min="0.0" 		Attribute="0xa552" 	AbsoluteValue="0"			Chinese="微分限幅值" English="Differential Limit" Show="1" />
  <FunctionCode Name="F04.09" Default="0.10" DeftEng="0.10"	Max="50.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="采样周期（T）" English="Sampling Period(T)" Show="1" />
  <FunctionCode Name="F04.10" Default="0.0"  DeftEng="0.0"	Max="20.0" 		Min="0.0" 		Attribute="0x2552" 	AbsoluteValue="0"			Chinese="偏差极限" English="deviation limit" Show="1" />
  <FunctionCode Name="F04.11" Default="0:由F04.13设定" DeftEng="0: Set by F04.13"		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器上限通道选择" English="PID Regulator Upper Channel Select" Show="1" />
  <FunctionCode Name="F04.12" Default="0:由F04.14设定" DeftEng="0: Set by F04.14"	Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器下限通道选择" English="PID Regulator Lower Channel Select" Show="1" />
  <FunctionCode Name="F04.13" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0xa592" 	AbsoluteValue="0"			Chinese="PID调节器上限值" English="PID Regulator Upper Limit" Show="1" />
  <FunctionCode Name="F04.14" Default="0.0"   DeftEng="0.0"	  Max="100.0" 	Min="0.0" 		Attribute="0xa592" 	AbsoluteValue="0"			Chinese="PID调节器下限值" English="PID regulator lower limit value" Show="1" />
  <FunctionCode Name="F04.15" Default="0:正特性" DeftEng="0: Positive Characteristics"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器调节特性" English="PID Regulator Adjustment Characteristics" Show="1" />
  <FunctionCode Name="F04.16" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F04.17" Default="0.05" DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="PID输出滤波时间" English="PID output filter time" Show="1" />
  <FunctionCode Name="F04.18" Default="0:PID调节禁止反转" DeftEng="0: PID adjustment prohibited to reverse"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID输出反转选择" English="PID output reversal selection" Show="1" />
  <FunctionCode Name="F04.19" Default="100.0" DeftEng="100.0"  Max="100.0" 	Min="0.0" 		Attribute="0xa592" 	AbsoluteValue="0"			Chinese="PID输出反转频率上限" English="limit the PID output inversion frequency" Show="1" />
  <FunctionCode Name="F04.20" Default="50.0"  DeftEng="50.0"	Max="500.0" 	Min="0.0" 		Attribute="0x2052" 	AbsoluteValue="0"			Chinese="比例增益（P2）" English="Proportional Gain (P2)" Show="1" />
  <FunctionCode Name="F04.21" Default="1.00"  DeftEng="1.00"	Max="10.00" 	Min="0.01" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="积分时间（I2）" English="Integral Time (I2)" Show="1" />
  <FunctionCode Name="F04.22" Default="0.00"  DeftEng="0.00"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="微分时间（D2）" English="Differential Time (D2)" Show="1" />
  <FunctionCode Name="F04.23" Default="0:不调整" DeftEng="0: Do not adjust"		Max="3" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="PID参数调整依据" English="PID parameter adjustment" Show="1" />
  <FunctionCode Name="F04.24" Default="0.0" DeftEng="0.0" Max="F04.25" 	Min="0.0" 		Attribute="0x2552" 	AbsoluteValue="0"			Chinese="PID参数切换点1" English="PID switching point 1" Show="1" />
  <FunctionCode Name="F04.25" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="F04.24" 		Attribute="0x2552" 	AbsoluteValue="0"			Chinese="PID参数切换点2" English="PID parameter switching point 2" Show="1" />
  <FunctionCode Name="F04.26" Default="0" DeftEng="0"		Max="24000" 			Min="0" 			Attribute="0x2468" 	AbsoluteValue="0"			Chinese="速度闭环给定" English="Speed Closed Loop Given" Show="1" />
  <FunctionCode Name="F04.27" Default="1024" DeftEng="1024" Max="9999" 	Min="1" 		Attribute="0x2088" 	AbsoluteValue="0"			Chinese="每转脉冲数" English="Number of pulses per revolution" Show="1" />
  <FunctionCode Name="F04.28" Default="1500" DeftEng="1500" Max="24000" 	Min="1" 		Attribute="0x2488" 	AbsoluteValue="0"			Chinese="最大闭环速度" English="Max Closed Loop Speed" Show="1" />
  <FunctionCode Name="F04.29" Default="0:停机时不运算" DeftEng="0: No operation when stopped"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID运算模式" English="PID operation mode" Show="1" />
  <FunctionCode Name="F04.30" Default="0:休眠禁止" DeftEng="0: Do not sleep"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID休眠使能" English="PID Sleep Enable" Show="1" />
  <FunctionCode Name="F04.31" Default="10.0" DeftEng="10.0" Max="100.0" 	Min="0.0" 		Attribute="0x2552" 	AbsoluteValue="0"			Chinese="唤醒容差" English="Wake Tolerance" Show="1" />
  <FunctionCode Name="F04.32" Default="0.0"  DeftEng="0.0"	Max="6000.0" 	Min="0.0" 		Attribute="0x2652" 	AbsoluteValue="0"			Chinese="唤醒延时" English="Wake-up delay" Show="1" />
  <FunctionCode Name="F04.33" Default="10.0" DeftEng="10.0" Max="100.0" 	Min="0.0" 		Attribute="0x2552" 	AbsoluteValue="0"			Chinese="休眠容差" English="Sleep Tolerance" Show="1" />
  <FunctionCode Name="F04.34" Default="0.0"  DeftEng="0.0"	Max="6000.0" 	Min="0.0" 		Attribute="0x2652" 	AbsoluteValue="0"			Chinese="休眠延时" English="Wake-up delay" Show="1" />
  <FunctionCode Name="F04.35" Default="20.00" DeftEng="20.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa15c" 	AbsoluteValue="0"			Chinese="休眠频率" English="Sleep Frequency" Show="1" />
  <FunctionCode Name="F04.36" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F05.00" Default="33333" DeftEng="33333" Max="33333" 	Min="00000" 			Attribute="0x20a8" 	AbsoluteValue="0"			Chinese="外部给定量曲线选择" English="External Quantitative Curve Selection" Show="1" />
  <FunctionCode Name="F05.01" Default="0.0" DeftEng="0.0"	Max="F05.03" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最小给定" English="Line 1 Minimum Given" Show="1" />
  <FunctionCode Name="F05.02" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最小给定对应值" English="Line 1 Minimum Given Value " Show="1" />
  <FunctionCode Name="F05.03" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="F05.01" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最大给定" English="Line 1 Maximum Given" Show="1" />
  <FunctionCode Name="F05.04" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最大给定对应值" English="Line 1 Maximum Given Value" Show="1" />
  <FunctionCode Name="F05.05" Default="0.0" DeftEng="0.0"	Max="F05.07" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最小给定" English="Line 2 Minimum Given" Show="1" />
  <FunctionCode Name="F05.06" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最小给定对应值" English="Line 2 Minimum Given Value" Show="1" />
  <FunctionCode Name="F05.07" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="F05.05" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最大给定" English="Line 2 Maximum Given" Show="1" />
  <FunctionCode Name="F05.08" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最大给定对应值" English="Line 2 maximum given value" Show="1" />
  <FunctionCode Name="F05.09" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="F05.11" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定" English="Maximum Given Line" Show="1" />
  <FunctionCode Name="F05.10" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定对应值" English="The maximum given value for polyline " Show="1" />
  <FunctionCode Name="F05.11" Default="100.0" DeftEng="100.0" Max="F05.09" 	Min="F05.13" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点2给定" English="Guideline inflection point 2 given" Show="1" />
  <FunctionCode Name="F05.12" Default="100.0" DeftEng="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点2对应值" English="Corresponding to Inflection 2" Show="1" />
  <FunctionCode Name="F05.13" Default="0.0" DeftEng="0.0"	Max="F05.11" 	Min="F05.15" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点1给定" English="Polygonal Inflection Point 1 Given" Show="1" />
  <FunctionCode Name="F05.14" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点1对应值" English="Corresponding to Inflection 1" Show="1" />
  <FunctionCode Name="F05.15" Default="0.0" DeftEng="0.0"	Max="F05.13" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定" English="Minimal Given" Show="1" />
  <FunctionCode Name="F05.16" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定对应值" English="Minimum Given Value polyline" Show="1" />
  <FunctionCode Name="F05.17" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="F00.09" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率1" English="jump frequency 1" Show="1" />
  <FunctionCode Name="F05.18" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="F00.09" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率2" English="jump frequency 2" Show="1" />
  <FunctionCode Name="F05.19" Default="0.00" DeftEng="0.00"	Max="F00.08" 	Min="F00.09" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率3" English="jump frequency 3" Show="1" />
  <FunctionCode Name="F05.20" Default="0.00" DeftEng="0.00"	Max="30.00" 	Min="0.00" 		Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="跳跃频率范围" English="jump frequency range" Show="1" />
  <FunctionCode Name="F05.21" Default="5.00" DeftEng="5.00"	Max="F00.08" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定2" English="Jog Operation Frequency Digital Setting 2" Show="1" />
  <FunctionCode Name="F05.22" Default="3:不处理" DeftEng="3: Do not process"	Max="3" 	Min="0" 		Attribute="0x2088" 	AbsoluteValue="0"			Chinese="操作面板电位计曲线选择" English="keypad potentiometer curve selection" Show="1" />
  <FunctionCode Name="F05.23" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F05.24" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.00" Default="5.5" DeftEng="5.5"	Max="500.0" 	Min="0.2" 		Attribute="0x1222" 	AbsoluteValue="0"			Chinese="电机1额定功率" English="motor1 rated power" Show="1" />
  <FunctionCode Name="F08.01" Default="380" DeftEng="380"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="电机1额定电压" English="motor1 rated voltage" Show="1" />
  <FunctionCode Name="F08.02" Default="13.00" DeftEng="13.00" Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="电机1额定电流" English="motor1 rated current" Show="1" />
  <FunctionCode Name="F08.03" Default="50.0" DeftEng="50.0"	Max="400.0" 	Min="1.0" 		Attribute="0x0122" 	AbsoluteValue="0"			Chinese="电机1额定频率" English="motor1 rated power" Show="1" />
  <FunctionCode Name="F08.04" Default="1455" DeftEng="1455"	Max="24000" 	Min="1" 			Attribute="0x0408" 	AbsoluteValue="0"			Chinese="电机1额定转速" English="motor1 rated Rpm" Show="1" />
  <FunctionCode Name="F08.05" Default="0" DeftEng="0"		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.06" Default="0:不动作" DeftEng="0: No action"		Max="3" 			Min="0" 			Attribute="0x0008" 	AbsoluteValue="0"			Chinese="电机1参数自整定" English="motor1 parameter auto-tuning" Show="1" />
  <FunctionCode Name="F08.07" Default="0.70" DeftEng="0.70"	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="电机1定子电阻" English="motor1 stator resistor" Show="1" />
  <FunctionCode Name="F08.08" Default="0.67" DeftEng="0.67"	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="电机1转子电阻" English="motor1 rotator resistor" Show="1" />
  <FunctionCode Name="F08.09" Default="5.0"  DeftEng="5.0"		Max="9999.0" 		Min="0.0" 			Attribute="0x0c12" 	AbsoluteValue="0"			Chinese="电机1漏电感" English="Motor 1 Leakage Inductor" Show="1" />
  <FunctionCode Name="F08.10" Default="124.0" DeftEng="124.0"	Max="9999.0" 		Min="0.0" 			Attribute="0x0c14" 	AbsoluteValue="0"			Chinese="电机1互感抗" English="Motor 1 Inductance" Show="1" />
  <FunctionCode Name="F08.11" Default="5.30"  DeftEng="5.30"	Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="电机1空载励磁电流" English="Motor 1 No Load Excitation Current" Show="1" />
  <FunctionCode Name="F08.12" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机1铁芯饱和系数1" English="Motor 1 Core Saturation Factor1" Show="1" />
  <FunctionCode Name="F08.13" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机1铁芯饱和系数2" English="Motor 1 Core Saturation Factor2" Show="1" />
  <FunctionCode Name="F08.14" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机1铁芯饱和系数3" English="Motor 1 Core Saturation Factor3" Show="1" />
  <FunctionCode Name="F08.15" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机1铁芯饱和系数4" English="Motor 1 Core Saturation Factor4" Show="1" />
  <FunctionCode Name="F08.16" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机1铁芯饱和系数5" English="Motor 1 Core Saturation Factor5" Show="1" />
  <FunctionCode Name="F08.17" Default="0" 	  DeftEng="0"	        Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.18" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F08.19" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F09.00" Default="0:直线" DeftEng="0: Straight"		Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机1 V/f曲线设定" English="Motor 1 V/f Curve Setting" Show="1" />
  <FunctionCode Name="F09.01" Default="0.0" DeftEng="0.0"	Max="100.0" 	Min="F09.03" 	Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f频率值F3" English="Motor 1 V/f Frequency Value F3" Show="1" />
  <FunctionCode Name="F09.02" Default="0.0" DeftEng="0.0"		Max="100.0" 	Min="F09.04" 	Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f电压值V3" English="Motor 1 V/f Voltage V3" Show="1" />
  <FunctionCode Name="F09.03" Default="0.0" DeftEng="0.0"	Max="F09.01" 	Min="F09.05" 	Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f频率值F2" English="Motor 1 V/f Frequency Value F2" Show="1" />
  <FunctionCode Name="F09.04" Default="0.0" DeftEng="0.0"		Max="F09.02" 	Min="F09.06" 	Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f电压值V2" English="Motor 1 V/f Voltage V2" Show="1" />
  <FunctionCode Name="F09.05" Default="0.0" DeftEng="0.0"	Max="F09.03" 	Min="0.0" 		Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f频率值F1" English="Motor 1 V/f Frequency Value F1" Show="1" />
  <FunctionCode Name="F09.06" Default="0.0" DeftEng="0.0"		Max="F09.04" 	Min="0.0" 			Attribute="0x2592" 	AbsoluteValue="0"			Chinese="电机1 V/f电压值V1" English="Motor 1 V/f Voltage V1" Show="1" />
  <FunctionCode Name="F09.07" Default="2.0" DeftEng="2.0"	Max="30.0" 		Min="0.0" 		Attribute="0x259a" 	AbsoluteValue="0"			Chinese="IM1转矩提升" English="IM1 Torque Boost" Show="1" />
  <FunctionCode Name="F09.08" Default="25.0" DeftEng="25.0"	Max="50.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"			Chinese="电机1手动转矩提升截止点" English="Motor 1 Manual Torque Boost Point" Show="1" />
  <FunctionCode Name="F09.09" Default="0.0" DeftEng="0.0"   Max="300.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1转差补偿增益" English="Motor 1 Slip Compensation Gain" Show="1" />
  <FunctionCode Name="F09.10" Default="0.10" DeftEng="0.10"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机1转差补偿滤波时间" English="Motor 1 Slip Compensation Filter Time" Show="1" />
  <FunctionCode Name="F09.11" Default="200.0" DeftEng="200.0" Max="250.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机1转差补偿限定" English="Motor 1 Slip Compensation Limit" Show="1" />
  <FunctionCode Name="F09.12" Default="0.193" DeftEng="0.193"	Max="9.999" 		Min="0.000" 		Attribute="0x32a6" 	AbsoluteValue="0"			Chinese="电机1铁损" English="Motor 1 Core Loss" Show="1" />
  <FunctionCode Name="F09.13" Default="0" 	DeftEng="0"	    Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F09.14" Default="1:一直动作" DeftEng="1: Always Action"		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1 AVR(自动电压调节)功能" English="Motor 1 AVR (Automatic Voltage Regulation) Function" Show="1" />
  <FunctionCode Name="F09.15" Default="50" 	DeftEng="50"	Max="200" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1低频抑制震荡系数" English="Motor 1 Low Frequency Suppression Oscillator" Show="1" />
  <FunctionCode Name="F09.16" Default="20" 	DeftEng="20"	Max="200" 		Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1高频抑制震荡系数" English="Motor 1 High Frequency Suppressed Oscillator" Show="1" />
  <FunctionCode Name="F09.17" Default="0:节能控制无效" DeftEng="0: Energy Saving Control Invalid"	Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机1节能控制选择" English="Motor 1 Energy Saving Control Option" Show="1" />
  <FunctionCode Name="F09.18" Default="5.0"  DeftEng="5.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2552" 	AbsoluteValue="0"			Chinese="电机1节能系数" English="Motor 1 Energy Efficiency" Show="1" />
  <FunctionCode Name="F09.19" Default="25.00" DeftEng="25.00"		Max="50.00" 			Min="0.00" 			Attribute="0x215c" 	AbsoluteValue="0"			Chinese="电机1节能起始频率" English="Motor 1 Energy Saving Start Frequency" Show="1" />
  <FunctionCode Name="F09.20" Default="100.0" DeftEng="100.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2552" 	AbsoluteValue="0"			Chinese="电机1节能切换点" English="Motor 1 Energy Saving Switch Point" Show="1" />
  <FunctionCode Name="F09.21" Default="10" 	DeftEng="10"	Max="5000" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="电机1节能检测次数" English="Motor 1 Energy Saving Test Times" Show="1" />
  <FunctionCode Name="F09.22" Default="100" DeftEng="100"		Max="4000" 			Min="40" 			Attribute="0x2850" 	AbsoluteValue="0"			Chinese="电机1节能电压恢复时间" English="Motor 1 Energy Saving Voltage Recovery Time" Show="1" />
  <FunctionCode Name="F09.23" Default="100" DeftEng="100"		Max="4000" 			Min="40" 			Attribute="0x2850" 	AbsoluteValue="0"			Chinese="电机1节能电压下降时间" English="Motor 1 Energy Saving Voltage Fall Time" Show="1" />
  <FunctionCode Name="F09.24" Default="0" 	DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F13.00" Default="0:无PG的V/f控制" DeftEng="0: V/f control without PG"		Max="2" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2控制方式选择" English="Motor 2 control mode selection" Show="1" />
  <FunctionCode Name="F13.01" Default="5.5"  DeftEng="5.5"	Max="500.0" 	Min="0.2" 		Attribute="0x1222" 	AbsoluteValue="0"			Chinese="电机2额定功率" English="Motor 2 Rated Power" Show="1" />
  <FunctionCode Name="F13.02" Default="380"  DeftEng="380"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="电机2额定电压" English="Motor 2 Rated Voltage" Show="1" />
  <FunctionCode Name="F13.03" Default="13.00" DeftEng="13.00" Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="电机2额定电流" English="Motor 2 Rated Current" Show="1" />
  <FunctionCode Name="F13.04" Default="50.0" DeftEng="50.0"	Max="400.0" 	Min="1.0" 		Attribute="0x0122" 	AbsoluteValue="0"			Chinese="电机2额定频率" English="Motor 2 Rated Frequency" Show="1" />
  <FunctionCode Name="F13.05" Default="1455" DeftEng="1455"	Max="24000" 	Min="1" 			Attribute="0x0408" 	AbsoluteValue="0"			Chinese="电机2额定转速" English="Motor 2 Rated Rpm" Show="1" />
  <FunctionCode Name="F13.06" Default="0"  DeftEng="0"	Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F13.07" Default="0:不动作" DeftEng="0: No action"		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2参数自整定" English="Motor 2 Parameter Auto-tuning" Show="1" />
  <FunctionCode Name="F13.08" Default="0.70"  DeftEng="0.70"	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="电机2定子电阻" English="Motor 2 Stator Resistance" Show="1" />
  <FunctionCode Name="F13.09" Default="0.67"  DeftEng="0.67"	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="电机2转子电阻" English="Motor 2 Rotor Resistance" Show="1" />
  <FunctionCode Name="F13.10" Default="5.0"   DeftEng="5.0"		Max="9999.0" 		Min="0.0" 			Attribute="0x0c12" 	AbsoluteValue="0"			Chinese="电机2漏电感" English="Motor 2 Leakage Inductor" Show="1" />
  <FunctionCode Name="F13.11" Default="124.0" DeftEng="124.0"	Max="9999.0" 		Min="0.0" 			Attribute="0x0c14" 	AbsoluteValue="0"			Chinese="电机2互感" English="Motor2 mutual inductance" Show="1" />
  <FunctionCode Name="F13.12" Default="5.30"  DeftEng="5.30"	Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="电机2空载励磁电流" English="Motor 2 No Load Excitation Current" Show="1" />
  <FunctionCode Name="F13.13" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机2铁芯饱和系数1" English="Motor 2 Core Saturation Factor 1" Show="1" />
  <FunctionCode Name="F13.14" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机2铁芯饱和系数2" English="Motor 2 Core Saturation Factor2" Show="1" />
  <FunctionCode Name="F13.15" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机2铁芯饱和系数3" English="Motor 2 Core Saturation Factor3" Show="1" />
  <FunctionCode Name="F13.16" Default="0:直线" DeftEng="0: Straight"		Max="4" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2 V/f曲线设定" English="Motor 2 V/f Curve Setting" Show="1" />
  <FunctionCode Name="F13.17" Default="0.00"  DeftEng="0.00"	Max="F13.04" 	Min="F13.19" 	Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f频率值F3" English="Motor 2 V/f Frequency Value F3" Show="1" />
  <FunctionCode Name="F13.18" Default="0"  DeftEng="0"		Max="F13.02" 	Min="F13.20" 	Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f电压值V3" English="Motor 2 V/f Voltage V3" Show="1" />
  <FunctionCode Name="F13.19" Default="0.00"  DeftEng="0.00"	Max="F13.17" 	Min="F13.21" 	Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f频率值F2" English="Motor 2 V/f Frequency Value F2" Show="1" />
  <FunctionCode Name="F13.20" Default="0"  DeftEng="0"	Max="F13.18" 	Min="F13.22" 	Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f电压值V2" English="Motor 2 V/f Voltage V2" Show="1" />
  <FunctionCode Name="F13.21" Default="0.00"  DeftEng="0.00"	Max="F13.19" 	Min="0.00" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f频率值F1" English="Motor 2 V/f Frequency Value F1" Show="1" />
  <FunctionCode Name="F13.22" Default="0" 	DeftEng="0"	Max="F13.20" 	Min="0" 			Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2 V/f电压值V1 " English="Motor 2 V/f Voltage V1" Show="1" />
  <FunctionCode Name="F13.23" Default="2.0" DeftEng="2.0"	Max="30.0" 		Min="0.0" 		Attribute="0x251a" 	AbsoluteValue="0"			Chinese="电机2转矩提升" English="Motor 2 Torque Boost" Show="1" />
  <FunctionCode Name="F13.24" Default="25.0" DeftEng="25.0"	Max="50.0" 		Min="0.0" 		Attribute="0x251a" 	AbsoluteValue="0"			Chinese="电机2手动转矩提升截止点" English="Motor 2 Manual Torque Boost Point" Show="1" />
  <FunctionCode Name="F13.25" Default="0.0" DeftEng="0.0" Max="300.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2转差补偿增益" English="Motor 2 Slip Compensation Gain" Show="1" />
  <FunctionCode Name="F13.26" Default="0.10" DeftEng="0.10"	Max="10.00" 	Min="0.01" 		Attribute="0x2624" 	AbsoluteValue="0"			Chinese="电机2转差补偿滤波时间" English="Motor 2 Slip Compensation Filter Time" Show="1" />
  <FunctionCode Name="F13.27" Default="200.0" DeftEng="200.0" Max="250.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2转差补偿限定" English="Motor 2 Slip Compensation Limit" Show="1" />
  <FunctionCode Name="F13.28" Default="0.193" DeftEng="0.193"	Max="9.999" 		Min="0.000" 		Attribute="0x3226" 	AbsoluteValue="0"			Chinese="电机2铁损" English="Motor 2 Core Loss" Show="1" />
  <FunctionCode Name="F13.29" Default="0"   DeftEng="0"	Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F13.30" Default="1:一直动作" DeftEng="1: Always Action"		Max="2" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2 AVR功能" English="Motor 2 AVR Function" Show="1" />
  <FunctionCode Name="F13.31" Default="50"  DeftEng="50"		Max="200" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2低频抑制震荡系数" English="Motor 2 Low Frequency Suppression Oscillator" Show="1" />
  <FunctionCode Name="F13.32" Default="20" 	DeftEng="20"	Max="200" 		Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2高频抑制震荡系数" English="Motor 2 High Frequency Suppression Oscillator" Show="1" />
  <FunctionCode Name="F13.33" Default="0:节能控制无效" DeftEng="0: Energy Saving Control Invalid"		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2节能控制选择" English="Motor 2 Energy Saving Control Option" Show="1" />
  <FunctionCode Name="F13.34" Default="5.0"  DeftEng="5.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2512" 	AbsoluteValue="0"			Chinese="电机2节能系数" English="Motor 2 Energy Saving Coefficient" Show="1" />
  <FunctionCode Name="F13.35" Default="10.0" DeftEng="10.0"	Max="200.0" 	Min="0.1" 		Attribute="0x2022" 	AbsoluteValue="0"			Chinese="电机2速度控制比例增益1" English="Motor 2 Speed Control Proportional Gain 1" Show="1" />
  <FunctionCode Name="F13.36" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x2624" 	AbsoluteValue="0"			Chinese="电机2速度控制积分时间1" English="Motor 2 Speed Control Integration Time 1" Show="1" />
  <FunctionCode Name="F13.37" Default="10.0" DeftEng="10.0"	Max="200.0" 	Min="0.1" 		Attribute="0x2022" 	AbsoluteValue="0"			Chinese="电机2速度控制比例增益2" English="Motor 2 Speed Control Proportional Gain 2" Show="1" />
  <FunctionCode Name="F13.38" Default="0.20" DeftEng="0.20"	Max="10.00" 	Min="0.00" 		Attribute="0x2624" 	AbsoluteValue="0"			Chinese="电机2速度控制积分时间2" English="Motor 2 Speed Control Integration Time 2" Show="1" />
  <FunctionCode Name="F13.39" Default="10.00" DeftEng="10.00" Max="50.00" 	Min="0.00" 		Attribute="0x2124" 	AbsoluteValue="0"			Chinese="电机2速度环PI切换频率1" English="Motor 2 Speed Loop PI Switching Frequency 1" Show="1" />
  <FunctionCode Name="F13.40" Default="15.00" DeftEng="15.00" Max="50.00" 	Min="0.00" 		Attribute="0x2124" 	AbsoluteValue="0"			Chinese="电机2速度环PI切换频率2" English="Motor 2 Speed Loop PI Switching Frequency 2" Show="1" />
  <FunctionCode Name="F13.41" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2速度环积分项限定" English="Motor 2 Speed Loop Integral Item Limit" Show="1" />
  <FunctionCode Name="F13.42" Default="0.00"  DeftEng="0.00"	Max="1.00" 		Min="0.00" 		Attribute="0x261c" 	AbsoluteValue="0"			Chinese="电机2速度环微分时间" English="Motor 2 Speed Loop Differential Time" Show="1" />
  <FunctionCode Name="F13.43" Default="0.000" DeftEng="0.000" Max="1.000" 	Min="0.000" 	Attribute="0x2626" 	AbsoluteValue="0"			Chinese="电机2速度环输出滤波时间" English="Motor 2 Speed Loop Output Filter Time" Show="1" />
  <FunctionCode Name="F13.44" Default="0:不锁定" DeftEng="0: No lock"		Max="1" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2转矩限定锁定选择" English="Motor 2 Torque Limit Lock Select" Show="1" />
  <FunctionCode Name="F13.45" Default="0000"  DeftEng="0000"		Max="7777" 			Min="0000" 			Attribute="0x2020" 	AbsoluteValue="0"			Chinese="电机2转矩限定通道" English="Motor 2 Torque Limiting Channel" Show="1" />
  <FunctionCode Name="F13.46" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2正转时电动转矩限定" English="Electric torque limit at motor 2 forward rotation" Show="1" />
  <FunctionCode Name="F13.47" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2反转时电动转矩限定" English="Electric Torque Limit at Motor 2 Reverse" Show="1" />
  <FunctionCode Name="F13.48" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2正转时再生转矩限定" English="Regeneration torque at motor 2 forward rotation" Show="1" />
  <FunctionCode Name="F13.49" Default="180.0" DeftEng="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2522" 	AbsoluteValue="0"			Chinese="电机2反转时再生转矩限定" English="Regeneration Torque Limit at Motor 2 Reverse" Show="1" />
  <FunctionCode Name="F13.50" Default="400"   DeftEng="400"		Max="2000" 			Min="1" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2电流环KP" English="Motor 2 Current Loop KP" Show="1" />
  <FunctionCode Name="F13.51" Default="200"   DeftEng="200"		Max="1000" 			Min="1" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2电流环KI" English="Motor 2 Current Loop KI" Show="1" />
  <FunctionCode Name="F13.52" Default="3" 	  DeftEng="3"	Max="31" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2电流环输出滤波次数" English="Motor 2 Current Loop Output Filter Times" Show="1" />
  <FunctionCode Name="F13.53" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机2铁芯饱和系数4" English="Motor 2 Core Saturation Factor 4" Show="1" />
  <FunctionCode Name="F13.54" Default="1.00"  DeftEng="1.00"		Max="1.00" 			Min="0.00" 			Attribute="0x201c" 	AbsoluteValue="0"			Chinese="电机2铁芯饱和系数5" English="Motor 2 Core Saturation Factor 5" Show="1" />
  <FunctionCode Name="F13.55" Default="1:使能前馈" 	DeftEng="1: Enable Feed Forward"	Max="1" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2电流环前馈使能" English="Motor 2 Current Loop Feed Forward Enable" Show="1" />
  <FunctionCode Name="F13.56" Default="0.0"   DeftEng="0.0"		Max="30.0" 			Min="0.0" 			Attribute="0x2512" 	AbsoluteValue="0"			Chinese="电机2励磁增强设定" English="Motor 2 Excitation Enhancement Settings" Show="1" />
  <FunctionCode Name="F13.57" Default="00" 	  DeftEng="00"	Max="11" 			Min="00" 			Attribute="0x2010" 	AbsoluteValue="0"			Chinese="电机2磁场定向优化设定" English="Motor 2 Field Orienting Optimization Settings" Show="1" />
  <FunctionCode Name="F13.58" Default="25.00" DeftEng="25.00"		Max="50.00" 			Min="0.00" 			Attribute="0x211c" 	AbsoluteValue="0"			Chinese="电机2节能起始频率" English="Motor 2 Energy Saving Start Frequency" Show="1" />
  <FunctionCode Name="F13.59" Default="100.0" DeftEng="100.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2512" 	AbsoluteValue="0"			Chinese="电机2节能切换点" English="Motor 2 Energy Saving Switch Point" Show="1" />
  <FunctionCode Name="F13.60" Default="10" 	  DeftEng="10"	Max="5000" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="电机2节能检测次数" English="Motor 2 Energy Saving Test Times" Show="1" />
  <FunctionCode Name="F13.61" Default="100"   DeftEng="100"		Max="4000" 			Min="40" 			Attribute="0x2810" 	AbsoluteValue="0"			Chinese="电机2节能电压恢复时间" English="Motor 2 Energy Saving Voltage Recovery Time" Show="1" />
  <FunctionCode Name="F13.62" Default="100"   DeftEng="100"		Max="4000" 			Min="40" 			Attribute="0x2810" 	AbsoluteValue="0"			Chinese="电机2节能电压下降时间" English="Motor 2 Energy Saving Voltage Fall Time" Show="1" />
  <FunctionCode Name="F13.63" Default="0"     DeftEng="0"	Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F15.00" Default="2:正转功能" 	DeftEng="2: Forward Function"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI1端子功能" English="DI1 Terminal Function" Show="1" />
  <FunctionCode Name="F15.01" Default="3:反转功能" 	DeftEng="3: Reverse Function"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI2端子功能" English="DI2 Terminal Function" Show="1" />
  <FunctionCode Name="F15.02" Default="0:保留"  DeftEng="0: Reserved"		Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI3端子功能" English="DI3 Terminal Function" Show="1" />
  <FunctionCode Name="F15.03" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI4端子功能" English="DI4 Terminal Function" Show="1" />
  <FunctionCode Name="F15.04" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI5端子功能" English="DI5 Terminal Function" Show="1" />
  <FunctionCode Name="F15.05" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI6端子功能" English="DI6 Terminal Function" Show="1" />
  <FunctionCode Name="F15.06" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI7端子功能" English="DI7 Terminal Function" Show="1" />
  <FunctionCode Name="F15.07" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI8端子功能" English="DI8 Terminal Function" Show="1" />
  <FunctionCode Name="F15.08" Default="0:保留" 	DeftEng="0: Reserved"	Max="54" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI9端子功能" English="DI9 Terminal Function" Show="1" />
  <FunctionCode Name="F15.09" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI10端子(扩展卡端子)功能" English="DI10 Terminal (Expansion Card Terminal) Function" Show="1" />
  <FunctionCode Name="F15.10" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI11端子(扩展卡端子)功能" English="DI11 Terminal (Expansion Card Terminal) Function" Show="1" />
  <FunctionCode Name="F15.11" Default="0" 	DeftEng="0" 	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="DI12端子(扩展卡端子)功能" English="DI12 Terminal (Expansion Card Terminal) Function" Show="1" />
  <FunctionCode Name="F15.12" Default="1.00" DeftEng="1.00"	Max="99.99" 	Min="0.00" 		Attribute="0x30a4" 	AbsoluteValue="0"			Chinese="端子UP/DN加减速速率" English="Terminal UP/DN Acceleration/Deceleration Rate" Show="1" />
  <FunctionCode Name="F15.13" Default="0: 2ms" 	DeftEng="0: 2ms"	Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="端子检测间隔时间" English="Terminal Detection Interval" Show="1" />
  <FunctionCode Name="F15.14" Default="2" 	DeftEng="2"	 Max="10000" 		Min="0" 			Attribute="0x3758" 	AbsoluteValue="0"			Chinese="端子检测滤波次数" English="Front Detection Filter Times" Show="1" />
  <FunctionCode Name="F15.15" Default="0" 	DeftEng="0"	Max="0x1ff" 	Min="0" 			Attribute="0x2059" 	AbsoluteValue="0"			Chinese="输入端子正反逻辑设定" English="Input Terminal Positive and Negative Logic Settings" Show="1" />
  <FunctionCode Name="F15.16" Default="0:两线式运转模式1" DeftEng="0: Two-line operation mode 1"		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="正转/反转运转模式设定" English="Forward/reverse operation Mode setting" Show="1" />
  <FunctionCode Name="F15.17" Default="0:自由停机" 	DeftEng="0: Free Stop"	Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="端子外部设备故障动作选择" English="Terminal External Device Fault Action Selection" Show="1" />
  <FunctionCode Name="F15.18" Default="2:变频器运行中" DeftEng="2: Drive Running"		Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO1端子功能" English="DO1 Terminal Function" Show="1" />
  <FunctionCode Name="F15.19" Default="0:保留" 	DeftEng="0: Reserved"	Max="38" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO2端子功能" English="DO2 Terminal Function" Show="1" />
  <FunctionCode Name="F15.20" Default="31:变频器故障" DeftEng="31: Drive Fault"		Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="继电器1输出功能" English="Relay 1 Output Function" Show="1" />
  <FunctionCode Name="F15.21" Default="0:保留" 	DeftEng="0: Reserved"	Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="继电器2(扩展继电器)输出功能" English="Relay 2 (Extended Relay) Output Function" Show="1" />
  <FunctionCode Name="F15.22" Default="0:保留" 	DeftEng="0: Reserved"	Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="继电器3(扩展继电器)输出功能" English="Relay 3 (Extended Relay) Output Function" Show="1" />
  <FunctionCode Name="F15.23" Default="0:保留" 	DeftEng="0: Reserved"	Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="继电器4(扩展继电器)输出功能" English="Relay 4 (Extended Relay) Output Function" Show="1" />
  <FunctionCode Name="F15.24" Default="000"     DeftEng="000"	Max="0x3f" 		Min="0" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="输出端子正反逻辑设定" English="Output Terminal Positive and Negative Logic Settings" Show="1" />
  <FunctionCode Name="F15.25" Default="0.00"    DeftEng="0.00"	Max="300.00" 	Min="0.00" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="定时功能ON侧延迟时间" English="Timing Function ON Side Delay Time" Show="1" />
  <FunctionCode Name="F15.26" Default="0.00"    DeftEng="0.00"	Max="300.00" 	Min="0.00" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="定时功能OFF侧延迟时间" English="Timing Function OFF Side Delay Time" Show="1" />
  <FunctionCode Name="F15.27" Default="2.50"    DeftEng="2.50"	Max="100.00" 	Min="0.00" 		Attribute="0x216c" 	AbsoluteValue="0"			Chinese="频率到达(FAR)检出宽度" English="Far Width (FAR) Check Out Width" Show="1" />
  <FunctionCode Name="F15.28" Default="0.00"    DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频信号检出值" English="zero frequency signal detected value" Show="1" />
  <FunctionCode Name="F15.29" Default="0.00"    DeftEng="0.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频回差" English="Zero Frequency Backlash" Show="1" />
  <FunctionCode Name="F15.30" Default="0:按给定频率检出" DeftEng="0: Check out by given frequency"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="FDT1检出方式" English="FDT1 Checkout Method" Show="1" />
  <FunctionCode Name="F15.31" Default="50.00"   DeftEng="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT1电平" English="DT1 Level" Show="1" />
  <FunctionCode Name="F15.32" Default="1.00"    DeftEng="1.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT1滞后" English="FDT1 Lag" Show="1" />
  <FunctionCode Name="F15.33" Default="0:按给定频率检出" DeftEng="0: Check out by given frequency"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="FDT2检出方式" English="FDT2 Checkout Method" Show="1" />
  <FunctionCode Name="F15.34" Default="50.00" DeftEng="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT2电平" English="FDT2 Level" Show="1" />
  <FunctionCode Name="F15.35" Default="1.00" DeftEng="1.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT2滞后" English="FDT2 delay" Show="1" />
  <FunctionCode Name="F15.36" Default="0" DeftEng="0"		Max="65535" 	Min="0" 			Attribute="0x3168" 	AbsoluteValue="0"			Chinese="设定运行时间" English="Set Runtime" Show="1" />
  <FunctionCode Name="F15.37" Default="0" DeftEng="0"		Max="9999" 		Min="F15.38" 	Attribute="0x2060" 	AbsoluteValue="0"			Chinese="设定计数值到达给定" English="Set count value to reach given" Show="1" />
  <FunctionCode Name="F15.38" Default="0" DeftEng="0"		Max="F15.37" 	Min="0" 			Attribute="0x2060" 	AbsoluteValue="0"			Chinese="指定计数值到达给定" English="Specify the count value to reach the given" Show="1" />
  <FunctionCode Name="F15.39" Default="0000"  DeftEng="0000"		Max="1133" 			Min="0000" 			Attribute="0x20a0" 	AbsoluteValue="0"			Chinese="模拟量输入超限选择" English="Analog Input Overrun Select" Show="1" />
  <FunctionCode Name="F15.40" Default="100.0" DeftEng="100.0"		Max="100.0" 			Min="F15.41" 			Attribute="0x2552" 	AbsoluteValue="0"			Chinese="模拟量输入超限上限值" English="analog input over limit upper limit value" Show="1" />
  <FunctionCode Name="F15.41" Default="0.0"   DeftEng="0.0"		Max="F15.40" 			Min="0.0" 			Attribute="0x2552" 	AbsoluteValue="0"			Chinese="模拟量输入超限下限值" English="Analog input over limit the lower limit value" Show="1" />
  <FunctionCode Name="F15.42" Default="5.00"  DeftEng="5.00"		Max="50.00" 			Min="0.00" 			Attribute="0x265c" 	AbsoluteValue="0"			Chinese="模拟量超限检测时间" English="Analog Overrun Detection Time" Show="1" />
  <FunctionCode Name="F15.43" Default="0.0"   DeftEng="0.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2652" 	AbsoluteValue="0"			Chinese="端子输出延时" English="Terminal Output Delay" Show="1" />
  <FunctionCode Name="F15.44" Default="15.00" DeftEng="15.00"		Max="50.00" 			Min="0.00" 			Attribute="0x265c" 	AbsoluteValue="0"			Chinese="起动模拟量超限检测时间" English="Starting Analog Overrun Detection Time" Show="1" />
  <FunctionCode Name="F15.45" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F15.46" Default="0" 	  DeftEng="0"	Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F16.00" Default="0:保留" 	DeftEng="0: Reserved"	Max="19" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="操作面板电位计功能" English="Panel Potentiometer Function " Show="1" />
  <FunctionCode Name="F16.01" Default="2:频率设定" 	DeftEng="2: Frequency Setting"	Max="19" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="AI1端子功能" English="AI1 Terminal Function" Show="1" />
  <FunctionCode Name="F16.02" Default="5:过程PID反馈" DeftEng="5: Process PID Feedback"		Max="19" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="AI2端子功能" English="AI2 Terminal Function" Show="1" />
  <FunctionCode Name="F16.03" Default="0:保留" 	DeftEng="0: Reserved"	Max="19" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="AI3端子功能" English="AI3 Terminal Function" Show="1" />
  <FunctionCode Name="F16.04" Default="0:保留" 	DeftEng="0: Reserved"	Max="19" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="AI4端子功能" English="AI4 Terminal Function" Show="1" />
  <FunctionCode Name="F16.05" Default="0.0"     DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AI1偏置" English="AI1 Offset" Show="1" />
  <FunctionCode Name="F16.06" Default="1.00"    DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x205c" 	AbsoluteValue="0"		Chinese="AI1增益" English="AI1 Gain" Show="1" />
  <FunctionCode Name="F16.07" Default="0.05"    DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="AI1滤波时间" English="AI1 Filter Time" Show="1" />
  <FunctionCode Name="F16.08" Default="0.0"     DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AI2偏置" English="AI2 Offset" Show="1" />
  <FunctionCode Name="F16.09" Default="1.00"    DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x205c" 	AbsoluteValue="0"		Chinese="AI2增益" English="AI2 Gain" Show="1" />
  <FunctionCode Name="F16.10" Default="0.05"    DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="AI2滤波时间" English="AI2 Filter Time" Show="1" />
  <FunctionCode Name="F16.11" Default="0.0"     DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AI3偏置" English="AI3 Offset" Show="1" />
  <FunctionCode Name="F16.12" Default="1.00"    DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x205c" 	AbsoluteValue="0"		Chinese="AI3增益" English="AI3 Gain" Show="1" />
  <FunctionCode Name="F16.13" Default="0.05"    DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="AI3滤波时间" English="AI3 Filter Time" Show="1" />
  <FunctionCode Name="F16.14" Default="0.0"     DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AI4偏置" English="AI4 Offset" Show="1" />
  <FunctionCode Name="F16.15" Default="1.00"    DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x205c" 	AbsoluteValue="0"		Chinese="AI4增益" English="AI4 Gain" Show="1" />
  <FunctionCode Name="F16.16" Default="0.05"    DeftEng="0.05"	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="AI4滤波时间" English="AI4 Filter Time" Show="1" />
  <FunctionCode Name="F16.17" Default="10000"   DeftEng="10000"	Max="50000" 		Min="0" 		Attribute="0x2148" 	AbsoluteValue="0"			Chinese="最大输入脉冲频率" English="Max Input Pulse Frequency" Show="1" />
  <FunctionCode Name="F16.18" Default="0.20" 	DeftEng="0.20"	Max="10.00" 		Min="0.01" 			Attribute="0x265c" 	AbsoluteValue="0"			Chinese="输入脉冲滤波时间" English="Input pulse filter time" Show="1" />
  <FunctionCode Name="F16.19" Default="2:给定频率(0-最大输出频率)" DeftEng="2: Given frequency (0-max output frequency)"		Max="20" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="AO1端子功能" English="AO1 terminal Function" Show="1" />
  <FunctionCode Name="F16.20" Default="0:保留" DeftEng="0: Reserved"		Max="20" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="AO2端子功能" English="AO2 terminal Function" Show="1" />
  <FunctionCode Name="F16.21" Default="0:保留" DeftEng="0: Reserved"		Max="20" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="高速脉冲输出功能" English="High-Speed Pulse Output Function" Show="1" />
  <FunctionCode Name="F16.22" Default="0.0"    DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AO1偏置" English="AO1 Offset" Show="1" />
  <FunctionCode Name="F16.23" Default="100.0"  DeftEng="100.0"  Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="AO1增益" English="AO2 Gain" Show="1" />
  <FunctionCode Name="F16.24" Default="0.0"    DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="AO2偏置" English="AO2 Offset" Show="1" />
  <FunctionCode Name="F16.25" Default="100.0"  DeftEng="100.0"  Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="AO2增益" English="AO2 Gain" Show="1" />
  <FunctionCode Name="F16.26" Default="10.0"   DeftEng="10.0"	Max="50.0" 		Min="0.1" 		Attribute="0x295a" 	AbsoluteValue="0"			Chinese="DO2最大输出脉冲频率" English="DO2 Maximum Output Pulse Frequency" Show="1" />
  <FunctionCode Name="F16.27" Default="0.0"    DeftEng="0.0"	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="操作面板电位计偏置" English="Panel Potentiometer Offset" Show="1" />
  <FunctionCode Name="F16.28" Default="1.00"   DeftEng="1.00"	Max="10.00" 	Min="0.00" 	Attribute="0x205c" 	AbsoluteValue="0"	Chinese="操作面板电位计增益" English="Panel Potentiometer Gain" Show="1" />
  <FunctionCode Name="F16.29" Default="0"      DeftEng="0"	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"	Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F17.00" Default="0:1-8-2格式,无校验,RTU" 	DeftEng="0:1-8-2 format, no verification, RTU"	Max="6" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="数据格式" English="Data Format" Show="1" />
  <FunctionCode Name="F17.01" Default="3:9600bps" 	DeftEng="3:9600bps" 	Max="8" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="波特率选择" English="Baud Rate Selection" Show="1" />
  <FunctionCode Name="F17.02" Default="2"  DeftEng="2"		Max="247" 		Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="本机地址" English="Local Address" Show="1" />
  <FunctionCode Name="F17.03" Default="1"  DeftEng="1"		Max="1000" 		Min="0" 			Attribute="0x2808" 	AbsoluteValue="0"			Chinese="本机应答时间" English="Local Answer Time" Show="1" />
  <FunctionCode Name="F17.04" Default="0.0" DeftEng="0.0"	Max="600.0" 	Min="0.0" 		Attribute="0x2612" 	AbsoluteValue="0"			Chinese="单机通讯超时检出时间" English="Single Communication Timeout Detection Time" Show="1" />
  <FunctionCode Name="F17.05" Default="0.0" DeftEng="0.0"	Max="600.0" 	Min="0.0" 		Attribute="0x2612" 	AbsoluteValue="0"			Chinese="通讯错误检出时间" English="Time of Communication Error Detection" Show="1" />
  <FunctionCode Name="F17.06" Default="3:继续运行"  DeftEng="3: Continue to run"		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯超时动作选择" English="Communication overtime action selection" Show="1" />
  <FunctionCode Name="F17.07" Default="3:继续运行" 	DeftEng="3: Continue to run"	Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯错误时动作选择" English="Activity at communication error" Show="1" />
  <FunctionCode Name="F17.08" Default="1:紧急停机" 	DeftEng="1: Emergency Stop"	Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯外部设备故障动作选择" English="Communication External Device Fault Action Selection" Show="1" />
  <FunctionCode Name="F17.09" Default="01" 	DeftEng="01"	Max="11" 			Min="00" 			Attribute="0x2010" 	AbsoluteValue="0"			Chinese="通讯写功能参数存EEPROM方式选择" English="Communication Write Function Parameters Store EEPROM Mode Select" Show="1" />
  <FunctionCode Name="F17.10" Default="0.0" DeftEng="0.0"		Max="600.0" 			Min="0.0" 			Attribute="0x262a" 	AbsoluteValue="0"			Chinese="组网通讯超时检出时间" English="Network Communication Timeout Check Out" Show="1" />
  <FunctionCode Name="F17.11" Default="0" 	DeftEng="0"	 Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F17.12" Default="0" 	DeftEng="0"	 Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.00" Default="0:汉语" 	DeftEng="0: Chinese"	Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="语言选择" English="Language Choice" Show="1" />
  <FunctionCode Name="F18.01" Default="5" 	DeftEng="5"	 Max="10" 			Min="1" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="操作面板LCD显示对比度" English="Control Panel LCD Display Contrast" Show="1" />
  <FunctionCode Name="F18.02" Default="8:给定频率（加减速后）" DeftEng="8: Given frequency (after acceleration/deceleration)"		Max="49" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数1设置" English="un display parameter 1 Set " Show="1" />
  <FunctionCode Name="F18.03" Default="7:设定频率" 	DeftEng="7: Setting Frequency"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数2设置" English="un display parameter 2Set " Show="1" />
  <FunctionCode Name="F18.04" Default="36:实际供水压力" 	DeftEng="36: Actual water supply pressure"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数3设置" English="un display parameter 3 Set " Show="1" />
  <FunctionCode Name="F18.05" Default="13:输出电压" DeftEng="13: Output Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数4设置" English="un display parameter 4 Set " Show="1" />
  <FunctionCode Name="F18.06" Default="14:输出电流" DeftEng="14: Output Current"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数5设置" English="un display parameter 5 Set " Show="1" />
  <FunctionCode Name="F18.07" Default="18:直流母线电压" DeftEng="18: DC Bus Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数6设置" English="un display parameter 6 Set " Show="1" />
  <FunctionCode Name="F18.08" Default="7:设定频率" 	DeftEng="7: Setting Frequency"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数1设置" English="" Show="1" />
  <FunctionCode Name="F18.09" Default="18:直流母线电压" DeftEng="18: DC Bus Voltage"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数2设置" English="Shutdown Display Parameter 2 Setting" Show="1" />
  <FunctionCode Name="F18.10" Default="20:AI1输入电压" 	DeftEng="20:AI1 input voltage"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数3设置" English="Shutdown Display Parameter 3 Setting" Show="1" />
  <FunctionCode Name="F18.11" Default="22:AI2输入电压" 	DeftEng="22:AI2 input voltage"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数4设置" English="Shutdown Display Parameter 4 Setting" Show="1" />
  <FunctionCode Name="F18.12" Default="35:设定供水压力" DeftEng="35: Set water supply pressure"		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数5设置" English="Shutdown Display Parameter 5 Setting" Show="1" />
  <FunctionCode Name="F18.13" Default="36:实际供水压力" DeftEng="36: Actual water supply pressure"	Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数6设置" English="Shutdown Display Parameter 6 Setting" Show="1" />
  <FunctionCode Name="F18.14" Default="1.0"  DeftEng="1.0"		Max="160.0"			Min="0.1" 			Attribute="0x2062" 	AbsoluteValue="0"			Chinese="频率显示增益" English="Frequency Display Gain" Show="1" />
  <FunctionCode Name="F18.15" Default="1000" DeftEng="1000"		Max="65535"			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="最大线速度" English="Maximum Line Speed" Show="1" />
  <FunctionCode Name="F18.16" Default="0:整数" DeftEng="0: Integer"		Max="3"			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="线速度显示精度" English="Line Speed Display Accuracy" Show="1" />
  <FunctionCode Name="F18.17" Default="0" 	 DeftEng="0"	 Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.18" Default="0" 	 DeftEng="0"	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F18.19" Default="0" 	 DeftEng="0"	Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.00" Default="0:无辅助频率通道" DeftEng="0: No auxiliary channel"		Max="11" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="辅助频率设定通道选择" English="Auxiliary Frequency Setting Channel Selection" Show="1" />
  <FunctionCode Name="F19.01" Default="10" 	DeftEng="10"	Max="41" 			Min="00" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="主辅设定运算" English="Main and Secondary Settings Calculation" Show="1" />
  <FunctionCode Name="F19.02" Default="1.00" DeftEng="1.00"	Max="9.99" 		Min="0.00" 		Attribute="0x205c" 	AbsoluteValue="0"			Chinese="辅助设定系数" English="auxiliary line set number" Show="1" />
  <FunctionCode Name="F19.03" Default="0.00" DeftEng="0.00"	Max="F00.06" 	Min="0.00" 			Attribute="0x616c" 	AbsoluteValue="0"			Chinese="数字辅助频率初值" English="Initial Digital Assistant Frequency" Show="1" />
  <FunctionCode Name="F19.04" Default="00" 	DeftEng="00"	Max="0x11" 		Min="00" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="数字辅助频率控制选择" English="Digital Assistant Frequency Control Selection" Show="1" />
  <FunctionCode Name="F19.05" Default="1:相对最大输出频率调整" DeftEng="1: Relative maximum output frequency adjustment"		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="设定频率比例调整选择" English="Set the frequency scaling factor" Show="1" />
  <FunctionCode Name="F19.06" Default="100.0" DeftEng="100.0"  Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="设定频率比例调整系数" English="Set frequency scaling selection" Show="1" />
  <FunctionCode Name="F19.07" Default="0:自动停止方式" DeftEng="0: Automatic Stop Method"		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="冷却风扇控制选择" English="Cooling Fan Control Selection" Show="1" />
  <FunctionCode Name="F19.08" Default="60.0"  DeftEng="60.0"	Max="600.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="冷却风扇控制延迟时间" English="Cooling Fan Control Delay Time" Show="1" />
  <FunctionCode Name="F19.09" Default="0"  DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F19.10" Default="1.00"  DeftEng="1.00"	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频阈值" English="Zero Frequency Threshold" Show="1" />
  <FunctionCode Name="F19.11" Default="0:按照频率指令运行" DeftEng="0: Run according to frequency command"		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="设定频率低于零频阈值时动作选择" English="Set frequency below zero frequency threshold Action selection" Show="1" />
  <FunctionCode Name="F19.12" Default="0:禁止瞬停不停" DeftEng="0: Prohibit Non-stop Stopping"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="瞬时失电不停机功能选择" English="nstantaneous power failure non-stop function selection" Show="1" />
  <FunctionCode Name="F19.13" Default="500"  DeftEng="500"	Max="1000" 	Min="10" 		Attribute="0x2050" 	AbsoluteValue="0"			Chinese="瞬停不停电压补偿增益" English="Transient Stop Voltage Compensation Gain" Show="1" />
  <FunctionCode Name="F19.14" Default="0"  DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F19.15" Default="430"  DeftEng="430"	Max="999" 		Min="0" 			Attribute="0x2398" 	AbsoluteValue="0"			Chinese="瞬时失电不停机动作判断电压" English=" instantaneous motor power loss kept for determination voltage" Show="1" />
  <FunctionCode Name="F19.16" Default="0:禁止欠压再起动" DeftEng="0: Prohibition of undervoltage restart"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="欠压再起动功能选择" English="Undervoltage restart function selection" Show="1" />
  <FunctionCode Name="F19.17" Default="2.00"  DeftEng="2.00"	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="欠压再起动等待时间" English="Undervoltage Restart Waiting Time" Show="1" />
  <FunctionCode Name="F19.18" Default="0.500" 	DeftEng="0.500"	 Max="1.000" 			Min="0.000" 			Attribute="0x2066" 	AbsoluteValue="0"			Chinese="过压抑制增益" English="Overpressure suppression gain" Show="1" />
  <FunctionCode Name="F19.19" Default="690"  DeftEng="690"	Max="999" 		Min="0" 			Attribute="0x2398" 	AbsoluteValue="0"			Chinese="过压失速点" English="ressure Stall Point" Show="1" />
  <FunctionCode Name="F19.20" Default="0.500" 	DeftEng="0.500" 	Max="1.000" 			Min="0.000" 			Attribute="0x2066" 	AbsoluteValue="0"			Chinese="自动限流增益" English="Automatic Current Limit Gain" Show="1" />
  <FunctionCode Name="F19.21" Default="150.0"  DeftEng="150.0"  Max="200.0" 	Min="20.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="自动限流水平" English="Automatic Current Limiting Level" Show="1" />
  <FunctionCode Name="F19.22" Default="0" DeftEng="0"  Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="F19.23" Default="0" DeftEng="0"		Max="11" 			Min="00" 			Attribute="0x2089" 	AbsoluteValue="0"			Chinese="端子运行命令有效方式" English="Effective way to run the terminal" Show="1" />
  <FunctionCode Name="F19.24" Default="680"  DeftEng="680"	Max="750" 		Min="330" 		Attribute="0x0398" 	AbsoluteValue="0"			Chinese="制动单元动作电压" English="Braking Unit Operating Voltage" Show="1" />
  <FunctionCode Name="F19.25" Default="0:禁止" DeftEng="0: Forbidden"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="磁通制动使能" English="Flux brake enable" Show="1" />
  <FunctionCode Name="F19.26" Default="0" 	DeftEng="0" 	Max="65535" 	Min="0" 			Attribute="0x2da8" 	AbsoluteValue="0"			Chinese="设定长度" English="Set Length" Show="1" />
  <FunctionCode Name="F19.27" Default="0" 	DeftEng="0" 	Max="65535" 	Min="0" 			Attribute="0x2d08" 	AbsoluteValue="0"			Chinese="实际长度" English="Actual Length" Show="1" />
  <FunctionCode Name="F19.28" Default="1.000" DeftEng="1.000"  Max="30.000" 	Min="0.001" 	Attribute="0x20ae" 	AbsoluteValue="0"			Chinese="长度倍率" English="Length Multiplication" Show="1" />
  <FunctionCode Name="F19.29" Default="1.000" DeftEng="1.000"  Max="1.000" 	Min="0.001" 	Attribute="0x20a6" 	AbsoluteValue="0"			Chinese="长度校正系数" English="Length Correction Factor" Show="1" />
  <FunctionCode Name="F19.30" Default="10.00" DeftEng="10.00"  Max="100.00" 	Min="1.00" 		Attribute="0x2eac" 	AbsoluteValue="0"			Chinese="测量轴直径" English="Axis Diameter Measurement" Show="1" />
  <FunctionCode Name="F19.31" Default="1" 	DeftEng="1" 	Max="9999" 		Min="1" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="轴每转脉冲" English="Axis Per Revolution" Show="1" />
  <FunctionCode Name="F19.32" Default="0:输出电平信号" DeftEng="0: Output Level Signal"		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度到达输出功能选择" English="Length Arrival Output Function Selection" Show="1" />
  <FunctionCode Name="F19.33" Default="0:自动清零" 	DeftEng="0: Automatically Cleared"	Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度到达后记录长度处理" English="Log Length Processing at Stop" Show="1" />
  <FunctionCode Name="F19.34" Default="0:自动清零" 	DeftEng="0: Automatically Cleared"	Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="停机时记录长度处理" English="Aux PID Output Limit" Show="1" />
  <FunctionCode Name="F19.35" Default="100.0"  DeftEng="100.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2592" 	AbsoluteValue="0"			Chinese="辅助PID输出限定" English="Auxiliary PID Output Limited Lift" Show="1" />
  <FunctionCode Name="F19.36" Default="0.0"    DeftEng="0.0"		Max="100.0" 			Min="0.0" 			Attribute="0x2592" 	AbsoluteValue="0"			Chinese="辅助PID输出限定提升量" English="" Show="1" />
  <FunctionCode Name="F19.37" Default="100"    DeftEng="100"		Max="111" 			Min="000" 			Attribute="0x2059" 	AbsoluteValue="0"			Chinese="频率调节范围选择" English="Frequency Adjustment Range Select" Show="1" />
  <FunctionCode Name="F19.38" Default="1:检测" 	DeftEng="1: Detect"	Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="相间短路检测动作选择" English="Interphase Short Detection Action Selection" Show="1" />
  <FunctionCode Name="F19.39" Default="0:380-460V" 	DeftEng="0:380-460V"	Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="输入电压选择" English="Input Voltage Selection" Show="1" />
  <FunctionCode Name="F19.40" Default="1000" 	DeftEng="1000" 	Max="4000" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="磁通制动PI调节器Kp" English="Fuse Braking PI Regulator Kp" Show="1" />
  <FunctionCode Name="F19.41" Default="20" 	DeftEng="20"	Max="500" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="磁通制动PI调节器Ki" English="Fused Brake PI Regulator Ki" Show="1" />
  <FunctionCode Name="F19.42" Default="0"   DeftEng="0"	    Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F19.43" Default="0"   DeftEng="0"	    Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="制动次数" English="Number of brakes" Show="0" />
  <FunctionCode Name="F19.44" Default="0"   DeftEng="0"	    Max="0" 	Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="制动判断电压" English="Brake judgment voltage" Show="0" />
  <FunctionCode Name="F20.00" Default="00000" DeftEng="00000"   Max="31111" 	Min="00000" 			Attribute="0x20a8" 	AbsoluteValue="0"			Chinese="过载预报警检出选择" English="Overload pre-alarm checkout selection" Show="1" />
  <FunctionCode Name="F20.01" Default="150.0" DeftEng="150.0"   Max="200.0" 	Min="20.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="过载预报警检出水平" English="Overload Pre-Alert Detection Level" Show="1" />
  <FunctionCode Name="F20.02" Default="5.0"   DeftEng="5.0"	    Max="60.0" 		Min="0.0" 		Attribute="0x269a" 	AbsoluteValue="0"			Chinese="过载预报警检出时间" English="Overload Pre-Alarm Detection Time" Show="1" />
  <FunctionCode Name="F20.03" Default="0:输出掉载检出无效" DeftEng="0: Output Offload Checkout Invalid"		Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出动作选择" English="nverter Output Offload Inspection the operation of selecting " Show="1" />
  <FunctionCode Name="F20.04" Default="30" 	DeftEng="30"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出水平" English="Inverter Output Off Load Detection Level" Show="1" />
  <FunctionCode Name="F20.05" Default="1.00" DeftEng="1.00"	Max="20.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出时间" English="Inverter Output Outage Detection Time" Show="1" />
  <FunctionCode Name="F20.06" Default="0:不检测电机过热" 	DeftEng="0: Do not detect motor overheating"	Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机过热信号输入类型" English="Motor overheat signal input type" Show="1" />
  <FunctionCode Name="F20.07" Default="5.0"  DeftEng="5.0"	Max="10.0" 		Min="0.0" 		Attribute="0x2f9a" 	AbsoluteValue="0"			Chinese="电机过热热敏电阻值" English="Motor Overheat Thermistor Value" Show="1" />
  <FunctionCode Name="F20.08" Default="30" 	 DeftEng="30"	Max="80" 			Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="输入缺相检测基准" English="Input Phase Loss Detection Standard" Show="1" />
  <FunctionCode Name="F20.09" Default="1.00" DeftEng="1.00"	Max="5.00" 		Min="1.00" 		Attribute="0x269c" 	AbsoluteValue="0"			Chinese="输入缺相检测时间" English="nput Defect Detection Time" Show="1" />
  <FunctionCode Name="F20.10" Default="20" 	 DeftEng="20"	Max="100" 			Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="输出缺相检测基准" English="Output Phase Loss Detection Standard" Show="1" />
  <FunctionCode Name="F20.11" Default="3.00" DeftEng="3.00"	Max="20.00" 	Min="1.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="输出缺相检测时间" English="Output Phase Detection Time" Show="1" />
  <FunctionCode Name="F20.12" Default="0" 	 DeftEng="0"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="PID给定丢失检出值" English="PID Given Loss Detection" Show="1" />
  <FunctionCode Name="F20.13" Default="0.20" DeftEng="0.20"	Max="1000.0" 	Min="0.00" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="PID给定丢失检出时间" English="PID Given Lost Checkout Time" Show="1" />
  <FunctionCode Name="F20.14" Default="0" 	 DeftEng="0"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出值" English="PID Feedback Loss Detection" Show="1" />
  <FunctionCode Name="F20.15" Default="0.20" DeftEng="0.20"	Max="1000.0" 	Min="0.00" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出时间" English="PID feedback lost detection time" Show="1" />
  <FunctionCode Name="F20.16" Default="100"  DeftEng="100"	Max="100" 		Min="0" 			Attribute="0x2588" 	AbsoluteValue="0"			Chinese="PID反馈超限检出值" English="PID feedback limit detection value" Show="1" />
  <FunctionCode Name="F20.17" Default="0.20" DeftEng="0.20"	Max="1000.0" 	Min="0.00" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="PID反馈超限检出时间" English="PID feedback limit detection time" Show="1" />
  <FunctionCode Name="F20.18" Default="0" 	 DeftEng="0"	Max="100" 		Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="自动复位次数" English="Auto Reset" Show="1" />
  <FunctionCode Name="F20.19" Default="5.00" DeftEng="5.00"	Max="200.00" 		Min="0.01" 		Attribute="0x345c" 	AbsoluteValue="0"			Chinese="自动复位间隔时间" English="Automatic Reset Interval" Show="1" />
  <FunctionCode Name="F20.20" Default="00" 	 DeftEng="00"	Max="0x11" 		Min="00" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="故障继电器动作选择" English="Fault Relay Action Selection" Show="1" />
  <FunctionCode Name="F20.21" Default="0" 	 DeftEng="0"	Max="37" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第五次（最近一次）故障类型" English="The fifth (last) fault type" Show="1" />
  <FunctionCode Name="F20.22" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时设定频率" English="Set Frequency at Last Fault" Show="1" />
  <FunctionCode Name="F20.23" Default="0.00" DeftEng="0.00"	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时输出频率" English="Output Frequency at Last Fault" Show="1" />
  <FunctionCode Name="F20.24" Default="0" 	 DeftEng="0"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时直流母线电压" English="DC Bus Voltage at Last Fault" Show="1" />
  <FunctionCode Name="F20.25" Default="0" 	 DeftEng="0"	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电压" English="Output Voltage at Last Fault" Show="1" />
  <FunctionCode Name="F20.26" Default="0.00" DeftEng="0.00"	Max="99.99" 	Min="0.00" 		Attribute="0x0222" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电流" English="Output current at Last Fault" Show="1" />
  <FunctionCode Name="F20.27" Default="0" 	 DeftEng="0"	Max="0x1ff" 	Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输入端子状态" English="intput Terminal Status at Last Fault" Show="1" />
  <FunctionCode Name="F20.28" Default="0" 	 DeftEng="0"	Max="0x3f" 		Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输出端子状态" English="Output Terminal Status at Last Fault" Show="1" />
  <FunctionCode Name="F20.29" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="最近一次故障间隔时间" English="Last Interval Time" Show="1" />
  <FunctionCode Name="F20.30" Default="0" 	 DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第四次故障类型" English="the Fourth Fault Type" Show="1" />
  <FunctionCode Name="F20.31" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第四次故障间隔时间" English="The fourth time between failures" Show="1" />
  <FunctionCode Name="F20.32" Default="0" 	 DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第三次故障类型" English="3rd Failure Type" Show="1" />
  <FunctionCode Name="F20.33" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第三次故障间隔时间" English="the interval time at the 3rd failures" Show="1" />
  <FunctionCode Name="F20.34" Default="0" 	 DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第二次故障类型" English="the second fault type" Show="1" />
  <FunctionCode Name="F20.35" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第二次故障间隔时间" English="the interval time of the 2nd fault" Show="1" />
  <FunctionCode Name="F20.36" Default="0" 	 DeftEng="0"	Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第一次故障类型" English="the 1st fault type" Show="1" />
  <FunctionCode Name="F20.37" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第一次故障间隔时间" English="the interval time of the 1st fault" Show="1" />
  <FunctionCode Name="F20.38" Default="0.0"  DeftEng="0.0"	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="上次故障间隔时间" English="Last fault Interval Time" Show="1" />
  <FunctionCode Name="F20.39" Default="0"    DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="F20.40" Default="0"    DeftEng="0"	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" /> 
  <FunctionCode Name="F23.00" Default="8"  DeftEng="8"		Max="8" 			Min="1" 			Attribute="0x0988" 	AbsoluteValue="0"			Chinese="载波频率设定" English="carrier frequency setting" Show="1" />
  <FunctionCode Name="F23.01" Default="1:载波频率自动调整1" DeftEng="1: Carrier frequency auto-adjust 1"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="载波频率自动调整" English="Carrier frequency auto-adjust" Show="1" />
  <FunctionCode Name="F23.02" Default="1:过调制使能有效" DeftEng="1: Overmodulation enabled"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PWM过调制使能" English="PWM Overmodulation Enable" Show="1" />
  <FunctionCode Name="F23.03" Default="0:两相调制/三相调制切换" DeftEng="0: Two-phase modulation/three-phase modulation switching"		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PWM调制模式" English="PWM modulation mode" Show="1" />
  <FunctionCode Name="F23.04" Default="5.00" DeftEng="5.00"	Max="F23.05-2" 	Min="10.00" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="PWM调制模式切换点1" English="PWM modulation mode switching point 1" Show="1" />
  <FunctionCode Name="F23.05" Default="10.00" DeftEng="10.00"	Max="50.00" 	Min="F23.04+2" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="PWM调制模式切换点2" English="PWM modulation mode switching point 2" Show="1" />
  <FunctionCode Name="F23.06" Default="0"  DeftEng="0"	Max="65535" 	Min="0" 		Attribute="0x00a8" 	AbsoluteValue="0"			Chinese="FO保护功能" English="FO Protection Function" Show="0" />
  <FunctionCode Name="F23.07" Default="0"  DeftEng="0"	Max="65535" 	Min="0" 		Attribute="0x00a8" 	AbsoluteValue="0"			Chinese="硬件故障屏蔽密码保护" English="Hardware Fault Masking Password Protection" Show="0" />
  <FunctionCode Name="F23.08" Default="0"  DeftEng="0"	Max="0xffff" 	Min="0" 		Attribute="0x00a1" 	AbsoluteValue="0"			Chinese="硬件故障屏蔽" English="Hardware Fault Shield" Show="0" />
  <FunctionCode Name="F23.09" Default="2"  DeftEng="2"	Max="2000" 	Min="0" 	Attribute="0x20A0" 	AbsoluteValue="0"			Chinese="随机载频系数K1" English="Random Carrier Frequency K1" Show="1" />
  <FunctionCode Name="F23.10" Default="3"  DeftEng="3"	Max="2000" 	Min="0" 	Attribute="0x20A0" 	AbsoluteValue="0"			Chinese="随机载频系数K2" English="Random Carrier Frequency K2" Show="1" />  
  <FunctionCode Name="P00.00" Default="1:供水调试模式" DeftEng="1:Water supply debugging mode"  Max="1" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="供水模式选择" 	English="Water supply mode selection" Show="1" /> 
  <FunctionCode Name="P00.01" Default="0:无输入"  		DeftEng="0:No input"					Max="2" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="水位信号输入选择" English="Water level signal input selection" Show="1" /> 
  <FunctionCode Name="P00.02" Default="50.0" 		DeftEng="50.0"  	Max="100.0" 		Min="0.0" 	Attribute="0x2552" 	AbsoluteValue="0"			Chinese="进水池上限水位" 	English="Upper pool water level" Show="1" />
  <FunctionCode Name="P00.03" Default="30.0"  		DeftEng="30.0"		Max="P00.02" 		Min="0.0" 	Attribute="0x2552" 	AbsoluteValue="0"			Chinese="进水池下限水位" 	English="Lower limit water level" Show="1" />
  <FunctionCode Name="P00.04" Default="10.0" 		DeftEng="10.0"  	Max="P00.03" 		Min="0.0" 	Attribute="0x2552" 	AbsoluteValue="0"			Chinese="进水池缺水水位" 	English="Water shortage in the pool" Show="1" />  
  <FunctionCode Name="P00.05" Default="0.0"  		DeftEng="0.0"		Max="P05.03×10" 	Min="0.0" 	Attribute="0x3952" 	AbsoluteValue="0"			Chinese="备用压力" 			English="Standby pressure" Show="1" />    
  <FunctionCode Name="P00.06" Default="0" 		DeftEng="0"  	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.07" Default="5.0"  		DeftEng="5.0"		Max="3600.0" 	Min="0.0" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="加泵检测时间" 	English="Adding pump detection time " Show="1" />  
  <FunctionCode Name="P00.08" Default="0" 		DeftEng="0"  	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 			English="reserved" Show="1" /> 
  <FunctionCode Name="P00.09" Default="10.0"  		DeftEng="10.0"		Max="100.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="加泵时主泵减速时间" 	English="Main pump dec. time when removing pumps" Show="1" /> 
  <FunctionCode Name="P00.10" Default="0" 		DeftEng="0"  	Max="0" 		Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 		English="reserved" Show="1" />
  <FunctionCode Name="P00.11" Default="5.0"  		DeftEng="5.0"		Max="3600.0" 	Min="0.0" 		Attribute="0x266a" 	AbsoluteValue="0"			Chinese="减泵检测时间" 		English="Removing pump detection time" Show="1" />
  <FunctionCode Name="P00.12" Default="10.0" 		DeftEng="10.0"  	Max="100.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="减泵时主泵加速时间" English="Main pump dec. time when adding pumps" Show="1" />  
  <FunctionCode Name="P00.13" Default="0.020"  		DeftEng="0.020"		Max="5.000" 	Min="0.000" 	Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 1 接触器断开延时" 	English="Pump 1 contactor disconnection delay" Show="1" />
  <FunctionCode Name="P00.14" Default="0.020" 		DeftEng="0.020"  	Max="5.000" 	Min="0.000" 	Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 1 接触器吸合延时" 	English="Pump 1 contactor pull-in delay" Show="1" />  
  <FunctionCode Name="P00.15" Default="1"  		DeftEng="1"			Max="5" 		Min="1" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="主泵默认泵号" 		English="Main pump default pump number" Show="1" />
  <FunctionCode Name="P00.16" Default="0"  		DeftEng="0"      	Max="40000" 		Min="0" 	        Attribute="0x316a" 	AbsoluteValue="0"			Chinese="主泵轮换周期" 		English="Main pump rotation period" Show="1" />
  <FunctionCode Name="P00.17" Default="0:禁止休眠"  		DeftEng="0:Stop sleeping"			Max="4" 		Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="休眠使能" 			English="Sleep enable" Show="1" />  
  <FunctionCode Name="P00.18" Default="10.0" 	DeftEng="10.0"  	Max="100.0" 	Min="0.0" 			Attribute="0x2562" 	AbsoluteValue="0"			Chinese="休眠唤醒压力容差" English="Pressure tolerance of dormancy awakening" Show="1" />  
  <FunctionCode Name="P00.19" Default="5.0"  	DeftEng="5.0"		Max="3600.0" 	Min="0.0" 			Attribute="0x266a" 	AbsoluteValue="0"			Chinese="休眠唤醒延迟时间" English="Delay time of dormancy awakening" Show="1" />  
  <FunctionCode Name="P00.20" Default="0"  	DeftEng="0"      	Max="0" 	Min="0" 	        Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 		English="reserved" Show="1" />
  <FunctionCode Name="P00.21" Default="0"  	DeftEng="0"		Max="0" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="P00.22" Default="6.0" 	DeftEng="6.0"  		Max="3600.0" 	Min="0.0" 			Attribute="0x2652" 	AbsoluteValue="0"			Chinese="休眠检测时间" 		English="Sleep detection time" Show="1" />
  <FunctionCode Name="P00.23" Default="25.00"  	DeftEng="25.00"		Max="50.00" 	Min="0.00" 			Attribute="0x215c" 	AbsoluteValue="0"			Chinese="无流量检测频率" 		English="No flow detection frequency" Show="1" />
  <FunctionCode Name="P00.24" Default="60.0" 	DeftEng="60.0"  	Max="3600.0" 	Min="0.0" 			Attribute="0x2652" 	AbsoluteValue="0"			Chinese="无流量检测启动延迟检测时间" 	English="No flow detection start delay detection time" Show="1" />
  <FunctionCode Name="P00.25" Default="100"  	DeftEng="100"		Max="400" 		Min="1" 			Attribute="0x2548" 	AbsoluteValue="0"			Chinese="无流量校正因数" 				English="No flow correction factor" Show="1" />
  <FunctionCode Name="P00.26" Default="0.00" 	DeftEng="0.00"  	Max="99.99" 	Min="0.00" 			Attribute="0x215c" 	AbsoluteValue="0"			Chinese="无流量低速" 					English="No flow and low speed" Show="1" />
  <FunctionCode Name="P00.27" Default="0.00"  	DeftEng="0.00"		Max="10.00" 	Min="0.00" 			Attribute="0x329c" 	AbsoluteValue="0"			Chinese="无流量低速功率" 				English="No flow low speed power" Show="1" />
  <FunctionCode Name="P00.28" Default="0.00" 	DeftEng="0.00"  	Max="99.99" 	Min="0.00" 			Attribute="0x215c" 	AbsoluteValue="0"			Chinese="无流量高速" 					English="No flow rate" Show="1" />  
  <FunctionCode Name="P00.29" Default="0.00"  	DeftEng="0.00"		Max="10.00" 	Min="0.00" 			Attribute="0x329c" 	AbsoluteValue="0"			Chinese="无流量高速功率" 				English="No flow high speed power" Show="1" />
  <FunctionCode Name="P00.30" Default="0:平方曲线" 		DeftEng="0:Square curve"  	Max="3" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="无流量检测曲线" 			English="No flow detection curve" Show="1" />
  <FunctionCode Name="P00.31" Default="0"  		DeftEng="0"			Max="1" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="变频器切工频检测使能" 	English="Inverter cut power frequency detection enable" Show="1" />  
  <FunctionCode Name="P00.32" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.33" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.34" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.35" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.36" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.37" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.38" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />   
  <FunctionCode Name="P00.39" Default="0.020"  DeftEng="0.020"	Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 2 接触器断开延时" English="Pump 2 contactor disconnection delay" Show="1" />
  <FunctionCode Name="P00.40" Default="0.020"  DeftEng="0.020"  Max="5.000" 	Min="0.000" 	    Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 2 接触器吸合延时" English="Pump 2 contactor pull-in delay" Show="1" />
  <FunctionCode Name="P00.41" Default="0.020"  DeftEng="0.020"	Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 3 接触器断开延时" English="Pump 3 contactor disconnection delay" Show="1" />
  <FunctionCode Name="P00.42" Default="0.020"  DeftEng="0.020"  Max="5.000" 	Min="0.000" 	    Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 3 接触器吸合延时" English="Pump 3 contactor pull-in delay" Show="1" />
  <FunctionCode Name="P00.43" Default="0.020"  DeftEng="0.020"	Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 4 接触器断开延时" English="Pump 4 contactor disconnection delay" Show="1" />
  <FunctionCode Name="P00.44" Default="0.020"  DeftEng="0.020"  Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 4 接触器吸合延时" English="Pump 4 contactor pull-in delay" Show="1" />
  <FunctionCode Name="P00.45" Default="0.020"  DeftEng="0.020"	Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 5 接触器断开延时" English="Pump 5 contactor disconnection delay" Show="1" />
  <FunctionCode Name="P00.46" Default="0.020"  DeftEng="0.020"  Max="5.000" 	Min="0.000" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="泵 5 接触器吸合延时" English="Pump 5 contactor pull-in delay" Show="1" />
  <FunctionCode Name="P00.47" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.48" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.49" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.50" Default="0"  		DeftEng="0"			Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" 	English="reserved" Show="1" />  
  <FunctionCode Name="P00.51" Default="0.0"  DeftEng="0.0"  Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="辅助泵 1 流量补偿" English="Auxiliary pump 1 flow compensation" Show="1" />  
  <FunctionCode Name="P00.52" Default="0.0"  DeftEng="0.0"  Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="辅助泵 2 流量补偿" English="Auxiliary pump 2 flow compensation" Show="1" />  
  <FunctionCode Name="P00.53" Default="0.0"  DeftEng="0.0"  Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="辅助泵 3 流量补偿" English="Auxiliary pump 3 flow compensation" Show="1" />  
  <FunctionCode Name="P00.54" Default="0.0"  DeftEng="0.0"  Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="辅助泵 4 流量补偿" English="Auxiliary pump 4 flow compensation" Show="1" />  
  <FunctionCode Name="P00.55" Default="50.00"  DeftEng="50.00"  Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="第 1 台辅助泵加泵频率" English="Auxiliary pump 1  start frequency" Show="1" />  
  <FunctionCode Name="P00.56" Default="50.00"  DeftEng="50.00"  Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="第 2 台辅助泵加泵频率" English="Auxiliary pump 2  start frequency" Show="1" />  
  <FunctionCode Name="P00.57" Default="50.00"  DeftEng="50.00"  Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="第 3 台辅助泵加泵频率" English="Auxiliary pump 3  start frequency" Show="1" />  
  <FunctionCode Name="P00.58" Default="50.00"  DeftEng="50.00"  Max="400.00" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="第 4 台辅助泵加泵频率" English="Auxiliary pump 4  start frequency" Show="1" />  
   <FunctionCode Name="P00.59" Default="25.00"  DeftEng="25.00"  Max="400.00"   Min="0.00"    Attribute="0xa16c"  AbsoluteValue="0"     Chinese="第 1 台辅助泵减泵频率" English="Auxiliary pump 1  stop frequency" Show="1" /> 
   <FunctionCode Name="P00.60" Default="25.00"  DeftEng="25.00"  Max="400.00"   Min="0.00"    Attribute="0xa16c"  AbsoluteValue="0"     Chinese="第 2 台辅助泵减泵频率" English="Auxiliary pump 2  stop frequency" Show="1" /> 
   <FunctionCode Name="P00.61" Default="25.00"  DeftEng="25.00"  Max="400.00"   Min="0.00"    Attribute="0xa16c"  AbsoluteValue="0"     Chinese="第 3 台辅助泵减泵频率" English="Auxiliary pump 3  stop frequency" Show="1" /> 
   <FunctionCode Name="P00.62" Default="25.00"  DeftEng="25.00"  Max="400.00"   Min="0.00"    Attribute="0xa16c"  AbsoluteValue="0"     Chinese="第 4 台辅助泵减泵频率" English="Auxiliary pump 4  stop frequency" Show="1" />  
   <FunctionCode Name="P00.63" Default="20.0"  DeftEng="20.0"  Max="3600.0"   Min="0.5"    Attribute="0x266a"  AbsoluteValue="0"     Chinese="主泵无效后禁止加减泵时间" English="Forbidden to increase or decrease the pump time " Show="1" />  
   <FunctionCode Name="P00.64" Default="5.0"  DeftEng="5.0"  Max="3600.0"   Min="0.5"    Attribute="0x266a"  AbsoluteValue="0"     Chinese="主泵无效后延迟切换时间" English="Delayed switching time after the main pump is disabled" Show="1" />  
  
  
  <FunctionCode Name="P01.00" Default="0:水泵无效"  	DeftEng="0:Invalid pump"		Max="1" 		Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="水泵 1 类型选择" English="Pump 1 type selection" Show="1" />
  <FunctionCode Name="P01.01" Default="0:水泵无效"   DeftEng="0:Invalid pump"    Max="1" 		Min="0" 	    Attribute="0x2088" 	AbsoluteValue="0"		Chinese="水泵 2 类型选择" English="Pump 2 type selection" Show="1" />
  <FunctionCode Name="P01.02" Default="0:水泵无效"  	DeftEng="0:Invalid pump"		Max="1" 		Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="水泵 3 类型选择" English="Pump 3 type selection" Show="1" />
  <FunctionCode Name="P01.03" Default="0:水泵无效"   DeftEng="0:Invalid pump"    Max="1" 		Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="水泵 4 类型选择" English="Pump 4 type selection" Show="1" />
  <FunctionCode Name="P01.04" Default="0:水泵无效"   DeftEng="0:Invalid pump"		Max="4" 		Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="水泵 5 类型选择" English="Pump 5 type selection" Show="1" />
  <FunctionCode Name="P01.05"  Default="0"   DeftEng="0"  		Max="0" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"		Chinese="保留" English="reserved" Show="1" />
  <FunctionCode Name="P01.06" Default="0"   DeftEng="0"		Max="0" 		Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"		Chinese="保留" English="reserved" Show="1" />  
  <FunctionCode Name="P01.07" Default="0"      DeftEng="0"      Max="999.9/99.99" 	Min="0.1/0.01" 	Attribute="0x02ac" 	AbsoluteValue="0"			Chinese="水泵 1 额定电流" English="Water pump 1 rated current" Show="1" />
  <FunctionCode Name="P01.08" Default="0"      DeftEng="0"      Max="999.9/99.99" 	Min="0.1/0.01" 	Attribute="0x02ac" 	AbsoluteValue="0"			Chinese="水泵 2 额定电流" English="Water pump 2 rated current" Show="1" />
  <FunctionCode Name="P01.09" Default="0"      DeftEng="0"      Max="999.9/99.99" 	Min="0.1/0.01" 	Attribute="0x02ac" 	AbsoluteValue="0"			Chinese="水泵 3 额定电流" English="Water pump 3 rated current" Show="1" />
  <FunctionCode Name="P01.10" Default="0"      DeftEng="0"		Max="999.9/99.99" 	Min="0.1/0.01" 	Attribute="0x02ac" 	AbsoluteValue="0"			Chinese="水泵 4 额定电流" English="Water pump 4 rated current" Show="1" />
  <FunctionCode Name="P01.11" Default="0"      DeftEng="0"      Max="999.9/99.99" 	Min="0.1/0.01" 	Attribute="0x02ac" 	AbsoluteValue="0"			Chinese="水泵 5 额定电流" English="Water pump 5 rated current" Show="1" />
  <FunctionCode Name="P01.12" Default="0"      DeftEng="0"		Max="0" 	Min="0"	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />
  <FunctionCode Name="P01.13" Default="0"      DeftEng="0"		Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="reserved" Show="0" />    
  
  <FunctionCode Name="P02.00" Default="0:数字设定"  	   	DeftEng="0:Digital setting"		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="压力设定通道选择" English="Pressure setting channel selection" Show="1" />
  <FunctionCode Name="P02.01" Default="0.0"      		    DeftEng="0.0"      				Max="P05.03× 10" 	Min="0" 	        Attribute="0x3952" 	AbsoluteValue="0"		Chinese="压力给定数字设定" English="Pressure given digital setting" Show="1" />
  <FunctionCode Name="P02.02" Default="1"  	   				DeftEng="1"						Max="12" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"		Chinese="压力段数选择" English="Number of pressure segments" Show="1" />
  <FunctionCode Name="P02.03" Default="00.00"      		DeftEng="00.00"  		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T1开始时刻" English="T1 start time" Show="1" />
  <FunctionCode Name="P02.04" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T1时段压力" English="T1 period pressure" Show="1" />
  <FunctionCode Name="P02.05" Default="00.00"      		DeftEng="00.00"  		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T2开始时刻" English="T2 start time" Show="1" />
  <FunctionCode Name="P02.06" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T2时段压力" English="T2 period pressure" Show="1" />
  <FunctionCode Name="P02.07" Default="00.00"   		DeftEng="00.00"   		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T3开始时刻" English="T3 start time" Show="1" />
  <FunctionCode Name="P02.08" Default="0.0"   			DeftEng="0.0"   		Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T3时段压力" English="T3 period pressure" Show="1" />
  <FunctionCode Name="P02.09" Default="00.00"   		DeftEng="00.00"   		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T4开始时刻" English="T4 start time" Show="1" />
  <FunctionCode Name="P02.10" Default="0.0"   			DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T4时段压力" English="T4 period pressure" Show="1" />
  <FunctionCode Name="P02.11" Default="00.00"      		DeftEng="00.00"      	Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T5开始时刻" English="T5 start time" Show="1" />
  <FunctionCode Name="P02.12" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0"			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T5时段压力" English="T5 period pressure" Show="1" />
  <FunctionCode Name="P02.13" Default="00.00"      		DeftEng="00.00"			Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T6开始时刻" English="T6 start time" Show="1" />
  <FunctionCode Name="P02.14" Default="0.0"  	   		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T6时段压力" English="T6 period pressure" Show="1" />
  <FunctionCode Name="P02.15" Default="00.00"      		DeftEng="00.00"     	Max="23.59" 		Min="00.00" 	    Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T7开始时刻" English="T7 start time" Show="1" />
  <FunctionCode Name="P02.16" Default="0.0"  	   		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T7时段压力" English="T7 period pressure" Show="1" />
  <FunctionCode Name="P02.17" Default="00.00"      		DeftEng="00.00"  		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T8开始时刻" English="T8 start time" Show="1" />
  <FunctionCode Name="P02.18" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T8时段压力" English="T8 period pressure" Show="1" />
  <FunctionCode Name="P02.19" Default="00.00"      		DeftEng="00.00"  		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T9开始时刻" English="T9 start time" Show="1" />
  <FunctionCode Name="P02.20" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T9时段压力" English="T9 period pressure" Show="1" />
  <FunctionCode Name="P02.21" Default="00.00"   		DeftEng="00.00"   		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T10开始时刻" English="T10 start time" Show="1" />
  <FunctionCode Name="P02.22" Default="0.0"   			DeftEng="0.0"   		Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T10时段压力" English="T10 period pressure" Show="1" />
  <FunctionCode Name="P02.23" Default="00.00"   		DeftEng="00.00"   		Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T11开始时刻" English="T11 start time" Show="1" />
  <FunctionCode Name="P02.24" Default="0.0"   			DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T11时段压力" English="T11 period pressure" Show="1" />
  <FunctionCode Name="P02.25" Default="00.00"      		DeftEng="00.00"      	Max="23.59" 		Min="00.00" 		Attribute="0x20a4" 	AbsoluteValue="0"		Chinese="T12开始时刻" English="T12 start time" Show="1" />
  <FunctionCode Name="P02.26" Default="0.0"      		DeftEng="0.0"			Max="P05.03× 10" 	Min="0.0"			Attribute="0x2062" 	AbsoluteValue="0"		Chinese="T12时段压力" English="T12 period pressure" Show="1" />
  <FunctionCode Name="P02.27" Default="50"      	DeftEng="50"		Max="上限频率" 	Min="0" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="压力闭环上限值" 	English="Pressure closed loop upper limit" Show="1" />
  <FunctionCode Name="P02.28" Default="0.01"      	DeftEng="0.01"		Max="10.00" 	Min="0.00" 	Attribute="0x2064" 	AbsoluteValue="0"			Chinese="压力闭环比例增益" English="Pressure closed loop proportional gain" Show="1" /> 
  <FunctionCode Name="P02.29" Default="0.10"   		DeftEng="0.10"   	Max="10.00" 	Min="0.01" 	Attribute="0x266C" 	AbsoluteValue="0"			Chinese="压力闭环积分时间" English="Pressure closed loop integration time" Show="1" />
  <FunctionCode Name="P02.30" Default="0.00"   		DeftEng="0.00"		Max="1.00" 		Min="0.00" 	Attribute="0x265c" 	AbsoluteValue="0"			Chinese="压力闭环微分时间" English="Pressure closed-loop differential time" Show="1" />
  <FunctionCode Name="P02.31" Default="0.50"      	DeftEng="0.50"      Max="30.00" 	Min="0.01" 	Attribute="0x2664" 	AbsoluteValue="0"			Chinese="采样周期" 			English="The sampling period" Show="1" />
  <FunctionCode Name="P02.32" Default="0.0"      	DeftEng="0.0"		Max="20.0" 		Min="0.0"	Attribute="0x255a" 	AbsoluteValue="0"			Chinese="偏差极限" 			English="Deviation limit" Show="1" />
  <FunctionCode Name="P02.33" Default="0.50"      	DeftEng="0.50"		Max="30.00" 	Min="0.01" 	Attribute="0x2664" 	AbsoluteValue="0"			Chinese="压力闭环输出滤波" English="Pressure closed loop output filtering" Show="1" />
  <FunctionCode Name="P02.34" Default="0:正特性"  	DeftEng="0:Positive characteristic"		Max="1" 		Min="0" 	Attribute="0x2048" 	AbsoluteValue="0"		Chinese="压力闭环调节特性" English="Pressure closed loop regulation" Show="1" />
  <FunctionCode Name="P02.35" Default="1:存储"      DeftEng="1:storage" Max="1" 		Min="0" 	Attribute="0x2048" 	AbsoluteValue="0"		Chinese="数字设定压力掉电存储选择" English="Digital setting pressure power-down storage option" Show="1" />
 
  <FunctionCode Name="P03.00" Default="0:保留"   DeftEng="0:Reserved"   Max="3" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="AI1 端子功能" English="AI1 terminal function" Show="1" />
  <FunctionCode Name="P03.01" Default="0:保留"   DeftEng="0:Reserved"   Max="3" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="AI2 端子功能" English="AI2 terminal function" Show="1" />
  <FunctionCode Name="P03.02" Default="0:保留"   DeftEng="0:Reserved"   Max="3" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="AI3 端子功能" English="AI3 terminal function" Show="1" />
  <FunctionCode Name="P03.03" Default="0:保留"   DeftEng="0:Reserved"   Max="3" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="AI4 端子功能" English="AI4 terminal function" Show="1" />
  <FunctionCode Name="P03.04" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI1 端子功能" English="DI1 terminal function" Show="1" />
  <FunctionCode Name="P03.05" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0"		Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI2 端子功能" English="DI2 terminal function" Show="1" />
  <FunctionCode Name="P03.06" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI3 端子功能" English="DI3 terminal function" Show="1" />
  <FunctionCode Name="P03.07" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI4 端子功能" English="DI4 terminal function" Show="1" />
  <FunctionCode Name="P03.08" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI5 端子功能" English="DI5 terminal function" Show="1" />
  <FunctionCode Name="P03.09" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI6 端子功能" English="DI6 terminal function" Show="1" />
  <FunctionCode Name="P03.10" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI7 端子功能" English="DI7 terminal function" Show="1" />
  <FunctionCode Name="P03.11" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI8 端子功能" English="DI8 terminal function" Show="1" />
  <FunctionCode Name="P03.12" Default="0:保留"   DeftEng="0:Reserved"   Max="19" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI9 端子功能" English="DI9 terminal function" Show="1" />
  <FunctionCode Name="P03.13" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0"		Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO1 端子功能" English="DO1 terminal function" Show="1" />
  <FunctionCode Name="P03.14" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO2 端子功能" English="DO2 terminal function" Show="1" />
  <FunctionCode Name="P03.15" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY1 继电器功能" English="RLY1 relay function" Show="1" />
  <FunctionCode Name="P03.16" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY2 继电器功能" English="RLY2 relay function" Show="1" />
  <FunctionCode Name="P03.17" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY3 继电器功能" English="RLY3 relay function" Show="1" />
  <FunctionCode Name="P03.18" Default="0:保留"   DeftEng="0:Reserved"   Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY4 继电器功能" English="RLY4 relay function" Show="1" />
  <FunctionCode Name="P03.19" Default="0:保留"   DeftEng="0:Reserved"	Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY5 继电器功能" English="RLY5 relay function" Show="1" />
  <FunctionCode Name="P03.20" Default="0:保留"   DeftEng="0:Reserved"	Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY6 继电器功能" English="RLY6 relay function" Show="1" />
  <FunctionCode Name="P03.21" Default="0:保留"   DeftEng="0:Reserved"	Max="23" 	Min="0"		Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY7 继电器功能" English="RLY7 relay function" Show="1" />
  <FunctionCode Name="P03.22" Default="0:保留"   DeftEng="0:Reserved"	Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY8 继电器功能" English="RLY8 relay function" Show="1" />
  <FunctionCode Name="P03.23" Default="0:保留"   DeftEng="0:Reserved"	Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY9 继电器功能" English="RLY9 relay function" Show="1" />
  <FunctionCode Name="P03.24" Default="0:保留"   DeftEng="0:Reserved" Max="23" 	Min="0" 	Attribute="0x2090" 	AbsoluteValue="0"			Chinese="RLY10 继电器功能" English="RLY10 relay function" Show="1" />  
  
  <FunctionCode Name="P04.00" Default="0.0 "      DeftEng="0.0"		Max="P05.03× 10" 	Min="0.0" 	Attribute="0x3952" 	AbsoluteValue="0"			Chinese="超压保护设定值" 	English="Overpressure protection setting" Show="1" />
  <FunctionCode Name="P04.01" Default="300.0"     DeftEng="300.0"	Max="3600.0" 		Min="0.0" 	Attribute="0x2652" 	AbsoluteValue="0"			Chinese="超压保护检测时间" English="Overpressure protection detection time" Show="1" />
  <FunctionCode Name="P04.02" Default="0.0"       DeftEng="0.0"		Max="P05.03× 10" 	Min="0.0" 	Attribute="0x3952" 	AbsoluteValue="0"			Chinese="欠压保护设定值" 	English="Undervoltage protection setting" Show="1" />
  <FunctionCode Name="P04.03" Default="300.0"     DeftEng="300.0"	Max="3600.0" 		Min="0.0" 	Attribute="0x2652" 	AbsoluteValue="0"			Chinese="欠压保护检测时间" English="Undervoltage protection detection time" Show="1" />
  <FunctionCode Name="P04.04" Default="0"         DeftEng="0"		Max="0x1F" 			Min="0" 	Attribute="0x0011" 	AbsoluteValue="0"			Chinese="故障泵记录" 		English="Fault pump record" Show="1" />
  <FunctionCode Name="P04.05" Default="0:全部停止"      DeftEng="0:Stop all"		Max="0" 	Min="0" 	Attribute="0x2049" 	AbsoluteValue="0"	Chinese="变频器故障处理方式" English="Inverter troubleshooting" Show="1" />
  <FunctionCode Name="P05.00" Default="0"      		DeftEng="0"			Max="99" 	Min="11" 	Attribute="0x2048" 	AbsoluteValue="0"			Chinese="当前时间设置(年)" 	English="Current time setting (year)" Show="1" />
  <FunctionCode Name="P05.01" Default="0"      		DeftEng="0"			Max="1231" 	Min="0101" 	Attribute="0x2048" 	AbsoluteValue="0"			Chinese="当前时间设置(月日)" 	English="Current time setting (month and day)" Show="1" />
  <FunctionCode Name="P05.02" Default="0"      		DeftEng="0"			Max="2359" 	Min="0000" 	Attribute="0x2048" 	AbsoluteValue="0"			Chinese="当前时间设置(时分)" 	English="Current time setting (hours and minutes)" Show="1" />
  <FunctionCode Name="P05.03" Default="1.6"    		DeftEng="1.6"		Max="10.0" 	Min="0.0" 	Attribute="0x3a92" 	AbsoluteValue="0"			Chinese="远程压力表量程设定" 	English="Remote pressure gauge range setting" Show="1" />
  <FunctionCode Name="P05.04" Default="0：0-10V"    	DeftEng="0：0-10V"	Max="2" 	Min="0" 	Attribute="0x2088" 	AbsoluteValue="0"			Chinese="远程压力表信号选择" 	English="Remote pressure gauge signal selection" Show="1" />
  <FunctionCode Name="P05.05" Default="0"      	DeftEng="0"		Max="5" 	Min="0" 	Attribute="0x2089" 	AbsoluteValue="0"			Chinese="供水方案选择" 	English="Setting of water supply plan" Show="1" />
  <FunctionCode Name="P05.06" Default="0"      	DeftEng="0"		Max="11" 	Min="0" 	Attribute="0x2051" 	AbsoluteValue="0"			Chinese="供水故障状态显示与清除" 	English="Water supply fault status display and cleanup" Show="1" />
  
</FuncGroup>