<?xml version="1.0" encoding="utf-8"?>
<!--This is FunctionCode Struct-->
<FuncGroup>
  <FunctionCode Name="F00.00" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028"	AbsoluteValue="0"			Chinese="控制模式选择" English="" Show="1" />
  <FunctionCode Name="F00.01" Default="0:无PG的V/f控制" 		Max="2" 			Min="0" 			Attribute="0x2088"	AbsoluteValue="0"			Chinese="速度控制方式选择" English="" Show="1" />
  <FunctionCode Name="F00.02" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028"	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F00.03" Default="0:电机1" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="电机选择" English="" Show="1" />
  <FunctionCode Name="F00.04" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F00.05" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="1" />
  <FunctionCode Name="F00.06" Default="50.00"	Max="400.00" 	Min="50.00"		Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="变频器最大输出频率" English="" Show="1" />
  <FunctionCode Name="F00.07" Default="0:数字设定" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="上限运行频率设定通道" English="" Show="1" />
  <FunctionCode Name="F00.08" Default="50.00" Max="F00.06" 	Min="0.00" 		Attribute="0x61ac" 	AbsoluteValue="0"			Chinese="上限运行频率" English="" Show="1" />
  <FunctionCode Name="F00.09" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="下限运行频率" English="" Show="1" />
  <FunctionCode Name="F00.10" Default="0:操作面板数字设定" 		Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="频率给定通道选择" English="" Show="1" />
  <FunctionCode Name="F00.11" Default="0:操作面板运行命令通道" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="命令给定通道选择" English="" Show="1" />
  <FunctionCode Name="F00.12" Default="4:实际长度和计时清零" 		Max="5" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="多功能键功能选择" English="" Show="1" />
  <FunctionCode Name="F00.13" Default="20.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="初始运行频率数字设定" English="" Show="1" />
  <FunctionCode Name="F00.14" Default="0x1001" Max="0x1111" 	Min="0x0000" 	Attribute="0x20a1" 	AbsoluteValue="0"			Chinese="UP/DOWN数字给定控制" English="" Show="1" />
  <FunctionCode Name="F00.15" Default="5.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定1" English="" Show="1" />
  <FunctionCode Name="F00.16" Default="0.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x26a2" 	AbsoluteValue="0"			Chinese="点动运行间隔时间" English="" Show="1" />
  <FunctionCode Name="F00.17" Default="0:方向一致" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="运行方向选择" English="" Show="1" />
  <FunctionCode Name="F00.18" Default="0:允许反转" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="防反转选择" English="" Show="1" />
  <FunctionCode Name="F00.19" Default="0.0" 	Max="3600.0" 	Min="0.0" 		Attribute="0x26aa" 	AbsoluteValue="0"			Chinese="正反转死区时间" English="" Show="1" />
  <FunctionCode Name="F00.20" Default="0" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="外引面板按键使能" English="" Show="1" />
  <FunctionCode Name="F00.21" Default="1" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="模拟量超限保护开关" English="" Show="1" />
  <FunctionCode Name="F00.22" Default="0" 	Max="1" 	Min="0" 		Attribute="0x2048" 	AbsoluteValue="0"			Chinese="多功能键运行清零使能" English="" Show="1" />
  <FunctionCode Name="F00.23" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F00.24" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F01.00" Default="0" 		Max="65535" 	Min="0" 			Attribute="0x0068" 	AbsoluteValue="0"			Chinese="用户密码" English="" Show="1" />
  <FunctionCode Name="F01.01" Default="0" 		Max="1" 			Min="0" 	  	Attribute="0x2048" 	AbsoluteValue="0"			Chinese="菜单模式" English="" Show="1" />
  <FunctionCode Name="F01.02" Default="0:无操作" 		Max="4" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="功能码参数初始化" English="" Show="1" />
  <FunctionCode Name="F01.03" Default="0:无操作" 		Max="2" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="操作面EEPROM参数初始化" English="" Show="1" />
  <FunctionCode Name="F01.04" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户权限密码1" English="" Show="1" />
  <FunctionCode Name="F01.05" Default="0.0" 		Max="999.9" 			Min="0.0" 			Attribute="0x6a" 	AbsoluteValue="0"			Chinese="用户允许运行时间1" English="" Show="1" />
  <FunctionCode Name="F01.06" Default="0" 		Max="1" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户状态1" English="" Show="1" />
  <FunctionCode Name="F01.07" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户权限密码2" English="" Show="1" />
  <FunctionCode Name="F01.08" Default="0.0" 		Max="999.9" 			Min="0.0" 			Attribute="0x6a" 	AbsoluteValue="0"			Chinese="用户允许运行时间2" English="" Show="1" />
  <FunctionCode Name="F01.09" Default="0" 		Max="1" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户状态2" English="" Show="1" />
  <FunctionCode Name="F01.10" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户权限密码3" English="" Show="1" />
  <FunctionCode Name="F01.11" Default="0.0" 		Max="999.9" 			Min="0.0" 			Attribute="0x6a" 	AbsoluteValue="0"			Chinese="用户允许运行时间3" English="" Show="1" />
  <FunctionCode Name="F01.12" Default="0" 		Max="1" 			Min="0" 			Attribute="0x48" 	AbsoluteValue="0"			Chinese="用户状态3" English="" Show="1" />
  <FunctionCode Name="F01.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F01.14" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F01.15" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F01.16" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F01.17" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F02.00" Default="0:从起动DWELL频率起动" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="起动方式选择" English="" Show="1" />
  <FunctionCode Name="F02.01" Default="0.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动延迟时间" English="" Show="1" />
  <FunctionCode Name="F02.02" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="起动时DWELL频率设定" English="" Show="1" />
  <FunctionCode Name="F02.03" Default="0.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动DWELL频率保持时间" English="" Show="1" />
  <FunctionCode Name="F02.04" Default="50" 		Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="直流制动电流设定" English="" Show="1" />
  <FunctionCode Name="F02.05" Default="0.50" 	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="起动时直流制动时间" English="" Show="1" />
  <FunctionCode Name="F02.06" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="转速跟踪模式选择" English="" Show="0" />
  <FunctionCode Name="F02.07" Default="1:从停机时刻的频率开始进行速度搜索" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="基于电流搜索时转速搜索方式" English="" Show="1" />
  <FunctionCode Name="F02.08" Default="50" 		Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="转速搜索电流基准设定" English="" Show="1" />
  <FunctionCode Name="F02.09" Default="5.0" 	Max="50.0" 		Min="1.0" 		Attribute="0x269a" 	AbsoluteValue="0"			Chinese="转速搜索加减速时间" English="" Show="1" />
  <FunctionCode Name="F02.10" Default="1.0" 	Max="5.0" 		Min="0.1" 		Attribute="0x2692" 	AbsoluteValue="0"			Chinese="转速搜索等待时间" English="" Show="1" />
  <FunctionCode Name="F02.11" Default="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="转速搜索V/F比值" English="" Show="1" />
  <FunctionCode Name="F02.12" Default="1.00" 	Max="5.00" 		Min="0.01" 		Attribute="0x269c" 	AbsoluteValue="0"			Chinese="转速搜索出后的处理时间" English="" Show="1" />
  <FunctionCode Name="F02.13" Default="0:减速停机" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="停机方式选择" English="" Show="1" />
  <FunctionCode Name="F02.14" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="停机DWELL频率设定" English="" Show="1" />
  <FunctionCode Name="F02.15" Default="0.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机DWELL频率保持时间" English="" Show="1" />
  <FunctionCode Name="F02.16" Default="0.50" 	Max="50.00" 	Min="0.00" 		Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="停机直流制动起始频率" English="" Show="1" />
  <FunctionCode Name="F02.17" Default="0.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机直流制动等待时间" English="" Show="1" />
  <FunctionCode Name="F02.18" Default="0.50" 	Max="60.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="停机时直流制动时间" English="" Show="1" />
  <FunctionCode Name="F02.19" Default="0x00" 	Max="0x11" 	Min="00" 		Attribute="0x2091" 	AbsoluteValue="0"			Chinese="点动控制方式" English="" Show="1" />
  <FunctionCode Name="F02.20" Default="0" 	    Max="0" 	        Min="0" 		    Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F02.21" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F02.22" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F02.23" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.00" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.01" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="加速时间1" English="" Show="1" />
  <FunctionCode Name="F03.02" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="减速时间1" English="" Show="1" />
  <FunctionCode Name="F03.03" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="加速时间2" English="" Show="1" />
  <FunctionCode Name="F03.04" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="减速时间2" English="" Show="1" />
  <FunctionCode Name="F03.05" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="加速时间3" English="" Show="1" />
  <FunctionCode Name="F03.06" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="减速时间3" English="" Show="1" />
  <FunctionCode Name="F03.07" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="加速时间4" English="" Show="1" />
  <FunctionCode Name="F03.08" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="减速时间4" English="" Show="1" />
  <FunctionCode Name="F03.09" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="加速时间1和2切换频率" English="" Show="1" />
  <FunctionCode Name="F03.10" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="减速时间1和2切换频率" English="" Show="1" />
  <FunctionCode Name="F03.11" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.12" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.14" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.15" Default="6.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="点动加速时间" English="" Show="1" />
  <FunctionCode Name="F03.16" Default="6.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="点动减速时间" English="" Show="1" />
  <FunctionCode Name="F03.17" Default="10.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="紧急停机减速时间" English="" Show="1" />
  <FunctionCode Name="F03.18" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.19" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.20" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.21" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F03.22" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F04.00" Default="0:PID控制无效" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="过程PID控制选择" English="" Show="1" />
  <FunctionCode Name="F04.01" Default="0:数字给定" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="给定通道选择" English="" Show="1" />
  <FunctionCode Name="F04.02" Default="0:模拟量反馈" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="反馈通道选择" English="" Show="1" />
  <FunctionCode Name="F04.03" Default="3.5" 		Max="+10.00" 	Min="-10.00"	Attribute="0x2364" 	AbsoluteValue="10.00"	Chinese="给定量数字设定" English="" Show="1" />
  <FunctionCode Name="F04.04" Default="20.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="比例增益1（P）" English="" Show="1" />
  <FunctionCode Name="F04.05" Default="0.50" 	Max="20.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="积分时间1（I）" English="" Show="1" />
  <FunctionCode Name="F04.06" Default="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="积分项上限" English="" Show="1" />
  <FunctionCode Name="F04.07" Default="0.04" 	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="微分时间1（D）" English="" Show="1" />
  <FunctionCode Name="F04.08" Default="20.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="微分限幅值" English="" Show="1" />
  <FunctionCode Name="F04.09" Default="0.10" 	Max="50.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="采样周期（T）" English="" Show="1" />
  <FunctionCode Name="F04.10" Default="0.0" 	Max="20.0" 		Min="0.0" 		Attribute="0x255a" 	AbsoluteValue="0"			Chinese="偏差极限" English="" Show="1" />
  <FunctionCode Name="F04.11" Default="0:由F04.13设定" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器上限通道" English="" Show="1" />
  <FunctionCode Name="F04.12" Default="0:由F04.14设定" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器下限通道" English="" Show="1" />
  <FunctionCode Name="F04.13" Default="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID调节器上限值" English="" Show="1" />
  <FunctionCode Name="F04.14" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID调节器下限值" English="" Show="1" />
  <FunctionCode Name="F04.15" Default="1:负特性" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID调节器调节特性" English="" Show="1" />
  <FunctionCode Name="F04.16" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="积分项调节选择" English="" Show="0" />
  <FunctionCode Name="F04.17" Default="0.05" 	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="PID输出滤波时间" English="" Show="1" />
  <FunctionCode Name="F04.18" Default="0:PID调节禁止反转" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PID输出反转选择" English="" Show="1" />
  <FunctionCode Name="F04.19" Default="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0xa1ac" 	AbsoluteValue="0"			Chinese="PID输出反转频率上限" English="" Show="1" />
  <FunctionCode Name="F04.20" Default="10.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x2062" 	AbsoluteValue="0"			Chinese="比例增益2(P)" English="" Show="1" />
  <FunctionCode Name="F04.21" Default="5.00" 		Max="20.0" 			Min="0.00" 			Attribute="0x2664" 	AbsoluteValue="0"			Chinese="积分时间2(I)" English="" Show="1" />
  <FunctionCode Name="F04.22" Default="0.00" 		Max="10.00" 			Min="0.00" 			Attribute="0x2664" 	AbsoluteValue="0"			Chinese="微分时间2(D)" English="" Show="1" />
  <FunctionCode Name="F04.23" Default="4" 		Max="4" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="两段PID调节依据" English="" Show="1" />
  <FunctionCode Name="F04.24" Default="0.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x2562" 	AbsoluteValue="0"			Chinese="PID参数切换点1" English="" Show="1" />
  <FunctionCode Name="F04.25" Default="100.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x2562" 	AbsoluteValue="0"			Chinese="PID参数切换点2" English="" Show="1" />
  <FunctionCode Name="F04.26" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F04.27" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F04.28" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F05.00" Default="00000" Max="22222" 	Min="0" 			Attribute="0x20a8" 	AbsoluteValue="0"			Chinese="外部给定曲线选择" English="" Show="1" />
  <FunctionCode Name="F05.01" Default="0.0" 	Max="F05.03" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最小给定" English="" Show="1" />
  <FunctionCode Name="F05.02" Default="0.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最小给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.03" Default="100.0" Max="100.0" 	Min="F05.01" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最大给定" English="" Show="1" />
  <FunctionCode Name="F05.04" Default="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线1最大给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.05" Default="0.0" 	Max="F05.07" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最小给定" English="" Show="1" />
  <FunctionCode Name="F05.06" Default="0.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最小给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.07" Default="100.0" Max="100.0" 	Min="F05.05" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最大给定" English="" Show="1" />
  <FunctionCode Name="F05.08" Default="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="直线2最大给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.09" Default="100.0" Max="100.0" 	Min="F05.11" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定" English="" Show="1" />
  <FunctionCode Name="F05.10" Default="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最大给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.11" Default="100.0" Max="F05.09" 	Min="F05.13" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点2给定" English="" Show="1" />
  <FunctionCode Name="F05.12" Default="100.0" Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点2对应值" English="" Show="1" />
  <FunctionCode Name="F05.13" Default="0.0" 	Max="F05.11" 	Min="F05.15" 	Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线拐点1给定" English="" Show="1" />
  <FunctionCode Name="F05.14" Default="0.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="拐点1对应值" English="" Show="1" />
  <FunctionCode Name="F05.15" Default="0.0" 	Max="F05.13" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定" English="" Show="1" />
  <FunctionCode Name="F05.16" Default="0.0" 	Max="100.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="折线最小给定对应值" English="" Show="1" />
  <FunctionCode Name="F05.17" Default="0.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率1" English="" Show="1" />
  <FunctionCode Name="F05.18" Default="0.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率2" English="" Show="1" />
  <FunctionCode Name="F05.19" Default="0.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="跳跃频率3" English="" Show="1" />
  <FunctionCode Name="F05.20" Default="0.00" 	Max="30.00" 	Min="0.00" 	Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="跳跃频率范围" English="" Show="1" />
  <FunctionCode Name="F05.21" Default="5.00" 	Max="400.00" 	Min="0.00" 	Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="点动运行频率数字设定2" English="" Show="1" />
  <FunctionCode Name="F05.22" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F05.23" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F05.24" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F05.25" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F05.26" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F06.00" Default="5.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令1" English="" Show="1" />
  <FunctionCode Name="F06.01" Default="5.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令2" English="" Show="1" />
  <FunctionCode Name="F06.02" Default="5.00" 	Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令3" English="" Show="1" />
  <FunctionCode Name="F06.03" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令4" English="" Show="1" />
  <FunctionCode Name="F06.04" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令5" English="" Show="1" />
  <FunctionCode Name="F06.05" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令6" English="" Show="1" />
  <FunctionCode Name="F06.06" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令7" English="" Show="1" />
  <FunctionCode Name="F06.07" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令8" English="" Show="1" />
  <FunctionCode Name="F06.08" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令9" English="" Show="1" />
  <FunctionCode Name="F06.09" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令10" English="" Show="1" />
  <FunctionCode Name="F06.10" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令11" English="" Show="1" />
  <FunctionCode Name="F06.11" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令12" English="" Show="1" />
  <FunctionCode Name="F06.12" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令13" English="" Show="1" />
  <FunctionCode Name="F06.13" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令14" English="" Show="1" />
  <FunctionCode Name="F06.14" Default="5.00" Max="400.00" 	Min="0.00" 	Attribute="0x216c" 	AbsoluteValue="0"			Chinese="多段频率指令15" English="" Show="1" />
  <FunctionCode Name="F06.15" Default="0:PLC运行无效" Max="1" Min="0" Attribute="0x2088" AbsoluteValue="0" Chinese="简易PLC控制选择" English="Simple PLC Control Option" Show="1" DeftEng="0: PLC operation invalid" />
  <FunctionCode Name="F06.16" Default="0000" Max="0x1122" Min="0x0000" Attribute="0x20a1" AbsoluteValue="0" Chinese="简易PLC运行方式选择" English="Simple PLC operation mode selection" Show="1" DeftEng="0000" />
  <FunctionCode Name="F06.17" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段1设置" English="PLC Phase 1 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.18" Default="5.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段1运行时间" English="phase 1 Runtime" Show="1" DeftEng="5.0" />
  <FunctionCode Name="F06.19" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段2设置" English="PLC Phase 2 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.20" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段2运行时间" English=" phase 2 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.21" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="阶段3设置" English=" phase 3 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.22" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段3运行时间" English=" phase 3 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.23" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="阶段4设置" English=" phase 4 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.24" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段4运行时间" English=" phase 4 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.25" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段5设置" English="PLC phase 5 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.26" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段5运行时间" English=" phase 5 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.27" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段6设置" English="PLC phase 6 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.28" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段6运行时间" English=" phase 6 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.29" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段7设置" English="PLC phase 7 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.30" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段7运行时间" English=" phase 7 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.31" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段8设置" English="PLC phase 8 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.32" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段8运行时间" English=" phase 8 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.33" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段9设置" English="PLC phase 9 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.34" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段9运行时间" English=" phase 9 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.35" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段10设置" English="PLC phase 10 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.36" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段10运行时间" English=" phase 10 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.37" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段11设置" English="PLC phase 11 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.38" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段11运行时间" English=" phase 11 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.39" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段12设置" English="PLC phase 12 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.40" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段12运行时间" English=" phase 12 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.41" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段13设置" English="PLC phase 13 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.42" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段13运行时间" English=" phase 13 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.43" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段14设置" English="PLC phase 14 settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.44" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段14运行时间" English=" phase 14 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.45" Default="000" Max="0x321" Min="0x000" Attribute="0x2059" AbsoluteValue="0" Chinese="PLC阶段15设置" English="PLC phase 15 Settings" Show="1" DeftEng="000" />
  <FunctionCode Name="F06.46" Default="0.0" Max="3276.7" Min="0.0" Attribute="0x206a" AbsoluteValue="0" Chinese="阶段15运行时间" English=" phase 15 Runtime" Show="1" DeftEng="0.0" />
  <FunctionCode Name="F06.47" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F06.48" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F06.49" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F06.50" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F06.51" Default="0" 	Max="0" 	Min="0" 	Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F08.00" Default="5.5" 	Max="500.0" 	Min="0.2" 		Attribute="0x1222" 	AbsoluteValue="0"			Chinese="异步电机1额定功率" English="" Show="1" />
  <FunctionCode Name="F08.01" Default="380" 	Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="异步电机1额定电压" English="" Show="1" />
  <FunctionCode Name="F08.02" Default="13.00" Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="异步电机1额定电流" English="" Show="1" />
  <FunctionCode Name="F08.03" Default="50.0" 	Max="400.0" 	Min="1.0" 		Attribute="0x0122" 	AbsoluteValue="0"			Chinese="异步电机1额定频率" English="" Show="1" />
  <FunctionCode Name="F08.04" Default="1500" 	Max="24000" 	Min="1" 			Attribute="0x0428" 	AbsoluteValue="0"			Chinese="异步电机1额定转速" English="" Show="1" />
  <FunctionCode Name="F08.05" Default="0.850" Max="1.000" 	Min="0.001" 	Attribute="0x0026" 	AbsoluteValue="0"			Chinese="异步电机1功率因素" English="" Show="1" />
  <FunctionCode Name="F08.06" Default="0:不动作" 		Max="2" 			Min="0" 			Attribute="0x0008" 	AbsoluteValue="0"			Chinese="异步电机1参数自整定" English="" Show="1" />
  <FunctionCode Name="F08.07" Default="0.70" 	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="异步电机1定子电阻" English="" Show="1" />
  <FunctionCode Name="F08.08" Default="0.66" 	Max="99.99" 	Min="0.00" 		Attribute="0x0724" 	AbsoluteValue="0"			Chinese="异步电机1转子电阻" English="" Show="1" />
  <FunctionCode Name="F08.09" Default="5.0" 		Max="9999.0" 		Min="0.0" 			Attribute="0x0c20" 	AbsoluteValue="0"			Chinese="异步电机1漏电感" English="" Show="1" />
  <FunctionCode Name="F08.10" Default="124.0" 	Max="9999.0" 		Min="0.0" 			Attribute="0x0c20" 	AbsoluteValue="0"			Chinese="异步电机1互感抗" English="" Show="1" />
  <FunctionCode Name="F08.11" Default="5.30" 	Max="99.99" 	Min="0.00" 		Attribute="0x0224" 	AbsoluteValue="0"			Chinese="异步电机1空载电流" English="" Show="1" />
  <FunctionCode Name="F08.12" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="异步电机1铁芯饱和系数1" English="" Show="1" />
  <FunctionCode Name="F08.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="异步电机1铁芯饱和系数2" English="" Show="1" />
  <FunctionCode Name="F08.14" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="异步电机1铁芯饱和系数3" English="" Show="1" />
  <FunctionCode Name="F08.15" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F08.16" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F08.17" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F08.18" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F08.19" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.00" Default="0:直线" 		Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="IM1 V/F曲线设定" English="" Show="1" />
  <FunctionCode Name="F09.01" Default="0.00" 	Max="F08.03" 	Min="F09.03" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="IM1 V/F频率值F3" English="" Show="1" />
  <FunctionCode Name="F09.02" Default="0" 		Max="F08.01" 	Min="F09.04" 	Attribute="0x2398" 	AbsoluteValue="0"			Chinese="IM1 V/F电压值V3" English="" Show="1" />
  <FunctionCode Name="F09.03" Default="0.00" 	Max="F09.01" 	Min="F09.05" 	Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="IM1 V/F频率值F2" English="" Show="1" />
  <FunctionCode Name="F09.04" Default="0" 		Max="F09.02" 	Min="F09.06" 	Attribute="0x2398" 	AbsoluteValue="0"			Chinese="IM1 V/F电压值V2" English="" Show="1" />
  <FunctionCode Name="F09.05" Default="0.00" 	Max="F09.03" 	Min="0.00" 		Attribute="0x21ac" 	AbsoluteValue="0"			Chinese="IM1 V/F频率值F1" English="" Show="1" />
  <FunctionCode Name="F09.06" Default="0" 		Max="F09.04" 	Min="0" 			Attribute="0x2398" 	AbsoluteValue="0"			Chinese="IM1 V/F电压值V1" English="" Show="1" />
  <FunctionCode Name="F09.07" Default="2.0" 	Max="30.0" 		Min="0.0" 		Attribute="0x259a" 	AbsoluteValue="0"			Chinese="IM1转矩提升" English="" Show="1" />
  <FunctionCode Name="F09.08" Default="3.00" 	Max="5.00" 		Min="0.00" 		Attribute="0x255c" 	AbsoluteValue="0"			Chinese="IM1手动转矩提升截止点" English="" Show="1" />
  <FunctionCode Name="F09.09" Default="0.0" Max="300.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="IM1转差补偿增益" English="" Show="1" />
  <FunctionCode Name="F09.10" Default="0.10" 	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="IM1转差补偿滤波时间" English="" Show="1" />
  <FunctionCode Name="F09.11" Default="200.0" Max="250.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="IM1转差补偿限定" English="" Show="1" />
  <FunctionCode Name="F09.12" Default="2.0" 	Max="25.0" 		Min="0.1" 		Attribute="0x265a" 	AbsoluteValue="0"			Chinese="IM1补偿时间常数" English="" Show="1" />
  <FunctionCode Name="F09.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.14" Default="1:一直动作" 		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="IM1AVR(自动电压调节)功能" English="" Show="1" />
  <FunctionCode Name="F09.15" Default="0:根据励磁分量抑制震荡" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="IM1抑制震荡模式" English="" Show="1" />
  <FunctionCode Name="F09.16" Default="50" 		Max="200" 		Min="0" 			Attribute="0x2058" 	AbsoluteValue="0"			Chinese="IM1抑制震荡系数" English="" Show="1" />
  <FunctionCode Name="F09.17" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="IM1节能控制选择" English="" Show="1" />
  <FunctionCode Name="F09.18" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="IM1节能系数" English="" Show="1" />
  <FunctionCode Name="F09.19" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.20" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.21" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.22" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F09.23" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F10.00" Default="20.0" 	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1速度控制比例增益1" English="" Show="1" />
  <FunctionCode Name="F10.01" Default="0.20" 	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机1速度控制积分时间1" English="" Show="1" />
  <FunctionCode Name="F10.02" Default="20.0" 	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1速度控制比例增益2" English="" Show="1" />
  <FunctionCode Name="F10.03" Default="0.20" 	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="电机1速度控制积分时间2" English="" Show="1" />
  <FunctionCode Name="F10.04" Default="10.00" Max="50.00" 	Min="0.00" 		Attribute="0x2164" 	AbsoluteValue="0"			Chinese="电机1速度环PI切换频率1" English="" Show="1" />
  <FunctionCode Name="F10.05" Default="15.00" Max="50.00" 	Min="0.00" 		Attribute="0x2164" 	AbsoluteValue="0"			Chinese="电机1速度环PI切换频率2" English="" Show="1" />
  <FunctionCode Name="F10.06" Default="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="电机1速度环积分项设定" English="" Show="1" />
  <FunctionCode Name="F10.07" Default="0.00" 	Max="1.00" 		Min="0.00" 		Attribute="0x265c" 	AbsoluteValue="0"			Chinese="电机1速度环微分时间" English="" Show="1" />
  <FunctionCode Name="F10.08" Default="0.020" Max="1.000" 	Min="0.000" 	Attribute="0x2666" 	AbsoluteValue="0"			Chinese="电机1速度环输出滤波时间" English="" Show="1" />
  <FunctionCode Name="F10.09" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机1电动转矩限定通道" English="" Show="1" />
  <FunctionCode Name="F10.10" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="电机1再生转矩限定通道" English="" Show="1" />
  <FunctionCode Name="F10.11" Default="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机1正转时电动转矩设定" English="" Show="1" />
  <FunctionCode Name="F10.12" Default="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机1反转时电动转矩设定" English="" Show="1" />
  <FunctionCode Name="F10.13" Default="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机1正转时再生转矩设定" English="" Show="1" />
  <FunctionCode Name="F10.14" Default="180.0" Max="200.0" 	Min="0.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="电机1反转时再生转矩设定" English="" Show="1" />
  <FunctionCode Name="F10.15" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F10.16" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F10.17" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F10.18" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F10.19" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F11.00" Default="20.0" 	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1电流环KP" English="" Show="1" />
  <FunctionCode Name="F11.01" Default="20.0" 	Max="200.0" 	Min="0.1" 		Attribute="0x2062" 	AbsoluteValue="0"			Chinese="电机1电流环KI" English="" Show="1" />
  <FunctionCode Name="F11.02" Default="0.008"   Max="1.000"   Min="0.0" 		Attribute="0x2666" 	AbsoluteValue="0"			Chinese="电机1电流环输出滤波时间" English="" Show="1" />
  <FunctionCode Name="F11.03" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F11.04" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F11.05" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F11.06" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F11.07" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.00" Default="2:正转功能" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI1端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.01" Default="3:反转功能" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI2端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.02" Default="49:实际长度清零输入" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI3端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.03" Default="0:保留" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.04" Default="0:保留" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.05" Default="52:长度计数输入" 		Max="86" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DI4端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.06" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.07" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.08" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.09" Default="0:保留" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.10" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.11" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.12" Default="1.00" 	Max="99.99" 	Min="0.00" 		Attribute="0x30a4" 	AbsoluteValue="0"			Chinese="端子UP/DN加减速速率" English="" Show="1" />
  <FunctionCode Name="F15.13" Default="0:2ms" 		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="端子检测间隔时间" English="" Show="1" />
  <FunctionCode Name="F15.14" Default="2" 		Max="100" 		Min="0" 			Attribute="0x3758" 	AbsoluteValue="0"			Chinese="端子检测滤波次数" English="" Show="1" />
  <FunctionCode Name="F15.15" Default="0" 		Max="0x1ff" 	Min="0" 			Attribute="0x2059" 	AbsoluteValue="0"			Chinese="输入端子正反逻辑设定" English="" Show="1" />
  <FunctionCode Name="F15.16" Default="0:两线式运转模式1" 		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="FWD/REV运转模式设定" English="" Show="1" />
  <FunctionCode Name="F15.17" Default="0:自由停机" 		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="端子外部设备故障动作选择" English="" Show="1" />
  <FunctionCode Name="F15.18" Default="34:设定长度1到达" 		Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO1端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.19" Default="25:定长输出" 		Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="DO2端子功能选择" English="" Show="1" />
  <FunctionCode Name="F15.20" Default="25:定长输出" 		Max="36" 			Min="0" 			Attribute="0x2090" 	AbsoluteValue="0"			Chinese="继电器1输出功能选择" English="" Show="1" />
  <FunctionCode Name="F15.21" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.22" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.23" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F15.24" Default="000" 	Max="0x3f" 		Min="0" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="输出端子正反逻辑设定" English="" Show="1" />
  <FunctionCode Name="F15.25" Default="0.00" 	Max="300.00" 	Min="0.00" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="定时功能ON侧延迟时间" English="" Show="1" />
  <FunctionCode Name="F15.26" Default="0.00" 	Max="300.00" 	Min="0.00" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="定时功能OFF侧延迟时间" English="" Show="1" />
  <FunctionCode Name="F15.27" Default="2.50" 	Max="100.00" 	Min="0.00" 		Attribute="0x216c" 	AbsoluteValue="0"			Chinese="频率到达(FAR)检出宽度" English="" Show="1" />
  <FunctionCode Name="F15.28" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频运行检出值" English="" Show="1" />
  <FunctionCode Name="F15.29" Default="0.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频回差" English="" Show="1" />
  <FunctionCode Name="F15.30" Default="0:按给定频率检出" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="FDT1检出方式" English="" Show="1" />
  <FunctionCode Name="F15.31" Default="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT1电平" English="" Show="1" />
  <FunctionCode Name="F15.32" Default="1.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT1滞后" English="" Show="1" />
  <FunctionCode Name="F15.33" Default="0:按给定频率检出" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="FDT2检出方式" English="" Show="1" />
  <FunctionCode Name="F15.34" Default="50.00" Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT2电平" English="" Show="1" />
  <FunctionCode Name="F15.35" Default="1.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="FDT2滞后" English="" Show="1" />
  <FunctionCode Name="F15.36" Default="0" 		Max="65535" 	Min="0" 			Attribute="0x3168" 	AbsoluteValue="0"			Chinese="设定运行时间" English="" Show="1" />
  <FunctionCode Name="F15.37" Default="0" 		Max="9999" 		Min="F15.38" 	Attribute="0x2060" 	AbsoluteValue="0"			Chinese="设定计数值到达给定" English="" Show="1" />
  <FunctionCode Name="F15.38" Default="0" 		Max="F15.37" 	Min="0" 			Attribute="0x2060" 	AbsoluteValue="0"			Chinese="指令计数值到达给定" English="" Show="1" />
  <FunctionCode Name="F15.39" Default="0x1122" 		Max="0x1233" 			Min="0" 			Attribute="0x20a1" 	AbsoluteValue="0"			Chinese="模拟量输入超限选择" English="" Show="1" />
  <FunctionCode Name="F15.40" Default="97.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x2562" 	AbsoluteValue="0"			Chinese="模拟量输入超限上限值" English="" Show="1" />
  <FunctionCode Name="F15.41" Default="3.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x2562" 	AbsoluteValue="0"			Chinese="模拟量输入超限下限值" English="" Show="1" />
  <FunctionCode Name="F15.42" Default="8.00" 		Max="50.00" 			Min="0.00" 			Attribute="0x2664" 	AbsoluteValue="0"			Chinese="模拟量上限超限检测时间" English="" Show="1" />
  <FunctionCode Name="F15.43" Default="0.0" 		Max="100.0" 			Min="0.0" 			Attribute="0x26a2" 	AbsoluteValue="0"			Chinese="输出端子延时" English="" Show="1" />
  <FunctionCode Name="F15.44" Default="0.10" 		Max="0.50" 			Min="0.02" 			Attribute="0x265c" 	AbsoluteValue="0"			Chinese="起动模拟量超限检测时间" English="" Show="1" />
  <FunctionCode Name="F15.45" Default="1.00" 		Max="50.00" 			Min="0.00" 			Attribute="0x2664" 	AbsoluteValue="0"			Chinese="模拟量下限超限检测时间" English="" Show="1" />
  <FunctionCode Name="F15.46" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x2068" 	AbsoluteValue="0"			Chinese="计时报警输出时间" English="" Show="1" />
  <FunctionCode Name="F15.47" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x2068" 	AbsoluteValue="0"			Chinese="计时停机时间" English="" Show="1" />
  <FunctionCode Name="F16.00" Default="0:保留" 		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="操作面板电位器功能选择" English="" Show="1" />
  <FunctionCode Name="F16.01" Default="5:过程PID反馈" 		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="模拟输入AI1功能选择" English="" Show="1" />
  <FunctionCode Name="F16.02" Default="0:保留" 		Max="7" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="模拟输入AI2功能选择" English="" Show="1" />
  <FunctionCode Name="F16.03" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.04" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.05" Default="0.0" 	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输入AI1偏置" English="" Show="1" />
  <FunctionCode Name="F16.06" Default="11.00" 	Max="20.00" 	Min="0.00" 	Attribute="0x2064" 	AbsoluteValue="0"	Chinese="模拟输入AI1增益" English="" Show="1" />
  <FunctionCode Name="F16.07" Default="0.05" 	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="模拟输入AI1滤波时间" English="" Show="1" />
  <FunctionCode Name="F16.08" Default="0.0" 	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输入AI2偏置" English="" Show="1" />
  <FunctionCode Name="F16.09" Default="11.00" 	Max="20.00" 	Min="0.00" 	Attribute="0x2064" 	AbsoluteValue="0.00"	Chinese="模拟输入AI2增益" English="" Show="1" />
  <FunctionCode Name="F16.10" Default="0.05" 	Max="10.00" 	Min="0.01" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="模拟输入AI2滤波时间" English="" Show="1" />
  <FunctionCode Name="F16.11" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="1000"	Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.12" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="100"		Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.14" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="1000"	Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.15" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="100"		Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.16" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.17" Default="10.0" 	Max="50.0" 		Min="0.0" 		Attribute="0x295a" 	AbsoluteValue="0"			Chinese="最大脉冲输入频率" English="" Show="1" />
  <FunctionCode Name="F16.18" Default="10" 		Max="500" 		Min="0" 			Attribute="0x2858" 	AbsoluteValue="0"			Chinese="输入脉冲滤波时间" English="" Show="1" />
  <FunctionCode Name="F16.19" Default="1:输出频率(0-最大输出频率)" 		Max="19" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="AO1端子输出功能选择" English="" Show="1" />
  <FunctionCode Name="F16.20" Default="0:保留" 		Max="19" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="AO2端子输出功能选择" English="" Show="1" />
  <FunctionCode Name="F16.21" Default="0:保留" 		Max="19" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="高速脉冲输出功能选择" English="" Show="1" />
  <FunctionCode Name="F16.22" Default="0.0" 	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输出AO1偏置" English="" Show="1" />
  <FunctionCode Name="F16.23" Default="100.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="模拟输出AO1增益" English="" Show="1" />
  <FunctionCode Name="F16.24" Default="0.0" 	Max="+100.0" 	Min="-100.0" 	Attribute="0x2562" 	AbsoluteValue="100.0"	Chinese="模拟输出AO2偏置" English="" Show="1" />
  <FunctionCode Name="F16.25" Default="100.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="模拟输出AO2增益" English="" Show="1" />
  <FunctionCode Name="F16.26" Default="10.0" 	Max="50.0" 		Min="0.1" 		Attribute="0x295a" 	AbsoluteValue="0"			Chinese="DO2最大输出脉冲频率" English="" Show="1" />
  <FunctionCode Name="F16.27" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.28" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.29" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.30" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F16.31" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F17.00" Default="0:1-8-2格式,无校验,RTU" 		Max="5" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="数据格式" English="" Show="1" />
  <FunctionCode Name="F17.01" Default="3:9600bps" 		Max="5" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="波特率选择" English="" Show="1" />
  <FunctionCode Name="F17.02" Default="2" 		Max="247" 		Min="0" 			Attribute="0x2018" 	AbsoluteValue="0"			Chinese="本机地址" English="" Show="1" />
  <FunctionCode Name="F17.03" Default="0" 		Max="1000" 		Min="0" 			Attribute="0x2820" 	AbsoluteValue="0"			Chinese="本机应答延时" English="" Show="1" />
  <FunctionCode Name="F17.04" Default="0.0" 	Max="1000.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="通讯超时检出时间" English="" Show="1" />
  <FunctionCode Name="F17.05" Default="0.0" 	Max="1000.0" 	Min="0.0" 		Attribute="0x262a" 	AbsoluteValue="0"			Chinese="通讯错误检出时间" English="" Show="1" />
  <FunctionCode Name="F17.06" Default="3:继续运行" 		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯超时时动作选择" English="" Show="1" />
  <FunctionCode Name="F17.07" Default="3:继续运行" 		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯错误时动作选择" English="" Show="1" />
  <FunctionCode Name="F17.08" Default="1:紧急停机" 		Max="3" 			Min="0" 			Attribute="0x2008" 	AbsoluteValue="0"			Chinese="通讯外部设备故障动作选择" English="" Show="1" />
  <FunctionCode Name="F17.09" Default="0x01" 		Max="0x11" 			Min="00" 			Attribute="0x2011" 	AbsoluteValue="0"			Chinese="通讯写功能参数存EEPROM方式选择" English="" Show="1" />
  <FunctionCode Name="F17.10" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F17.11" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F17.12" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F17.13" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F18.00" Default="0:汉语" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="语言选择" English="" Show="1" />
  <FunctionCode Name="F18.01" Default="5" 		Max="10" 			Min="1" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="键盘LCD显示对比度" English="" Show="1" />
  <FunctionCode Name="F18.02" Default="8:给定频率" 		Max="49" 			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数1设置" English="" Show="1" />
  <FunctionCode Name="F18.03" Default="7:设定频率" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数2设置" English="" Show="1" />
  <FunctionCode Name="F18.04" Default="9:输出频率" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数3设置" English="" Show="1" />
  <FunctionCode Name="F18.05" Default="13:输出电压" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数4设置" English="" Show="1" />
  <FunctionCode Name="F18.06" Default="14:输出电流" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数5设置" English="" Show="1" />
  <FunctionCode Name="F18.07" Default="18:直流母线电压" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="运行显示参数6设置" English="" Show="1" />
  <FunctionCode Name="F18.08" Default="7:设定频率" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数1设置" English="" Show="1" />
  <FunctionCode Name="F18.09" Default="18:直流母线电压" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数2设置" English="" Show="1" />
  <FunctionCode Name="F18.10" Default="20:AI1输入电压" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数3设置" English="" Show="1" />
  <FunctionCode Name="F18.11" Default="22:AI2输入电压" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数4设置" English="" Show="1" />
  <FunctionCode Name="F18.12" Default="43:输入端子状态" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数5设置" English="" Show="1" />
  <FunctionCode Name="F18.13" Default="44:输出端子状态" 		Max="49"			Min="0" 			Attribute="0x2050" 	AbsoluteValue="0"			Chinese="停机显示参数6设置" English="" Show="1" />
  <FunctionCode Name="F18.14" Default="0" 		Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="频率显示增益" English="" Show="1" />
  <FunctionCode Name="F18.15" Default="1000" 		Max="65535"			Min="0" 			Attribute="0x2068" 	AbsoluteValue="0"			Chinese="最大线速度" English="" Show="1" />
  <FunctionCode Name="F18.16" Default="0" 		Max="3"			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="线速度显示精度" English="" Show="1" />
  <FunctionCode Name="F18.17" Default="0" 		Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F18.18" Default="0" 		Max="0"			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F19.00" Default="0:无辅助频率通道" 		Max="6" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="频率给定通道辅助通道选择" English="" Show="1" />
  <FunctionCode Name="F19.01" Default="0:主设定+辅助设定" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="主辅给定频率" English="" Show="1" />
  <FunctionCode Name="F19.02" Default="1.00" 	Max="9.99" 		Min="0.00" 		Attribute="0x205c" 	AbsoluteValue="0"			Chinese="模拟辅助给定系数" English="" Show="1" />
  <FunctionCode Name="F19.03" Default="0.00" 	Max="F00.06" 	Min="0" 			Attribute="0x616c" 	AbsoluteValue="0"			Chinese="数字辅助频率初值" English="" Show="1" />
  <FunctionCode Name="F19.04" Default="0" 		Max="0x11" 		Min="0" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="数字辅助频率控制选择" English="" Show="1" />
  <FunctionCode Name="F19.05" Default="1:相对最大输出频率调整" 		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="设定频率比例调整选择" English="" Show="1" />
  <FunctionCode Name="F19.06" Default="100.0" Max="200.0" 	Min="0.0" 		Attribute="0x2562" 	AbsoluteValue="0"			Chinese="设定频率比例调整系数" English="" Show="1" />
  <FunctionCode Name="F19.07" Default="0:自动停止" 		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="冷却风扇控制选择" English="" Show="1" />
  <FunctionCode Name="F19.08" Default="30.0" 	Max="600.0" 	Min="0.0" 		Attribute="0x2662" 	AbsoluteValue="0"			Chinese="冷却风扇控制延迟时间" English="" Show="1" />
  <FunctionCode Name="F19.09" Default="0.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x21a4" 	AbsoluteValue="0"			Chinese="下垂控制量" English="" Show="1" />
  <FunctionCode Name="F19.10" Default="1.00" 	Max="F00.08" 	Min="0.00" 		Attribute="0x616c" 	AbsoluteValue="0"			Chinese="零频阈值" English="" Show="1" />
  <FunctionCode Name="F19.11" Default="0:按照频率指令运行" 		Max="3" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="设定频率低于零频阈值时动作选择" English="" Show="1" />
  <FunctionCode Name="F19.12" Default="0:禁止瞬停不停" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="瞬时失电不停机功能选择" English="" Show="1" />
  <FunctionCode Name="F19.13" Default="5.00" 	Max="600.00" 	Min="0.01" 		Attribute="0x266c" 	AbsoluteValue="0"			Chinese="瞬停不停功能减速时间" English="" Show="1" />
  <FunctionCode Name="F19.14" Default="0.10" 	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="瞬时失电不停机电压回升判断时间" English="" Show="1" />
  <FunctionCode Name="F19.15" Default="430" 	Max="999" 		Min="0" 			Attribute="0x2398" 	AbsoluteValue="0"			Chinese="瞬时失电不停机动作判断电压" English="" Show="1" />
  <FunctionCode Name="F19.16" Default="0:禁止停电再起动" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="停电再起动功能选择" English="" Show="1" />
  <FunctionCode Name="F19.17" Default="2.00" 	Max="10.00" 	Min="0.00" 		Attribute="0x2664" 	AbsoluteValue="0"			Chinese="停机再起动等待时间" English="" Show="1" />
  <FunctionCode Name="F19.18" Default="1:允许过压失速" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="过压失速选择" English="" Show="1" />
  <FunctionCode Name="F19.19" Default="740" 	Max="999" 		Min="0" 			Attribute="0x2398" 	AbsoluteValue="0"			Chinese="过压失速点" English="" Show="1" />
  <FunctionCode Name="F19.20" Default="1:加减速有效,恒速无效" 		Max="2" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="自动限流动作选择" English="" Show="1" />
  <FunctionCode Name="F19.21" Default="150.0" Max="200.0" 	Min="20.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="自动限流水平" English="" Show="1" />
  <FunctionCode Name="F19.22" Default="10.00" 	Max="600.00" 	Min="0.00" 		Attribute="0x26ac" 	AbsoluteValue="0"			Chinese="自动限流时减速时间" English="" Show="1" />
  <FunctionCode Name="F19.23" Default="0:上升沿有效" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="端子运行命令有效模式" English="" Show="1" />
  <FunctionCode Name="F19.24" Default="720" 	Max="750" 		Min="330" 		Attribute="0x0398" 	AbsoluteValue="0"			Chinese="制动单元动作电压" English="" Show="1" />
  <FunctionCode Name="F19.25" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F19.26" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x2d6a" 	AbsoluteValue="0"			Chinese="设定长度" English="" Show="1" />
  <FunctionCode Name="F19.27" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x2d6a" 	AbsoluteValue="0"			Chinese="实际长度" English="" Show="1" />
  <FunctionCode Name="F19.28" Default="1.000" 		Max="30.000" 			Min="0.001" 			Attribute="0x20ae" 	AbsoluteValue="0"			Chinese="长度倍率" English="" Show="1" />
  <FunctionCode Name="F19.29" Default="1.000" 		Max="1.000" 			Min="0.001" 			Attribute="0x20a6" 	AbsoluteValue="0"			Chinese="长度校正系数" English="" Show="1" />
  <FunctionCode Name="F19.30" Default="2.10" 		Max="100.00" 			Min="1.00" 			Attribute="0x2eac" 	AbsoluteValue="0"			Chinese="测量轴直径" English="" Show="1" />
  <FunctionCode Name="F19.31" Default="1" 		Max="9999" 			Min="1" 			Attribute="0x20a0" 	AbsoluteValue="0"			Chinese="轴每转脉冲" English="" Show="1" />
  <FunctionCode Name="F19.32" Default="0" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度到达输出功能选择" English="" Show="1" />
  <FunctionCode Name="F19.33" Default="2" 		Max="2" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度到达后记录长度处理" English="" Show="1" />
  <FunctionCode Name="F19.34" Default="1" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="停机时记录长度处理" English="" Show="1" />
  <FunctionCode Name="F19.35" Default="1" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度到达动作选择" English="" Show="1" />
  <FunctionCode Name="F19.36" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="零伺服起始频率" English="" Show="1" />
  <FunctionCode Name="F19.37" Default="0x100" 		Max="0x111" 			Min="0" 			Attribute="0x2099" 	AbsoluteValue="0"			Chinese="频率调节范围选择" English="" Show="1" />
  <FunctionCode Name="F19.38" Default="0" 		Max="65535" 			Min="0" 			Attribute="0x2d6a" 	AbsoluteValue="0"			Chinese="设定长度1" English="" Show="1" />
  <FunctionCode Name="F19.39" Default="1" 		Max="3" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="长度1到达输出功能选择" English="" Show="1" />
  <FunctionCode Name="F19.40" Default="10.00" 		Max="400.00" 			Min="0.00" 			Attribute="0xa16c" 	AbsoluteValue="0"			Chinese="预警减速频率" English="" Show="1" />
  <FunctionCode Name="F19.41" Default="1" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="计时报警输出功能选择" English="" Show="1" />
  <FunctionCode Name="F19.42" Default="0" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="计时停机输出功能选择" English="" Show="1" />
  <FunctionCode Name="F19.43" Default="0" 		Max="1" 			Min="0" 			Attribute="0x2048" 	AbsoluteValue="0"			Chinese="计时停机动作选择" English="" Show="1" />
  <FunctionCode Name="F19.44" Default="0x0201" 		Max="0x2222" 			Min="0" 			Attribute="0x2061" 	AbsoluteValue="0"			Chinese="LCD灯和蜂鸣器报警控制" English="" Show="1" />
  <FunctionCode Name="F19.45" Default="0x10" 		Max="0x11" 			Min="0" 			Attribute="0x2091" 	AbsoluteValue="0"			Chinese="AI角度自学习" English="" Show="1" />
  <FunctionCode Name="F19.46" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F19.47" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F19.48" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.00" Default="00000" Max="11111" 	Min="0" 			Attribute="0x20a8" 	AbsoluteValue="0"			Chinese="过载预报警检出选择" English="" Show="1" />
  <FunctionCode Name="F20.01" Default="150.0" Max="200.0" 	Min="20.0" 		Attribute="0x25a2" 	AbsoluteValue="0"			Chinese="过载预报警检出水平" English="" Show="1" />
  <FunctionCode Name="F20.02" Default="5.0" 	Max="60.0" 		Min="0.0" 		Attribute="0x269a" 	AbsoluteValue="0"			Chinese="过载预报警检出时间" English="" Show="1" />
  <FunctionCode Name="F20.03" Default="0:输出掉载检出无效" 		Max="4" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出动作选择" English="" Show="1" />
  <FunctionCode Name="F20.04" Default="30" 		Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="变频器输出掉载检出水平" English="" Show="1" />
  <FunctionCode Name="F20.05" Default="1.00" 	Max="20.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="变频器输出掉载检测时间" English="" Show="1" />
  <FunctionCode Name="F20.06" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.07" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.08" Default="30" 		Max="50" 			Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="输入缺相检出基准" English="" Show="1" />
  <FunctionCode Name="F20.09" Default="1.00" 	Max="5.00" 		Min="1.00" 		Attribute="0x269c" 	AbsoluteValue="0"			Chinese="输入缺相检测时间" English="" Show="1" />
  <FunctionCode Name="F20.10" Default="20" 		Max="50" 			Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="输出缺相检测基准" English="" Show="1" />
  <FunctionCode Name="F20.11" Default="3.00" 	Max="20.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="输出缺相检测时间" English="" Show="1" />
  <FunctionCode Name="F20.12" Default="0" 		Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="PID给定丢失检出值" English="" Show="1" />
  <FunctionCode Name="F20.13" Default="0.20" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="PID给定丢失检出时间" English="" Show="1" />
  <FunctionCode Name="F20.14" Default="0" 		Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出值" English="" Show="1" />
  <FunctionCode Name="F20.15" Default="0.20" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="PID反馈丢失检出时间" English="" Show="1" />
  <FunctionCode Name="F20.16" Default="100" 	Max="100" 		Min="0" 			Attribute="0x2598" 	AbsoluteValue="0"			Chinese="PID反馈超限检出值" English="" Show="1" />
  <FunctionCode Name="F20.17" Default="0.20" 	Max="10.00" 	Min="0.00" 		Attribute="0x26a4" 	AbsoluteValue="0"			Chinese="PID反馈超限检出时间" English="" Show="1" />
  <FunctionCode Name="F20.18" Default="0" 		Max="100" 		Min="0" 			Attribute="0x2098" 	AbsoluteValue="0"			Chinese="自动复位次数" English="" Show="1" />
  <FunctionCode Name="F20.19" Default="5.0" 	Max="20.0" 		Min="2.0" 		Attribute="0x269a" 	AbsoluteValue="0"			Chinese="自动复位间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.20" Default="00" 		Max="0x11" 		Min="0" 			Attribute="0x2051" 	AbsoluteValue="0"			Chinese="故障继电器动作选择" English="" Show="1" />
  <FunctionCode Name="F20.21" Default="0" 		Max="34" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第五次（最近一次）故障类型" English="" Show="1" />
  <FunctionCode Name="F20.22" Default="0.00" 	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时设定频率" English="" Show="1" />
  <FunctionCode Name="F20.23" Default="0.00" 	Max="400.00" 	Min="0.00" 		Attribute="0x012c" 	AbsoluteValue="0"			Chinese="最近一次故障时输出频率" English="" Show="1" />
  <FunctionCode Name="F20.24" Default="0" 		Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时直流母线电压" English="" Show="1" />
  <FunctionCode Name="F20.25" Default="0" 		Max="999" 		Min="0" 			Attribute="0x0318" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电压" English="" Show="1" />
  <FunctionCode Name="F20.26" Default="0.00" 	Max="99.99" 	Min="0.00" 		Attribute="0x0222" 	AbsoluteValue="0"			Chinese="最近一次故障时输出电流" English="" Show="1" />
  <FunctionCode Name="F20.27" Default="0" 		Max="0x1ff" 	Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输入端子状态" English="" Show="1" />
  <FunctionCode Name="F20.28" Default="0" 		Max="0x3f" 		Min="0" 			Attribute="0x0019" 	AbsoluteValue="0"			Chinese="最近一次故障时输出端子状态" English="" Show="1" />
  <FunctionCode Name="F20.29" Default="0.0" 	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="最近一次故障间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.30" Default="0" 		Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第四次故障类型" English="" Show="1" />
  <FunctionCode Name="F20.31" Default="0.0" 	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第四次故障间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.32" Default="0" 		Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第三次故障类型" English="" Show="1" />
  <FunctionCode Name="F20.33" Default="0.0" 	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第三次故障间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.34" Default="0" 		Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第二次故障类型" English="" Show="1" />
  <FunctionCode Name="F20.35" Default="0.0" 	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第二次故障间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.36" Default="0" 		Max="99" 			Min="0" 			Attribute="0x0010" 	AbsoluteValue="0"			Chinese="第一次故障类型" English="" Show="1" />
  <FunctionCode Name="F20.37" Default="0.0" 	Max="6553.5" 	Min="0.0" 		Attribute="0x112a" 	AbsoluteValue="0"			Chinese="第一次故障间隔时间" English="" Show="1" />
  <FunctionCode Name="F20.38" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.39" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.40" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.41" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F20.42" Default="0" 	Max="0" 	Min="0" 		Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F23.00" Default="6" 		Max="16" 			Min="1" 			Attribute="0x0988" 	AbsoluteValue="0"			Chinese="载波频率设定" English="" Show="1" />
  <FunctionCode Name="F23.01" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="载波频率自动调整选择" English="" Show="1" />
  <FunctionCode Name="F23.02" Default="1:过调制使能有效" 		Max="1" 			Min="0" 			Attribute="0x2088" 	AbsoluteValue="0"			Chinese="PWM过调制使能" English="" Show="1" />
  <FunctionCode Name="F23.03" Default="0" 		Max="0" 			Min="0" 			Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F23.04" Default="0" 	    Max="0" 	        Min="0" 	        Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F23.05" Default="0" 	    Max="0" 	        Min="0" 	        Attribute="0x0028" 	AbsoluteValue="0"			Chinese="保留" English="" Show="0" />
  <FunctionCode Name="F23.06" Default="0" 	Max="65535" 	Min="0" 		Attribute="0x00a8" 	AbsoluteValue="0"			Chinese="屏蔽FO" English="" Show="0" />
  <FunctionCode Name="F23.07" Default="0" 	Max="65535" 	Min="0" 		Attribute="0x00a8" 	AbsoluteValue="0"			Chinese="屏蔽硬件故障密码" English="" Show="0" />
  <FunctionCode Name="F23.08" Default="0" 	Max="0xffff" 	Min="0" 		Attribute="0x00a1" 	AbsoluteValue="0"			Chinese="屏蔽硬件故障选择" English="" Show="0" />
</FuncGroup>